Main Page | Modules | Data Structures | Directories | File List | Data Fields | Globals | Related Pages

# sta013conf.h

Go to the documentation of this file.

    00001 /*! \file sta013conf.h \brief STA013 MP3 player driver configuration. */
    00002 //*****************************************************************************
    00003 //
    00004 // File Name    : 'sta013.h'
    00005 // Title        : STMicroelectronics STA013 MP3 player driver
    00006 // Author       : Pascal Stang - Copyright (C) 2000-2002
    00007 // Created      : 10/22/2000
    00008 // Revised      : 12/04/2000
    00009 // Version      : 0.3
    00010 // Target MCU   : ATmega103 (should work for Atmel AVR Series)
    00011 // Editor Tabs  : 4
    00012 //
    00013 // NOTE: This code is currently below version 1.0, and therefore is considered
    00014 // to be lacking in some functionality or documentation, or may not be fully
    00015 // tested.  Nonetheless, you can expect most functions to work.
    00016 //
    00017 // This code is distributed under the GNU Public License
    00018 //      which can be found at http://www.gnu.org/licenses/gpl.txt
    00019 //
    00020 //*****************************************************************************
    00021
    00022
    00023 #ifndef STA013CONF_H
    00024 #define STA013CONF_H
    00025
    00026 // STA013 Configuration
    00027
    00028 // STA013 demand line
    00029 #define STA013_DEMAND_PORT      PORTE               // port to which DEMAND line is connected
    00030 #define STA013_DEMAND_PORTIN    PINE                // input port to which DEMAND line is connected
    00031 #define STA013_DEMAND_PIN       PE4             // port pin to which DEMAND line is connected
    00032 #define STA013_DEMAND_INTR      SIG_INTERRUPT4  // interrupt to which DEMAND line is connected
    00033
    00034 #endif