<?xml version="1.0" encoding= "UTF-8" ?>
<configuration name="MKL27Z256xxx4" xsi:schemaLocation="http://mcuxpresso.nxp.com/XSD/mex_configuration_11 http://mcuxpresso.nxp.com/XSD/mex_configuration_11.xsd" uuid="10a9a6fb-6f02-4b6e-8d89-1e966cee6270" version="11" xmlns="http://mcuxpresso.nxp.com/XSD/mex_configuration_11" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">
   <common>
      <processor>MKL27Z256xxx4</processor>
      <package>MKL27Z256VLH4</package>
      <mcu_data>ksdk2_0</mcu_data>
      <cores selected="core0">
         <core name="Cortex-M0P" id="core0" description="M0P core"/>
      </cores>
      <description>Configuration imported from MKL27Z4_Highlevel</description>
   </common>
   <preferences>
      <validate_boot_init_only>true</validate_boot_init_only>
      <generate_extended_information>false</generate_extended_information>
      <generate_code_modified_registers_only>false</generate_code_modified_registers_only>
      <update_include_paths>true</update_include_paths>
      <generate_registers_defines>false</generate_registers_defines>
   </preferences>
   <tools>
      <pins name="Pins" version="11.0" enabled="true" update_project_code="true">
         <generated_project_files>
            <file path="board/pin_mux.c" update_enabled="true"/>
            <file path="board/pin_mux.h" update_enabled="true"/>
         </generated_project_files>
         <pins_profile>
            <processor_version>11.0.1</processor_version>
         </pins_profile>
         <functions_list>
            <function name="BOARD_InitPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>true</callFromInitBoot>
                  <coreID>core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins/>
            </function>
         </functions_list>
      </pins>
      <clocks name="Clocks" version="9.0" enabled="true" update_project_code="true">
         <generated_project_files>
            <file path="board/clock_config.c" update_enabled="true"/>
            <file path="board/clock_config.h" update_enabled="true"/>
         </generated_project_files>
         <clocks_profile>
            <processor_version>11.0.1</processor_version>
         </clocks_profile>
         <clock_configurations>
            <clock_configuration name="BOARD_BootClockRUN" id_prefix="" prefix_user_defined="false">
               <description></description>
               <options/>
               <dependencies>
                  <dependency resourceType="PinSignal" resourceId="USB0.CLKIN" description="&apos;USB clock input&apos; (Pins tool id: USB0.CLKIN, Clocks tool id: SIM.USB_CLKIN) needs to be routed" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="routed" evaluation="">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Clocks initialization requires the COMMON Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockRUN">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <clock_sources>
                  <clock_source id="MCG.HIRC.outFreq" value="48 MHz" locked="false" enabled="false"/>
                  <clock_source id="SIM.USBCLK_EXT.outFreq" value="48 MHz" locked="false" enabled="true"/>
               </clock_sources>
               <clock_outputs>
                  <clock_output id="Bus_clock.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="Core_clock.outFreq" value="48 MHz" locked="false" accuracy=""/>
                  <clock_output id="Flash_clock.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPO_clock.outFreq" value="1 kHz" locked="false" accuracy=""/>
                  <clock_output id="MCGIRCLK.outFreq" value="8 MHz" locked="false" accuracy=""/>
                  <clock_output id="MCGPCLK.outFreq" value="48 MHz" locked="false" accuracy=""/>
                  <clock_output id="System_clock.outFreq" value="48 MHz" locked="false" accuracy=""/>
                  <clock_output id="USB48MCLK.outFreq" value="48 MHz" locked="false" accuracy=""/>
               </clock_outputs>
               <clock_settings>
                  <setting id="MCGMode" value="HIRC" locked="false"/>
                  <setting id="MCG.CLKS.sel" value="MCG.HIRC" locked="false"/>
                  <setting id="MCG_MC_HIRCEN_CFG" value="Enabled" locked="false"/>
                  <setting id="SIM.USBSRCSEL.sel" value="MCG.MCGPCLK" locked="false"/>
                  <setting id="USBClkConfig" value="yes" locked="false"/>
               </clock_settings>
               <called_from_default_init>true</called_from_default_init>
            </clock_configuration>
         </clock_configurations>
      </clocks>
      <dcdx name="DCDx" version="3.0" enabled="false" update_project_code="true">
         <generated_project_files/>
         <dcdx_profile>
            <processor_version>N/A</processor_version>
         </dcdx_profile>
         <dcdx_configurations/>
      </dcdx>
      <periphs name="Peripherals" version="11.0" enabled="true" update_project_code="true">
         <dependencies>
            <dependency resourceType="SWComponent" resourceId="middleware.usb.common_header" description="USB Common Header not found in the toolchain/IDE project. Project will not compile!" problem_level="2" source="Peripherals">
               <feature name="enabled" evaluation="equal">
                  <data type="Boolean">true</data>
               </feature>
            </dependency>
            <dependency resourceType="SWComponent" resourceId="middleware.usb.common_header" description="Unsupported version of the USB Common Header in the toolchain/IDE project. Required: ${required_value}, actual: ${actual_value}. Project might not compile correctly." problem_level="1" source="Peripherals">
               <feature name="version" evaluation="equivalent">
                  <data type="Version">2.6.0</data>
               </feature>
            </dependency>
         </dependencies>
         <generated_project_files>
            <file path="board/peripherals.c" update_enabled="true"/>
            <file path="board/peripherals.h" update_enabled="true"/>
            <file path="source/generated/usb_device_composite.c" update_enabled="true"/>
            <file path="source/generated/usb_device_composite.h" update_enabled="true"/>
            <file path="source/generated/usb_device_config.h" update_enabled="true"/>
            <file path="source/generated/usb_device_descriptor.c" update_enabled="true"/>
            <file path="source/generated/usb_device_descriptor.h" update_enabled="true"/>
            <file path="source/usb_device_interface_0_cic_vcom.c" update_enabled="true"/>
            <file path="source/usb_device_interface_0_cic_vcom.h" update_enabled="true"/>
         </generated_project_files>
         <peripherals_profile>
            <processor_version>11.0.1</processor_version>
         </peripherals_profile>
         <functional_groups>
            <functional_group name="BOARD_InitPeripherals" uuid="0cbd73ea-a159-4d8d-bbcd-3eee0032aee0" called_from_default_init="true" id_prefix="" core="core0">
               <description></description>
               <options/>
               <dependencies>
                  <dependency resourceType="SWComponent" resourceId="middleware.usb.device_controller_khci" description="&quot;USB Device KHCI Controller Driver(FS)&quot; component is missing in the project." problem_level="2" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="enabled" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="&quot;Common&quot; driver is missing in the project." problem_level="2" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="enabled" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="ClockOutput" resourceId="USB48MCLK" description="USB Function Clock (USB48MCLK) is inactive and USB module will not work." problem_level="2" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="frequency" evaluation="greaterThan">
                        <data type="Frequency" unit="Hz">0</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="middleware.usb.device.cdc.external" description="&quot;USB device CDC&quot; driver is missing in the project." problem_level="2" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="enabled" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="middleware.usb.device.cdc.external" description="&quot;USB device CDC&quot; driver is missing in the project." problem_level="2" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="enabled" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <instances>
                  <instance name="NVIC" uuid="67ca6761-bf4d-4372-9dcc-a7722d33fefd" type="nvic" type_id="nvic_57b5eef3774cc60acaede6f5b8bddc67" mode="general" peripheral="NVIC" enabled="true" comment="" custom_name_enabled="false" editing_lock="false">
                     <config_set name="nvic">
                        <array name="interrupt_table"/>
                        <array name="interrupts"/>
                     </config_set>
                  </instance>
                  <instance name="USB0" uuid="bffd4d91-55f0-4d34-b900-a3d4d9e1ea4b" type="usb" type_id="usb_c84d398fe7344af73d7dbb640d3b1867" mode="device" peripheral="USB0" enabled="true" comment="" custom_name_enabled="false" editing_lock="false">
                     <config_set name="deviceSetting" quick_selection="QS_DEVICE_CDC_VCOM">
                        <setting name="vendor_id" value="0x1FC9"/>
                        <setting name="product_id" value="0x0094"/>
                        <setting name="manufacturer_string" value="NXP"/>
                        <setting name="product_string" value="VCOM"/>
                        <setting name="self_powered" value="true"/>
                        <setting name="suspend_resume" value="false"/>
                        <setting name="max_power" value="100"/>
                        <array name="interfaces">
                           <struct name="0">
                              <setting name="interface_class" value="kClassCic"/>
                              <struct name="setting_cic" quick_selection="QS_INTERFACE_CIC_VCOM">
                                 <setting name="interface_name" value="CIC VCOM"/>
                                 <setting name="subclass" value="kSubclassAcm"/>
                                 <setting name="protocol" value="kProtocolNone"/>
                                 <setting name="implementation" value="kImplementationCicVcom"/>
                                 <array name="endpoints_settings">
                                    <struct name="0">
                                       <setting name="setting_name" value="Default"/>
                                       <array name="endpoints">
                                          <struct name="0">
                                             <setting name="direction" value="kIn"/>
                                             <setting name="transfer_type" value="kInterrupt"/>
                                             <setting name="synchronization" value="kNoSynchronization"/>
                                             <setting name="usage" value="kData"/>
                                             <setting name="max_packet_size_fs" value="k16"/>
                                             <setting name="polling_interval_fs" value="8"/>
                                             <setting name="bRefresh" value="0"/>
                                             <setting name="bSynchAddress" value="NoSynchronization"/>
                                          </struct>
                                       </array>
                                    </struct>
                                 </array>
                                 <setting name="data_interface_count" value="1"/>
                              </struct>
                           </struct>
                           <struct name="1">
                              <setting name="interface_class" value="kClassDic"/>
                              <struct name="setting_dic" quick_selection="QS_INTERFACE_DIC_VCOM">
                                 <setting name="interface_name" value="DIC VCOM"/>
                                 <setting name="subclass" value="kSubclassNone"/>
                                 <setting name="protocol" value="kProtocolNone"/>
                                 <setting name="implementation" value="kImplementationDicVcom"/>
                                 <array name="endpoints_settings">
                                    <struct name="0">
                                       <setting name="setting_name" value="Default"/>
                                       <array name="endpoints">
                                          <struct name="0">
                                             <setting name="direction" value="kIn"/>
                                             <setting name="transfer_type" value="kBulk"/>
                                             <setting name="synchronization" value="kNoSynchronization"/>
                                             <setting name="usage" value="kData"/>
                                             <setting name="max_packet_size_fs" value="k64"/>
                                             <setting name="polling_interval_fs" value="0"/>
                                             <setting name="bRefresh" value="0"/>
                                             <setting name="bSynchAddress" value="NoSynchronization"/>
                                          </struct>
                                          <struct name="1">
                                             <setting name="direction" value="kOut"/>
                                             <setting name="transfer_type" value="kBulk"/>
                                             <setting name="synchronization" value="kNoSynchronization"/>
                                             <setting name="usage" value="kData"/>
                                             <setting name="max_packet_size_fs" value="k64"/>
                                             <setting name="polling_interval_fs" value="0"/>
                                             <setting name="bRefresh" value="0"/>
                                             <setting name="bSynchAddress" value="NoSynchronization"/>
                                          </struct>
                                       </array>
                                    </struct>
                                 </array>
                              </struct>
                           </struct>
                        </array>
                     </config_set>
                  </instance>
               </instances>
            </functional_group>
         </functional_groups>
         <components>
            <component name="system" uuid="5eb2729f-1ef8-49fe-82e0-8d0818c6cb5f" type_id="system_54b53072540eeeb8f8e9343e71f28176">
               <config_set_global name="global_system_definitions">
                  <setting name="user_definitions" value=""/>
                  <setting name="user_includes" value=""/>
               </config_set_global>
            </component>
            <component name="uart_cmsis_common" uuid="7e24348b-5568-423f-8641-02d7e1a00edd" type_id="uart_cmsis_common_9cb8e302497aa696fdbb5a4fd622c2a8">
               <config_set_global name="global_USART_CMSIS_common" quick_selection="default"/>
            </component>
            <component name="msg" uuid="c0d06567-09fa-411d-ad73-4fe4cf3bf8ae" type_id="msg_6e2baaf3b97dbeef01c0043275f9a0e7">
               <config_set_global name="global_messages"/>
            </component>
            <component name="gpio_adapter_common" uuid="47d75c19-d6fb-4541-abf1-60181c5d0764" type_id="gpio_adapter_common_57579b9ac814fe26bf95df0a384c36b6">
               <config_set_global name="global_gpio_adapter_common" quick_selection="default"/>
            </component>
            <component name="generic_uart" uuid="56b5e0ef-8de3-45cd-b48d-3c4c4a47579e" type_id="generic_uart_8cae00565451cf2346eb1b8c624e73a6">
               <config_set_global name="global_uart"/>
            </component>
            <component name="generic_enet" uuid="c9dfd2f7-56e3-4432-8b76-58cce70e078b" type_id="generic_enet_74db5c914f0ddbe47d86af40cb77a619">
               <config_set_global name="global_enet"/>
            </component>
            <component name="generic_can" uuid="65ab95d6-b061-4b71-829a-e1790ff95a64" type_id="generic_can_1bfdd78b1af214566c1f23cf6a582d80">
               <config_set_global name="global_can"/>
            </component>
         </components>
      </periphs>
      <tee name="TEE" version="4.0" enabled="false" update_project_code="true">
         <generated_project_files/>
         <tee_profile>
            <processor_version>N/A</processor_version>
         </tee_profile>
      </tee>
   </tools>
</configuration>