/*!
\page page_pinalloc Pin Allocation

		<h2 style='font-family: Arial;'>Pin Allocation Report</h2>
		<table cellpadding='2' border='1' style='border: 2px solid #000000;' bgcolor='WHITE' align='center'>
			<tr bgcolor='#E8E8E8'><th>Peripheral</th><th>Custom peripheral name</th><th>Peripheral description</th></tr>
			<tr bgcolor='#F8FF9A'><td>ADC0</td><td>ADC0</td><td><small>Analog-to-Digital Converter</small></td></tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>CMP0</td><td><small>High-Speed Comparator (CMP), Voltage Reference (VREF) Digital-to-Analog Converter (DAC), and Analog Mux (ANMUX)</small></td></tr>
			<tr bgcolor='#E5E44D'><td>DAC0</td><td>DAC0</td><td><small>12-Bit Digital-to-Analog Converter</small></td></tr>
			<tr bgcolor='#F7DCFF'><td>GPIOA</td><td>GPIOA</td><td><small>General Purpose Input/Output</small></td></tr>
			<tr bgcolor='#F7DCFF'><td>GPIOB</td><td>GPIOB</td><td><small>General Purpose Input/Output</small></td></tr>
			<tr bgcolor='#F7DCFF'><td>GPIOC</td><td>GPIOC</td><td><small>General Purpose Input/Output</small></td></tr>
			<tr bgcolor='#F7DCFF'><td>GPIOD</td><td>GPIOD</td><td><small>General Purpose Input/Output</small></td></tr>
			<tr bgcolor='#F7DCFF'><td>GPIOE</td><td>GPIOE</td><td><small>General Purpose Input/Output</small></td></tr>
			<tr bgcolor='#AFFF8E'><td>I2C0</td><td>I2C0</td><td><small>Inter-integrated circuit bus</small></td></tr>
			<tr bgcolor='#AFFF8E'><td>I2C1</td><td>I2C1</td><td><small>Inter-integrated circuit bus</small></td></tr>
			<tr bgcolor='#EBD4BD'><td>LLWU</td><td>LLWU</td><td><small>Low Leakage Wake-up Unit</small></td></tr>
			<tr bgcolor='#CEFFFF'><td>LPTMR0</td><td>LPTMR0</td><td><small>Low Power Timer Module</small></td></tr>
			<tr bgcolor='#DDC7B5'><td>OSC0</td><td>OSC0</td><td><small>Oscillator</small></td></tr>
			<tr bgcolor='#CCB6A0'><td>RCM</td><td>RCM</td><td><small>Reset Control Module</small></td></tr>
			<tr bgcolor='#B3EAFF'><td>RTC</td><td>RTC</td><td><small>Real Time Clock - RTC</small></td></tr>
			<tr bgcolor='#FFE1C7'><td>SIM</td><td>SIM</td><td><small>System Integration Module</small></td></tr>
			<tr bgcolor='#90EE67'><td>SPI0</td><td>SPI0</td><td><small>Serial Peripheral Interface</small></td></tr>
			<tr bgcolor='#90EE67'><td>SPI1</td><td>SPI1</td><td><small>Serial Peripheral Interface</small></td></tr>
			<tr bgcolor='#F7DCFF'><td>SUPPLY</td><td>SUPPLY</td><td><small>Chip power supply</small></td></tr>
			<tr bgcolor='#EBD4BD'><td>SWD</td><td>SWD</td><td><small>Serial wire debug interface</small></td></tr>
			<tr bgcolor='#C7A886'><td>SystemControl</td><td>SystemControl</td><td><small>System control</small></td></tr>
			<tr bgcolor='#86DAFF'><td>TPM0</td><td>TPM0</td><td><small>Timer/PWM Module</small></td></tr>
			<tr bgcolor='#86DAFF'><td>TPM1</td><td>TPM1</td><td><small>Timer/PWM Module</small></td></tr>
			<tr bgcolor='#86DAFF'><td>TPM2</td><td>TPM2</td><td><small>Timer/PWM Module</small></td></tr>
			<tr bgcolor='#E5C3FF'><td>TSI0</td><td>TSI0</td><td><small>Touch Sensing Input</small></td></tr>
			<tr bgcolor='#20E04E'><td>UART0</td><td>UART0</td><td><small>Serial Communications Interface Module UART0</small></td></tr>
			<tr bgcolor='#5FE356'><td>UART1</td><td>UART1</td><td><small>Serial Communications Interface Module UART1</small></td></tr>
			<tr bgcolor='#5FE356'><td>UART2</td><td>UART2</td><td><small>Serial Communications Interface Module UART2</small></td></tr>
			<tr bgcolor='#00CA3A'><td>USB0</td><td>USB0</td><td><small>Universal Serial Bus On The Go - USB0</small></td></tr>
		</table>
		<br/>
		<br/>

		<h2 style='font-family: Arial;'>Routed Pins</h2>
		<table cellpadding='2' border='1' style='border: 2px solid #000000;' bgcolor='WHITE' width='100%' align='center'>
			<tr><td colspan='3'></td><th colspan='4' align='center' bgcolor='#D0D0D0'>Assigned Pin Function(s)</th></tr>
			<tr>
				<th bgcolor='#E8E8E8'>Package Pin #</th><th bgcolor='#E8E8E8'>Pin Name</th><th bgcolor='#E8E8E8'>User Assigned Signal Name</th><th bgcolor='#E8E8E8'>Assigned Peripheral</th><th bgcolor='#E8E8E8'>Assigned Function</th><th bgcolor='#E8E8E8'>Package Function</th><th bgcolor='#E8E8E8'>Dir</th>
			</tr>
			<tr>
				<td>1</td><td>PTE0/UART1_TX/RTC_CLKOUT/CMP0_OUT/I2C1_SDA</td><td>J2_18</td>
				<td bgcolor='#5FE356'>UART1</td><td bgcolor='#5FE356'>uart_tx</td><td bgcolor='#5FE356'>alt3</td><td bgcolor='#5FE356'>Output</td>
			</tr>
			<tr>
				<td>2</td><td>PTE1/SPI1_MOSI/UART1_RX/SPI1_MISO/I2C1_SCL</td><td>J2_20</td>
				<td bgcolor='#5FE356'>UART1</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>alt3</td><td bgcolor='#5FE356'>Input</td>
			</tr>
			<tr>
				<td>3</td><td>PTE2/SPI1_SCK</td><td>J9_9</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>4</td><td>PTE3/SPI1_MISO/SPI1_MOSI</td><td>J9_11</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>5</td><td>PTE4/SPI1_PCS0</td><td>J9_13</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>6</td><td>PTE5</td><td>J9_15</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>7</td><td>VDD8</td><td><small><i>same</i></small></td>
				<td bgcolor='#F7DCFF'>SUPPLY</td><td bgcolor='#F7DCFF'>pwr_vdd0</td><td bgcolor='#F7DCFF'>alt0</td><td bgcolor='#F7DCFF'>Input</td>
			</tr>
			<tr>
				<td>8</td><td>VSS9</td><td><small><i>same</i></small></td>
				<td bgcolor='#F7DCFF'>SUPPLY</td><td bgcolor='#F7DCFF'>pwr_vss0</td><td bgcolor='#F7DCFF'>alt0</td><td bgcolor='#F7DCFF'>Input</td>
			</tr>
			<tr>
				<td>9</td><td>USB0_DP</td><td><small><i>same</i></small></td>
				<td bgcolor='#00CA3A'>USB0</td><td bgcolor='#00CA3A'>usb_dp</td><td bgcolor='#00CA3A'>alt0</td><td bgcolor='#00CA3A'>Input</td>
			</tr>
			<tr>
				<td>10</td><td>USB0_DM</td><td><small><i>same</i></small></td>
				<td bgcolor='#00CA3A'>USB0</td><td bgcolor='#00CA3A'>usb_dm</td><td bgcolor='#00CA3A'>alt0</td><td bgcolor='#00CA3A'>Input</td>
			</tr>
			<tr>
				<td>11</td><td>VOUT33</td><td><small><i>same</i></small></td>
				<td bgcolor='#00CA3A'>USB0</td><td bgcolor='#00CA3A'>usb_vout</td><td bgcolor='#00CA3A'>alt0</td><td bgcolor='#00CA3A'>Output</td>
			</tr>
			<tr>
				<td>12</td><td>VREGIN</td><td><small><i>same</i></small></td>
				<td bgcolor='#00CA3A'>USB0</td><td bgcolor='#00CA3A'>usb_vrin</td><td bgcolor='#00CA3A'>alt0</td><td bgcolor='#00CA3A'>Input</td>
			</tr>
			<tr>
				<td rowspan='2'>13</td><td rowspan='2'>ADC0_DP0/ADC0_SE0/PTE20/TPM1_CH0/UART0_TX</td><td rowspan='2'>J10_1</td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_dp0</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC0</td><td>adc_se0</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='2'>14</td><td rowspan='2'>ADC0_DM0/ADC0_SE4a/PTE21/TPM1_CH1/UART0_RX</td><td rowspan='2'>J10_3</td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_dm0</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC0</td><td>adc_sea4</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='2'>15</td><td rowspan='2'>ADC0_DP3/ADC0_SE3/PTE22/TPM2_CH0/UART2_TX</td><td rowspan='2'>J10_5</td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_dp3</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC0</td><td>adc_se3</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='2'>16</td><td rowspan='2'>ADC0_DM3/ADC0_SE7a/PTE23/TPM2_CH1/UART2_RX</td><td rowspan='2'>J10_7</td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_dm3</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC0</td><td>adc_sea7</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='2'>17</td><td rowspan='2'>VDDA</td><td rowspan='2'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_vref_vdda</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F7DCFF'><td>SUPPLY</td><td>pwr_vdda0</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td>18</td><td>VREFH</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_vref_vrefh</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr>
				<td>19</td><td>VREFL</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_vref_vrefl</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr>
				<td rowspan='2'>20</td><td rowspan='2'>VSSA</td><td rowspan='2'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_vref_vssa</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F7DCFF'><td>SUPPLY</td><td>pwr_vssa0</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='4'>21</td><td rowspan='4'>CMP0_IN5/ADC0_SE4b/PTE29/TPM0_CH2/TPM_CLKIN0</td><td rowspan='4'>J10_9</td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>cmp_in5</td><td bgcolor='#EFF174'>alt0</td><td bgcolor='#EFF174'>Input</td>
			</tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>cmp_neg5</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>cmp_pos5</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#F8FF9A'><td>ADC0</td><td>adc_seb4</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td>22</td><td>DAC0_OUT/ADC0_SE23/CMP0_IN4/PTE30/TPM0_CH3/TPM_CLKIN1</td><td>J10_11</td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port30</td><td bgcolor='#F7DCFF'>alt1</td><td bgcolor='#F7DCFF'>Output</td>
			</tr>
			<tr>
				<td>23</td><td>PTE31/TPM0_CH4</td><td>J2_13</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>24</td><td>PTE24/TPM0_CH0/I2C0_SCL</td><td>ACCEL_SCL</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>25</td><td>PTE25/TPM0_CH1/I2C0_SDA</td><td>ACCEL_SDA</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>26</td><td>TSI0_CH1/PTA0/TPM0_CH5/SWD_CLK</td><td>SWD_CLK/J11_1</td>
				<td bgcolor='#EBD4BD'>SWD</td><td bgcolor='#EBD4BD'>swd_clk</td><td bgcolor='#EBD4BD'>alt7</td><td bgcolor='#EBD4BD'>Input/Output</td>
			</tr>
			<tr>
				<td>27</td><td>TSI0_CH2/PTA1/UART0_RX/TPM2_CH0</td><td>DBG_CONSOLE_RX/J1_2</td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port1</td><td bgcolor='#F7DCFF'>alt1</td><td bgcolor='#F7DCFF'>Output</td>
			</tr>
			<tr>
				<td>28</td><td>TSI0_CH3/PTA2/UART0_TX/TPM2_CH1</td><td>DBG_CONSOLE_TX/J1_4</td>
				<td bgcolor='#E5C3FF'>TSI0</td><td bgcolor='#E5C3FF'>tsi_ch3</td><td bgcolor='#E5C3FF'>alt0</td><td bgcolor='#E5C3FF'>Input</td>
			</tr>
			<tr>
				<td>29</td><td>TSI0_CH4/PTA3/I2C1_SCL/TPM0_CH0/SWD_DIO</td><td>SWD_DIO</td>
				<td bgcolor='#EBD4BD'>SWD</td><td bgcolor='#EBD4BD'>swd_dio</td><td bgcolor='#EBD4BD'>alt7</td><td bgcolor='#EBD4BD'>Input/Output</td>
			</tr>
			<tr>
				<td rowspan='2'>30</td><td rowspan='2'>TSI0_CH5/PTA4/I2C1_SDA/TPM0_CH1/NMI_b</td><td rowspan='2'>J1_10</td>
				<td bgcolor='#C7A886'>SystemControl</td><td bgcolor='#C7A886'>scb_nmi</td><td bgcolor='#C7A886'>alt7</td><td bgcolor='#C7A886'>Input</td>
			</tr>
			<tr bgcolor='#969696'><td>non-peripheral</td><td>NMI</td><td>alt7</td><td>Not Specified</td></tr>
			<tr>
				<td>31</td><td>PTA5/USB_CLKIN/TPM0_CH2</td><td>J1_12</td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port5</td><td bgcolor='#F7DCFF'>alt1</td><td bgcolor='#F7DCFF'>Output</td>
			</tr>
			<tr>
				<td>32</td><td>PTA12/TPM1_CH0</td><td>J1_8</td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port12</td><td bgcolor='#F7DCFF'>alt1</td><td bgcolor='#F7DCFF'>Not Specified</td>
			</tr>
			<tr>
				<td>33</td><td>PTA13/TPM1_CH1</td><td>J2_2</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>34</td><td>PTA14/SPI0_PCS0/UART0_TX</td><td>ACCEL_INT1</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>35</td><td>PTA15/SPI0_SCK/UART0_RX</td><td>ACCEL_INT2</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>36</td><td>PTA16/SPI0_MOSI/SPI0_MISO</td><td>J2_9</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>37</td><td>PTA17/SPI0_MISO/SPI0_MOSI</td><td>J2_11</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>38</td><td>VDD48</td><td><small><i>same</i></small></td>
				<td bgcolor='#F7DCFF'>SUPPLY</td><td bgcolor='#F7DCFF'>pwr_vdd1</td><td bgcolor='#F7DCFF'>alt0</td><td bgcolor='#F7DCFF'>Input</td>
			</tr>
			<tr>
				<td>39</td><td>VSS49</td><td><small><i>same</i></small></td>
				<td bgcolor='#F7DCFF'>SUPPLY</td><td bgcolor='#F7DCFF'>pwr_vss1</td><td bgcolor='#F7DCFF'>alt0</td><td bgcolor='#F7DCFF'>Input</td>
			</tr>
			<tr>
				<td>40</td><td>EXTAL0/PTA18/UART1_RX/TPM_CLKIN0</td><td>EXTAL</td>
				<td bgcolor='#DDC7B5'>OSC0</td><td bgcolor='#DDC7B5'>extal</td><td bgcolor='#DDC7B5'>alt0</td><td bgcolor='#DDC7B5'>Input</td>
			</tr>
			<tr>
				<td>41</td><td>XTAL0/PTA19/UART1_TX/TPM_CLKIN1/LPTMR0_ALT1</td><td>XTAL</td>
				<td bgcolor='#DDC7B5'>OSC0</td><td bgcolor='#DDC7B5'>xtal</td><td bgcolor='#DDC7B5'>alt0</td><td bgcolor='#DDC7B5'>Output</td>
			</tr>
			<tr>
				<td>42</td><td>PTA20/RESET_b</td><td>RESET</td>
				<td bgcolor='#CCB6A0'>RCM</td><td bgcolor='#CCB6A0'>reset</td><td bgcolor='#CCB6A0'>alt7</td><td bgcolor='#CCB6A0'>Input</td>
			</tr>
			<tr>
				<td>43</td><td>ADC0_SE8/TSI0_CH0/PTB0/LLWU_P5/I2C0_SCL/TPM1_CH0</td><td>J10_2</td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sclk</td><td bgcolor='#AFFF8E'>alt2</td><td bgcolor='#AFFF8E'>Input/Output</td>
			</tr>
			<tr>
				<td>44</td><td>ADC0_SE9/TSI0_CH6/PTB1/I2C0_SDA/TPM1_CH1</td><td>J10_4</td>
				<td bgcolor='#86DAFF'>TPM1</td><td bgcolor='#86DAFF'>tmr_ch1</td><td bgcolor='#86DAFF'>alt3</td><td bgcolor='#86DAFF'>Not Specified</td>
			</tr>
			<tr>
				<td rowspan='2'>45</td><td rowspan='2'>ADC0_SE12/TSI0_CH7/PTB2/I2C0_SCL/TPM2_CH0</td><td rowspan='2'>J10_6</td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_se12</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#E5C3FF'><td>TSI0</td><td>tsi_ch7</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td>46</td><td>ADC0_SE13/TSI0_CH8/PTB3/I2C0_SDA/TPM2_CH1</td><td>J10_8</td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sda</td><td bgcolor='#AFFF8E'>alt2</td><td bgcolor='#AFFF8E'>Input/Output</td>
			</tr>
			<tr>
				<td>47</td><td>PTB8/EXTRG_IN</td><td>J9_1</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>48</td><td>PTB9</td><td>J9_3</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>49</td><td>PTB10/SPI1_PCS0</td><td>J9_5</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>50</td><td>PTB11/SPI1_SCK</td><td>J9_7</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>51</td><td>TSI0_CH9/PTB16/SPI1_MOSI/UART0_RX/TPM_CLKIN0/SPI1_MISO</td><td>TOUCH_SLIDER_A</td>
				<td bgcolor='#E5C3FF'>TSI0</td><td bgcolor='#E5C3FF'>tsi_ch9</td><td bgcolor='#E5C3FF'>alt0</td><td bgcolor='#E5C3FF'>Input</td>
			</tr>
			<tr>
				<td>52</td><td>TSI0_CH10/PTB17/SPI1_MISO/UART0_TX/TPM_CLKIN1/SPI1_MOSI</td><td>TOUCH_SLIDER_B</td>
				<td bgcolor='#E5C3FF'>TSI0</td><td bgcolor='#E5C3FF'>tsi_ch10</td><td bgcolor='#E5C3FF'>alt0</td><td bgcolor='#E5C3FF'>Input</td>
			</tr>
			<tr>
				<td>53</td><td>TSI0_CH11/PTB18/TPM2_CH0</td><td>LEDRGB_RED</td>
				<td bgcolor='#E5C3FF'>TSI0</td><td bgcolor='#E5C3FF'>tsi_ch11</td><td bgcolor='#E5C3FF'>alt0</td><td bgcolor='#E5C3FF'>Input</td>
			</tr>
			<tr>
				<td>54</td><td>TSI0_CH12/PTB19/TPM2_CH1</td><td>LEDRGB_GREEN</td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port19</td><td bgcolor='#F7DCFF'>alt1</td><td bgcolor='#F7DCFF'>Output</td>
			</tr>
			<tr>
				<td>55</td><td>ADC0_SE14/TSI0_CH13/PTC0/EXTRG_IN/CMP0_OUT</td><td>J1_3</td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port0</td><td bgcolor='#F7DCFF'>alt1</td><td bgcolor='#F7DCFF'>Output</td>
			</tr>
			<tr>
				<td>56</td><td>ADC0_SE15/TSI0_CH14/PTC1/LLWU_P6/RTC_CLKIN/I2C1_SCL/TPM0_CH0</td><td>J10_12</td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch0</td><td bgcolor='#86DAFF'>alt4</td><td bgcolor='#86DAFF'>Not Specified</td>
			</tr>
			<tr>
				<td>57</td><td>ADC0_SE11/TSI0_CH15/PTC2/I2C1_SDA/TPM0_CH1</td><td>J10_10</td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port2</td><td bgcolor='#F7DCFF'>alt1</td><td bgcolor='#F7DCFF'>Output</td>
			</tr>
			<tr>
				<td>58</td><td>PTC3/LLWU_P7/UART1_RX/TPM0_CH2/CLKOUTa</td><td>J1_5</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>59</td><td>VSS74</td><td><small><i>same</i></small></td>
				<td bgcolor='#F7DCFF'>SUPPLY</td><td bgcolor='#F7DCFF'>pwr_vss2</td><td bgcolor='#F7DCFF'>alt0</td><td bgcolor='#F7DCFF'>Input</td>
			</tr>
			<tr>
				<td>60</td><td>VDD75</td><td><small><i>same</i></small></td>
				<td bgcolor='#F7DCFF'>SUPPLY</td><td bgcolor='#F7DCFF'>pwr_vdd2</td><td bgcolor='#F7DCFF'>alt0</td><td bgcolor='#F7DCFF'>Input</td>
			</tr>
			<tr>
				<td>61</td><td>PTC4/LLWU_P8/SPI0_PCS0/UART1_TX/TPM0_CH3</td><td>J1_7</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>62</td><td>PTC5/LLWU_P9/SPI0_SCK/LPTMR0_ALT2/CMP0_OUT</td><td>J1_9</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td rowspan='3'>63</td><td rowspan='3'>CMP0_IN0/PTC6/LLWU_P10/SPI0_MOSI/EXTRG_IN/SPI0_MISO</td><td rowspan='3'>J1_11</td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>cmp_in0</td><td bgcolor='#EFF174'>alt0</td><td bgcolor='#EFF174'>Input</td>
			</tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>cmp_neg0</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>cmp_pos0</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='3'>64</td><td rowspan='3'>CMP0_IN1/PTC7/SPI0_MISO/SPI0_MOSI</td><td rowspan='3'>J1_1</td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>cmp_in1</td><td bgcolor='#EFF174'>alt0</td><td bgcolor='#EFF174'>Input</td>
			</tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>cmp_neg1</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>cmp_pos1</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='3'>65</td><td rowspan='3'>CMP0_IN2/PTC8/I2C0_SCL/TPM0_CH4</td><td rowspan='3'>J1_14</td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>cmp_in2</td><td bgcolor='#EFF174'>alt0</td><td bgcolor='#EFF174'>Input</td>
			</tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>cmp_neg2</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>cmp_pos2</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='3'>66</td><td rowspan='3'>CMP0_IN3/PTC9/I2C0_SDA/TPM0_CH5</td><td rowspan='3'>J1_16</td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>cmp_in3</td><td bgcolor='#EFF174'>alt0</td><td bgcolor='#EFF174'>Input</td>
			</tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>cmp_neg3</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>cmp_pos3</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td>67</td><td>PTC10/I2C1_SCL</td><td>J1_13</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>68</td><td>PTC11/I2C1_SDA</td><td>J1_15</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>69</td><td>PTC12/TPM_CLKIN0</td><td>J2_1</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>70</td><td>PTC13/TPM_CLKIN1</td><td>J2_3</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>71</td><td>PTC16</td><td>J2_5</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>72</td><td>PTC17</td><td>J2_7</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>73</td><td>PTD0/SPI0_PCS0/TPM0_CH0</td><td>J2_6</td>
				<td bgcolor='#F7DCFF'>GPIOD</td><td bgcolor='#F7DCFF'>port0</td><td bgcolor='#F7DCFF'>alt1</td><td bgcolor='#F7DCFF'>Not Specified</td>
			</tr>
			<tr>
				<td>74</td><td>ADC0_SE5b/PTD1/SPI0_SCK/TPM0_CH1</td><td>LEDRGB_BLUE/J2_12</td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_seb5</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr>
				<td>75</td><td>PTD2/SPI0_MOSI/UART2_RX/TPM0_CH2/SPI0_MISO</td><td>J2_8</td>
				<td bgcolor='#5FE356'>UART2</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>alt3</td><td bgcolor='#5FE356'>Input</td>
			</tr>
			<tr>
				<td>76</td><td>PTD3/SPI0_MISO/UART2_TX/TPM0_CH3/SPI0_MOSI</td><td>J2_10</td>
				<td bgcolor='#5FE356'>UART2</td><td bgcolor='#5FE356'>uart_tx</td><td bgcolor='#5FE356'>alt3</td><td bgcolor='#5FE356'>Output</td>
			</tr>
			<tr>
				<td>77</td><td>PTD4/LLWU_P14/SPI1_PCS0/UART2_RX/TPM0_CH4</td><td>J1_6</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>78</td><td>ADC0_SE6b/PTD5/SPI1_SCK/UART2_TX/TPM0_CH5</td><td>J2_4</td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_seb6</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr>
				<td>79</td><td>ADC0_SE7b/PTD6/LLWU_P15/SPI1_MOSI/UART0_RX/SPI1_MISO</td><td>J2_17</td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_seb7</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr>
				<td>80</td><td>PTD7/SPI1_MISO/UART0_TX/SPI1_MOSI</td><td>J2_19</td>
				<td></td><td></td><td></td><td></td>
			</tr>
		</table>

		<h2 style='font-family: Arial;'>Routable Pins</h2>
		<table cellpadding='2' border='1' style='border: 2px solid #000000;' bgcolor='WHITE' width='100%' align='center'>
			<tr><td colspan='3'></td><th colspan='3' align='center' bgcolor='#D0D0D0'>alt0</th><th colspan='3' align='center' bgcolor='#D0D0D0'>alt1</th><th colspan='3' align='center' bgcolor='#D0D0D0'>alt2</th><th colspan='3' align='center' bgcolor='#D0D0D0'>alt3</th><th colspan='3' align='center' bgcolor='#D0D0D0'>alt4</th><th colspan='3' align='center' bgcolor='#D0D0D0'>alt5</th><th colspan='3' align='center' bgcolor='#D0D0D0'>alt6</th><th colspan='3' align='center' bgcolor='#D0D0D0'>alt7</th></tr>
			<tr>
				<th bgcolor='#E8E8E8'>Package Pin #</th><th bgcolor='#E8E8E8'>Pin Name</th><th bgcolor='#E8E8E8'>User Assigned Signal Name</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
			</tr>
			<tr>
				<td>1</td><td>PTE0/UART1_TX/RTC_CLKOUT/CMP0_OUT/I2C1_SDA</td><td>J2_18</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port0</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#5FE356'>UART1</td><td bgcolor='#5FE356'>uart_tx</td><td bgcolor='#5FE356'>Output</td>
				<td bgcolor='#B3EAFF'>RTC</td><td bgcolor='#B3EAFF'>rtc_clkout</td><td bgcolor='#B3EAFF'>Output</td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>cmp_out</td><td bgcolor='#EFF174'>Output</td>
				<td bgcolor='#AFFF8E'>I2C1</td><td bgcolor='#AFFF8E'>i2c_sda</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>2</td><td>PTE1/SPI1_MOSI/UART1_RX/SPI1_MISO/I2C1_SCL</td><td>J2_20</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port1</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_mosi</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#5FE356'>UART1</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
				<td></td><td></td><td></td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_miso</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C1</td><td bgcolor='#AFFF8E'>i2c_sclk</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>3</td><td>PTE2/SPI1_SCK</td><td>J9_9</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port2</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_sck</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>4</td><td>PTE3/SPI1_MISO/SPI1_MOSI</td><td>J9_11</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port3</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_miso</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_mosi</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>5</td><td>PTE4/SPI1_PCS0</td><td>J9_13</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port4</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_cs0<br/>spi_ss</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>6</td><td>PTE5</td><td>J9_15</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port5</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>7</td><td>VDD8</td><td><small><i>same</i></small></td>
				<td bgcolor='#F7DCFF'>SUPPLY</td><td bgcolor='#F7DCFF'>pwr_vdd0</td><td bgcolor='#F7DCFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>8</td><td>VSS9</td><td><small><i>same</i></small></td>
				<td bgcolor='#F7DCFF'>SUPPLY</td><td bgcolor='#F7DCFF'>pwr_vss0</td><td bgcolor='#F7DCFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>9</td><td>USB0_DP</td><td><small><i>same</i></small></td>
				<td bgcolor='#00CA3A'>USB0</td><td bgcolor='#00CA3A'>usb_dp</td><td bgcolor='#00CA3A'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>10</td><td>USB0_DM</td><td><small><i>same</i></small></td>
				<td bgcolor='#00CA3A'>USB0</td><td bgcolor='#00CA3A'>usb_dm</td><td bgcolor='#00CA3A'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>11</td><td>VOUT33</td><td><small><i>same</i></small></td>
				<td bgcolor='#00CA3A'>USB0</td><td bgcolor='#00CA3A'>usb_vout</td><td bgcolor='#00CA3A'>Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>12</td><td>VREGIN</td><td><small><i>same</i></small></td>
				<td bgcolor='#00CA3A'>USB0</td><td bgcolor='#00CA3A'>usb_vrin</td><td bgcolor='#00CA3A'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>13</td><td>ADC0_DP0/ADC0_SE0/PTE20/TPM1_CH0/UART0_TX</td><td>J10_1</td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_dp0<br/>adc_se0</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port20</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM1</td><td bgcolor='#86DAFF'>tmr_ch0</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td bgcolor='#20E04E'>UART0</td><td bgcolor='#20E04E'>uart_tx</td><td bgcolor='#20E04E'>Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>14</td><td>ADC0_DM0/ADC0_SE4a/PTE21/TPM1_CH1/UART0_RX</td><td>J10_3</td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_dm0<br/>adc_sea4</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port21</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM1</td><td bgcolor='#86DAFF'>tmr_ch1</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td bgcolor='#20E04E'>UART0</td><td bgcolor='#20E04E'>uart_rx</td><td bgcolor='#20E04E'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>15</td><td>ADC0_DP3/ADC0_SE3/PTE22/TPM2_CH0/UART2_TX</td><td>J10_5</td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_dp3<br/>adc_se3</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port22</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM2</td><td bgcolor='#86DAFF'>tmr_ch0</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td bgcolor='#5FE356'>UART2</td><td bgcolor='#5FE356'>uart_tx</td><td bgcolor='#5FE356'>Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>16</td><td>ADC0_DM3/ADC0_SE7a/PTE23/TPM2_CH1/UART2_RX</td><td>J10_7</td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_dm3<br/>adc_sea7</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port23</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM2</td><td bgcolor='#86DAFF'>tmr_ch1</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td bgcolor='#5FE356'>UART2</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>17</td><td>VDDA</td><td><small><i>same</i></small></td>
				<td bgcolor='#FFFFFF'>ADC0<br/>ADC0<br/>ADC0<br/>ADC0<br/>SUPPLY</td><td bgcolor='#FFFFFF'>adc_vrefh<br/>adc_se29<br/>adc_dp29<br/>adc_vref_vdda<br/>pwr_vdda0</td><td bgcolor='#FFFFFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>18</td><td>VREFH</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_vrefh<br/>adc_se29<br/>adc_dp29<br/>adc_vref_vrefh</td><td bgcolor='#F8FF9A'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>19</td><td>VREFL</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_vrefl<br/>adc_se30<br/>adc_dm29<br/>adc_vref_vrefl</td><td bgcolor='#F8FF9A'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>20</td><td>VSSA</td><td><small><i>same</i></small></td>
				<td bgcolor='#FFFFFF'>ADC0<br/>ADC0<br/>ADC0<br/>ADC0<br/>SUPPLY</td><td bgcolor='#FFFFFF'>adc_vrefl<br/>adc_se30<br/>adc_dm29<br/>adc_vref_vssa<br/>pwr_vssa0</td><td bgcolor='#FFFFFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>21</td><td>CMP0_IN5/ADC0_SE4b/PTE29/TPM0_CH2/TPM_CLKIN0</td><td>J10_9</td>
				<td bgcolor='#FFFFFF'>CMP0<br/>CMP0<br/>CMP0<br/>ADC0</td><td bgcolor='#FFFFFF'>cmp_in5<br/>cmp_neg5<br/>cmp_pos5<br/>adc_seb4</td><td bgcolor='#FFFFFF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port29</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch2</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td bgcolor='#86DAFF'>TPM0<br/>TPM1<br/>TPM2</td><td bgcolor='#86DAFF'>tmr_clk</td><td bgcolor='#86DAFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>22</td><td>DAC0_OUT/ADC0_SE23/CMP0_IN4/PTE30/TPM0_CH3/TPM_CLKIN1</td><td>J10_11</td>
				<td bgcolor='#FFFFFF'>DAC0<br/>ADC0<br/>CMP0<br/>CMP0<br/>CMP0</td><td bgcolor='#FFFFFF'>dac_out<br/>adc_se23<br/>cmp_in4<br/>cmp_neg4<br/>cmp_pos4</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port30</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch3</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td bgcolor='#86DAFF'>TPM0<br/>TPM1<br/>TPM2</td><td bgcolor='#86DAFF'>tmr_clk</td><td bgcolor='#86DAFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>23</td><td>PTE31/TPM0_CH4</td><td>J2_13</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port31</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch4</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>24</td><td>PTE24/TPM0_CH0/I2C0_SCL</td><td>ACCEL_SCL</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port24</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch0</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sclk</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>25</td><td>PTE25/TPM0_CH1/I2C0_SDA</td><td>ACCEL_SDA</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port25</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch1</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sda</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>26</td><td>TSI0_CH1/PTA0/TPM0_CH5/SWD_CLK</td><td>SWD_CLK/J11_1</td>
				<td bgcolor='#E5C3FF'>TSI0</td><td bgcolor='#E5C3FF'>tsi_ch1</td><td bgcolor='#E5C3FF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port0</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch5</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#EBD4BD'>SWD</td><td bgcolor='#EBD4BD'>swd_clk</td><td bgcolor='#EBD4BD'>Input/Output</td>
			</tr>
			<tr>
				<td>27</td><td>TSI0_CH2/PTA1/UART0_RX/TPM2_CH0</td><td>DBG_CONSOLE_RX/J1_2</td>
				<td bgcolor='#E5C3FF'>TSI0</td><td bgcolor='#E5C3FF'>tsi_ch2</td><td bgcolor='#E5C3FF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port1</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#20E04E'>UART0</td><td bgcolor='#20E04E'>uart_rx</td><td bgcolor='#20E04E'>Input</td>
				<td bgcolor='#86DAFF'>TPM2</td><td bgcolor='#86DAFF'>tmr_ch0</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>28</td><td>TSI0_CH3/PTA2/UART0_TX/TPM2_CH1</td><td>DBG_CONSOLE_TX/J1_4</td>
				<td bgcolor='#E5C3FF'>TSI0</td><td bgcolor='#E5C3FF'>tsi_ch3</td><td bgcolor='#E5C3FF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port2</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#20E04E'>UART0</td><td bgcolor='#20E04E'>uart_tx</td><td bgcolor='#20E04E'>Output</td>
				<td bgcolor='#86DAFF'>TPM2</td><td bgcolor='#86DAFF'>tmr_ch1</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>29</td><td>TSI0_CH4/PTA3/I2C1_SCL/TPM0_CH0/SWD_DIO</td><td>SWD_DIO</td>
				<td bgcolor='#E5C3FF'>TSI0</td><td bgcolor='#E5C3FF'>tsi_ch4</td><td bgcolor='#E5C3FF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port3</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C1</td><td bgcolor='#AFFF8E'>i2c_sclk</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch0</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#EBD4BD'>SWD</td><td bgcolor='#EBD4BD'>swd_dio</td><td bgcolor='#EBD4BD'>Input/Output</td>
			</tr>
			<tr>
				<td>30</td><td>TSI0_CH5/PTA4/I2C1_SDA/TPM0_CH1/NMI_b</td><td>J1_10</td>
				<td bgcolor='#E5C3FF'>TSI0</td><td bgcolor='#E5C3FF'>tsi_ch5</td><td bgcolor='#E5C3FF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port4</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C1</td><td bgcolor='#AFFF8E'>i2c_sda</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch1</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>SystemControl<br/>non-peripheral</td><td bgcolor='#FFFFFF'>scb_nmi<br/>NMI</td><td bgcolor='#FFFFFF'>Input</td>
			</tr>
			<tr>
				<td>31</td><td>PTA5/USB_CLKIN/TPM0_CH2</td><td>J1_12</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port5</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#00CA3A'>USB0</td><td bgcolor='#00CA3A'>usb_clkin</td><td bgcolor='#00CA3A'>Input</td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch2</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>32</td><td>PTA12/TPM1_CH0</td><td>J1_8</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port12</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM1</td><td bgcolor='#86DAFF'>tmr_ch0</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>33</td><td>PTA13/TPM1_CH1</td><td>J2_2</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port13</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM1</td><td bgcolor='#86DAFF'>tmr_ch1</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>34</td><td>PTA14/SPI0_PCS0/UART0_TX</td><td>ACCEL_INT1</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port14</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_cs0<br/>spi_ss</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#20E04E'>UART0</td><td bgcolor='#20E04E'>uart_tx</td><td bgcolor='#20E04E'>Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>35</td><td>PTA15/SPI0_SCK/UART0_RX</td><td>ACCEL_INT2</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port15</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_sck</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#20E04E'>UART0</td><td bgcolor='#20E04E'>uart_rx</td><td bgcolor='#20E04E'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>36</td><td>PTA16/SPI0_MOSI/SPI0_MISO</td><td>J2_9</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port16</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_mosi</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_miso</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>37</td><td>PTA17/SPI0_MISO/SPI0_MOSI</td><td>J2_11</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port17</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_miso</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_mosi</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>38</td><td>VDD48</td><td><small><i>same</i></small></td>
				<td bgcolor='#F7DCFF'>SUPPLY</td><td bgcolor='#F7DCFF'>pwr_vdd1</td><td bgcolor='#F7DCFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>39</td><td>VSS49</td><td><small><i>same</i></small></td>
				<td bgcolor='#F7DCFF'>SUPPLY</td><td bgcolor='#F7DCFF'>pwr_vss1</td><td bgcolor='#F7DCFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>40</td><td>EXTAL0/PTA18/UART1_RX/TPM_CLKIN0</td><td>EXTAL</td>
				<td bgcolor='#DDC7B5'>OSC0</td><td bgcolor='#DDC7B5'>extal</td><td bgcolor='#DDC7B5'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port18</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#5FE356'>UART1</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
				<td bgcolor='#86DAFF'>TPM0<br/>TPM1<br/>TPM2</td><td bgcolor='#86DAFF'>tmr_clk</td><td bgcolor='#86DAFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>41</td><td>XTAL0/PTA19/UART1_TX/TPM_CLKIN1/LPTMR0_ALT1</td><td>XTAL</td>
				<td bgcolor='#DDC7B5'>OSC0</td><td bgcolor='#DDC7B5'>xtal</td><td bgcolor='#DDC7B5'>Output</td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port19</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#5FE356'>UART1</td><td bgcolor='#5FE356'>uart_tx</td><td bgcolor='#5FE356'>Output</td>
				<td bgcolor='#86DAFF'>TPM0<br/>TPM1<br/>TPM2</td><td bgcolor='#86DAFF'>tmr_clk</td><td bgcolor='#86DAFF'>Input</td>
				<td></td><td></td><td></td>
				<td bgcolor='#CEFFFF'>LPTMR0</td><td bgcolor='#CEFFFF'>tmr_clk1</td><td bgcolor='#CEFFFF'>Input</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>42</td><td>PTA20/RESET_b</td><td>RESET</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port20</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#CCB6A0'>RCM</td><td bgcolor='#CCB6A0'>reset</td><td bgcolor='#CCB6A0'>Input</td>
			</tr>
			<tr>
				<td>43</td><td>ADC0_SE8/TSI0_CH0/PTB0/LLWU_P5/I2C0_SCL/TPM1_CH0</td><td>J10_2</td>
				<td bgcolor='#FFFFFF'>ADC0<br/>TSI0</td><td bgcolor='#FFFFFF'>adc_se8<br/>tsi_ch0</td><td bgcolor='#FFFFFF'>Input</td>
				<td bgcolor='#FFFFFF'>GPIOB<br/>LLWU</td><td bgcolor='#FFFFFF'>port0<br/>llwu_wakeup5</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sclk</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td bgcolor='#86DAFF'>TPM1</td><td bgcolor='#86DAFF'>tmr_ch0</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>44</td><td>ADC0_SE9/TSI0_CH6/PTB1/I2C0_SDA/TPM1_CH1</td><td>J10_4</td>
				<td bgcolor='#FFFFFF'>ADC0<br/>TSI0</td><td bgcolor='#FFFFFF'>adc_se9<br/>tsi_ch6</td><td bgcolor='#FFFFFF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port1</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sda</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td bgcolor='#86DAFF'>TPM1</td><td bgcolor='#86DAFF'>tmr_ch1</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>45</td><td>ADC0_SE12/TSI0_CH7/PTB2/I2C0_SCL/TPM2_CH0</td><td>J10_6</td>
				<td bgcolor='#FFFFFF'>ADC0<br/>TSI0</td><td bgcolor='#FFFFFF'>adc_se12<br/>tsi_ch7</td><td bgcolor='#FFFFFF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port2</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sclk</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td bgcolor='#86DAFF'>TPM2</td><td bgcolor='#86DAFF'>tmr_ch0</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>46</td><td>ADC0_SE13/TSI0_CH8/PTB3/I2C0_SDA/TPM2_CH1</td><td>J10_8</td>
				<td bgcolor='#FFFFFF'>ADC0<br/>TSI0</td><td bgcolor='#FFFFFF'>adc_se13<br/>tsi_ch8</td><td bgcolor='#FFFFFF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port3</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sda</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td bgcolor='#86DAFF'>TPM2</td><td bgcolor='#86DAFF'>tmr_ch1</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>47</td><td>PTB8/EXTRG_IN</td><td>J9_1</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port8</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>ADC0<br/>ADC0<br/>TPM0<br/>TPM1<br/>TPM2</td><td bgcolor='#FFFFFF'>adc_triggerA<br/>adc_triggerB<br/>tmr_trigger<br/>tmr_trigger<br/>tmr_trigger</td><td bgcolor='#FFFFFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>48</td><td>PTB9</td><td>J9_3</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port9</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>49</td><td>PTB10/SPI1_PCS0</td><td>J9_5</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port10</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_cs0<br/>spi_ss</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>50</td><td>PTB11/SPI1_SCK</td><td>J9_7</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port11</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_sck</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>51</td><td>TSI0_CH9/PTB16/SPI1_MOSI/UART0_RX/TPM_CLKIN0/SPI1_MISO</td><td>TOUCH_SLIDER_A</td>
				<td bgcolor='#E5C3FF'>TSI0</td><td bgcolor='#E5C3FF'>tsi_ch9</td><td bgcolor='#E5C3FF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port16</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_mosi</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#20E04E'>UART0</td><td bgcolor='#20E04E'>uart_rx</td><td bgcolor='#20E04E'>Input</td>
				<td bgcolor='#86DAFF'>TPM0<br/>TPM1<br/>TPM2</td><td bgcolor='#86DAFF'>tmr_clk</td><td bgcolor='#86DAFF'>Input</td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_miso</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>52</td><td>TSI0_CH10/PTB17/SPI1_MISO/UART0_TX/TPM_CLKIN1/SPI1_MOSI</td><td>TOUCH_SLIDER_B</td>
				<td bgcolor='#E5C3FF'>TSI0</td><td bgcolor='#E5C3FF'>tsi_ch10</td><td bgcolor='#E5C3FF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port17</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_miso</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#20E04E'>UART0</td><td bgcolor='#20E04E'>uart_tx</td><td bgcolor='#20E04E'>Output</td>
				<td bgcolor='#86DAFF'>TPM0<br/>TPM1<br/>TPM2</td><td bgcolor='#86DAFF'>tmr_clk</td><td bgcolor='#86DAFF'>Input</td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_mosi</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>53</td><td>TSI0_CH11/PTB18/TPM2_CH0</td><td>LEDRGB_RED</td>
				<td bgcolor='#E5C3FF'>TSI0</td><td bgcolor='#E5C3FF'>tsi_ch11</td><td bgcolor='#E5C3FF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port18</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM2</td><td bgcolor='#86DAFF'>tmr_ch0</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>54</td><td>TSI0_CH12/PTB19/TPM2_CH1</td><td>LEDRGB_GREEN</td>
				<td bgcolor='#E5C3FF'>TSI0</td><td bgcolor='#E5C3FF'>tsi_ch12</td><td bgcolor='#E5C3FF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port19</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM2</td><td bgcolor='#86DAFF'>tmr_ch1</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>55</td><td>ADC0_SE14/TSI0_CH13/PTC0/EXTRG_IN/CMP0_OUT</td><td>J1_3</td>
				<td bgcolor='#FFFFFF'>ADC0<br/>TSI0</td><td bgcolor='#FFFFFF'>adc_se14<br/>tsi_ch13</td><td bgcolor='#FFFFFF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port0</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>ADC0<br/>ADC0<br/>TPM0<br/>TPM1<br/>TPM2</td><td bgcolor='#FFFFFF'>adc_triggerA<br/>adc_triggerB<br/>tmr_trigger<br/>tmr_trigger<br/>tmr_trigger</td><td bgcolor='#FFFFFF'>Input</td>
				<td></td><td></td><td></td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>cmp_out</td><td bgcolor='#EFF174'>Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>56</td><td>ADC0_SE15/TSI0_CH14/PTC1/LLWU_P6/RTC_CLKIN/I2C1_SCL/TPM0_CH0</td><td>J10_12</td>
				<td bgcolor='#FFFFFF'>ADC0<br/>TSI0</td><td bgcolor='#FFFFFF'>adc_se15<br/>tsi_ch14</td><td bgcolor='#FFFFFF'>Input</td>
				<td bgcolor='#FFFFFF'>GPIOC<br/>LLWU<br/>RTC</td><td bgcolor='#FFFFFF'>port1<br/>llwu_wakeup6<br/>rtc_clkin</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C1</td><td bgcolor='#AFFF8E'>i2c_sclk</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch0</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>57</td><td>ADC0_SE11/TSI0_CH15/PTC2/I2C1_SDA/TPM0_CH1</td><td>J10_10</td>
				<td bgcolor='#FFFFFF'>ADC0<br/>TSI0</td><td bgcolor='#FFFFFF'>adc_se11<br/>tsi_ch15</td><td bgcolor='#FFFFFF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port2</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C1</td><td bgcolor='#AFFF8E'>i2c_sda</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch1</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>58</td><td>PTC3/LLWU_P7/UART1_RX/TPM0_CH2/CLKOUTa</td><td>J1_5</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>GPIOC<br/>LLWU</td><td bgcolor='#FFFFFF'>port3<br/>llwu_wakeup7</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#5FE356'>UART1</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch2</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td bgcolor='#FFE1C7'>SIM</td><td bgcolor='#FFE1C7'>clkout</td><td bgcolor='#FFE1C7'>Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>59</td><td>VSS74</td><td><small><i>same</i></small></td>
				<td bgcolor='#F7DCFF'>SUPPLY</td><td bgcolor='#F7DCFF'>pwr_vss2</td><td bgcolor='#F7DCFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>60</td><td>VDD75</td><td><small><i>same</i></small></td>
				<td bgcolor='#F7DCFF'>SUPPLY</td><td bgcolor='#F7DCFF'>pwr_vdd2</td><td bgcolor='#F7DCFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>61</td><td>PTC4/LLWU_P8/SPI0_PCS0/UART1_TX/TPM0_CH3</td><td>J1_7</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>GPIOC<br/>LLWU</td><td bgcolor='#FFFFFF'>port4<br/>llwu_wakeup8</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_cs0<br/>spi_ss</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#5FE356'>UART1</td><td bgcolor='#5FE356'>uart_tx</td><td bgcolor='#5FE356'>Output</td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch3</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>62</td><td>PTC5/LLWU_P9/SPI0_SCK/LPTMR0_ALT2/CMP0_OUT</td><td>J1_9</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>GPIOC<br/>LLWU</td><td bgcolor='#FFFFFF'>port5<br/>llwu_wakeup9</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_sck</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#CEFFFF'>LPTMR0</td><td bgcolor='#CEFFFF'>tmr_clk2</td><td bgcolor='#CEFFFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>cmp_out</td><td bgcolor='#EFF174'>Output</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>63</td><td>CMP0_IN0/PTC6/LLWU_P10/SPI0_MOSI/EXTRG_IN/SPI0_MISO</td><td>J1_11</td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>cmp_in0<br/>cmp_neg0<br/>cmp_pos0</td><td bgcolor='#EFF174'>Input</td>
				<td bgcolor='#FFFFFF'>GPIOC<br/>LLWU</td><td bgcolor='#FFFFFF'>port6<br/>llwu_wakeup10</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_mosi</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#FFFFFF'>ADC0<br/>ADC0<br/>TPM0<br/>TPM1<br/>TPM2</td><td bgcolor='#FFFFFF'>adc_triggerA<br/>adc_triggerB<br/>tmr_trigger<br/>tmr_trigger<br/>tmr_trigger</td><td bgcolor='#FFFFFF'>Input</td>
				<td></td><td></td><td></td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_miso</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>64</td><td>CMP0_IN1/PTC7/SPI0_MISO/SPI0_MOSI</td><td>J1_1</td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>cmp_in1<br/>cmp_neg1<br/>cmp_pos1</td><td bgcolor='#EFF174'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port7</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_miso</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_mosi</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>65</td><td>CMP0_IN2/PTC8/I2C0_SCL/TPM0_CH4</td><td>J1_14</td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>cmp_in2<br/>cmp_neg2<br/>cmp_pos2</td><td bgcolor='#EFF174'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port8</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sclk</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch4</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>66</td><td>CMP0_IN3/PTC9/I2C0_SDA/TPM0_CH5</td><td>J1_16</td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>cmp_in3<br/>cmp_neg3<br/>cmp_pos3</td><td bgcolor='#EFF174'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port9</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sda</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch5</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>67</td><td>PTC10/I2C1_SCL</td><td>J1_13</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port10</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C1</td><td bgcolor='#AFFF8E'>i2c_sclk</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>68</td><td>PTC11/I2C1_SDA</td><td>J1_15</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port11</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C1</td><td bgcolor='#AFFF8E'>i2c_sda</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>69</td><td>PTC12/TPM_CLKIN0</td><td>J2_1</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port12</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM0<br/>TPM1<br/>TPM2</td><td bgcolor='#86DAFF'>tmr_clk</td><td bgcolor='#86DAFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>70</td><td>PTC13/TPM_CLKIN1</td><td>J2_3</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port13</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM0<br/>TPM1<br/>TPM2</td><td bgcolor='#86DAFF'>tmr_clk</td><td bgcolor='#86DAFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>71</td><td>PTC16</td><td>J2_5</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port16</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>72</td><td>PTC17</td><td>J2_7</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port17</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>73</td><td>PTD0/SPI0_PCS0/TPM0_CH0</td><td>J2_6</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOD</td><td bgcolor='#F7DCFF'>port0</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_cs0<br/>spi_ss</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch0</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>74</td><td>ADC0_SE5b/PTD1/SPI0_SCK/TPM0_CH1</td><td>LEDRGB_BLUE/J2_12</td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_seb5</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOD</td><td bgcolor='#F7DCFF'>port1</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_sck</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch1</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>75</td><td>PTD2/SPI0_MOSI/UART2_RX/TPM0_CH2/SPI0_MISO</td><td>J2_8</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOD</td><td bgcolor='#F7DCFF'>port2</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_mosi</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#5FE356'>UART2</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch2</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_miso</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>76</td><td>PTD3/SPI0_MISO/UART2_TX/TPM0_CH3/SPI0_MOSI</td><td>J2_10</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOD</td><td bgcolor='#F7DCFF'>port3</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_miso</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#5FE356'>UART2</td><td bgcolor='#5FE356'>uart_tx</td><td bgcolor='#5FE356'>Output</td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch3</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_mosi</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>77</td><td>PTD4/LLWU_P14/SPI1_PCS0/UART2_RX/TPM0_CH4</td><td>J1_6</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>GPIOD<br/>LLWU</td><td bgcolor='#FFFFFF'>port4<br/>llwu_wakeup14</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_cs0<br/>spi_ss</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#5FE356'>UART2</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch4</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>78</td><td>ADC0_SE6b/PTD5/SPI1_SCK/UART2_TX/TPM0_CH5</td><td>J2_4</td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_seb6</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOD</td><td bgcolor='#F7DCFF'>port5</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_sck</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#5FE356'>UART2</td><td bgcolor='#5FE356'>uart_tx</td><td bgcolor='#5FE356'>Output</td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch5</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>79</td><td>ADC0_SE7b/PTD6/LLWU_P15/SPI1_MOSI/UART0_RX/SPI1_MISO</td><td>J2_17</td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_seb7</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#FFFFFF'>GPIOD<br/>LLWU</td><td bgcolor='#FFFFFF'>port6<br/>llwu_wakeup15</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_mosi</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#20E04E'>UART0</td><td bgcolor='#20E04E'>uart_rx</td><td bgcolor='#20E04E'>Input</td>
				<td></td><td></td><td></td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_miso</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>80</td><td>PTD7/SPI1_MISO/UART0_TX/SPI1_MOSI</td><td>J2_19</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOD</td><td bgcolor='#F7DCFF'>port7</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_miso</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#20E04E'>UART0</td><td bgcolor='#20E04E'>uart_tx</td><td bgcolor='#20E04E'>Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_mosi</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
		</table>

*/
/*!
\page page_pinalloc Pin Allocation

		<h2 style='font-family: Arial;'>Pin Allocation Report</h2>
		<table cellpadding='2' border='1' style='border: 2px solid #000000;' bgcolor='WHITE' align='center'>
			<tr bgcolor='#E8E8E8'><th>Peripheral</th><th>Custom peripheral name</th><th>Peripheral description</th></tr>
			<tr bgcolor='#F8FF9A'><td>ADC0</td><td>ADC0</td><td><small>Analog-to-Digital Converter</small></td></tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>CMP0</td><td><small>High-Speed Comparator (CMP), Voltage Reference (VREF) Digital-to-Analog Converter (DAC), and Analog Mux (ANMUX)</small></td></tr>
			<tr bgcolor='#E5E44D'><td>DAC0</td><td>DAC0</td><td><small>12-Bit Digital-to-Analog Converter</small></td></tr>
			<tr bgcolor='#F7DCFF'><td>GPIOA</td><td>GPIOA</td><td><small>General Purpose Input/Output</small></td></tr>
			<tr bgcolor='#F7DCFF'><td>GPIOB</td><td>GPIOB</td><td><small>General Purpose Input/Output</small></td></tr>
			<tr bgcolor='#F7DCFF'><td>GPIOC</td><td>GPIOC</td><td><small>General Purpose Input/Output</small></td></tr>
			<tr bgcolor='#F7DCFF'><td>GPIOD</td><td>GPIOD</td><td><small>General Purpose Input/Output</small></td></tr>
			<tr bgcolor='#F7DCFF'><td>GPIOE</td><td>GPIOE</td><td><small>General Purpose Input/Output</small></td></tr>
			<tr bgcolor='#AFFF8E'><td>I2C0</td><td>I2C0</td><td><small>Inter-integrated circuit bus</small></td></tr>
			<tr bgcolor='#AFFF8E'><td>I2C1</td><td>I2C1</td><td><small>Inter-integrated circuit bus</small></td></tr>
			<tr bgcolor='#EBD4BD'><td>LLWU</td><td>LLWU</td><td><small>Low Leakage Wake-up Unit</small></td></tr>
			<tr bgcolor='#CEFFFF'><td>LPTMR0</td><td>LPTMR0</td><td><small>Low Power Timer Module</small></td></tr>
			<tr bgcolor='#DDC7B5'><td>OSC0</td><td>OSC0</td><td><small>Oscillator</small></td></tr>
			<tr bgcolor='#CCB6A0'><td>RCM</td><td>RCM</td><td><small>Reset Control Module</small></td></tr>
			<tr bgcolor='#B3EAFF'><td>RTC</td><td>RTC</td><td><small>Real Time Clock - RTC</small></td></tr>
			<tr bgcolor='#FFE1C7'><td>SIM</td><td>SIM</td><td><small>System Integration Module</small></td></tr>
			<tr bgcolor='#90EE67'><td>SPI0</td><td>SPI0</td><td><small>Serial Peripheral Interface</small></td></tr>
			<tr bgcolor='#90EE67'><td>SPI1</td><td>SPI1</td><td><small>Serial Peripheral Interface</small></td></tr>
			<tr bgcolor='#F7DCFF'><td>SUPPLY</td><td>SUPPLY</td><td><small>Chip power supply</small></td></tr>
			<tr bgcolor='#EBD4BD'><td>SWD</td><td>SWD</td><td><small>Serial wire debug interface</small></td></tr>
			<tr bgcolor='#C7A886'><td>SystemControl</td><td>SystemControl</td><td><small>System control</small></td></tr>
			<tr bgcolor='#86DAFF'><td>TPM0</td><td>TPM0</td><td><small>Timer/PWM Module</small></td></tr>
			<tr bgcolor='#86DAFF'><td>TPM1</td><td>TPM1</td><td><small>Timer/PWM Module</small></td></tr>
			<tr bgcolor='#86DAFF'><td>TPM2</td><td>TPM2</td><td><small>Timer/PWM Module</small></td></tr>
			<tr bgcolor='#E5C3FF'><td>TSI0</td><td>TSI0</td><td><small>Touch Sensing Input</small></td></tr>
			<tr bgcolor='#20E04E'><td>UART0</td><td>UART0</td><td><small>Serial Communications Interface Module UART0</small></td></tr>
			<tr bgcolor='#5FE356'><td>UART1</td><td>UART1</td><td><small>Serial Communications Interface Module UART1</small></td></tr>
			<tr bgcolor='#5FE356'><td>UART2</td><td>UART2</td><td><small>Serial Communications Interface Module UART2</small></td></tr>
			<tr bgcolor='#00CA3A'><td>USB0</td><td>USB0</td><td><small>Universal Serial Bus On The Go - USB0</small></td></tr>
		</table>
		<br/>
		<br/>

		<h2 style='font-family: Arial;'>Routed Pins</h2>
		<table cellpadding='2' border='1' style='border: 2px solid #000000;' bgcolor='WHITE' width='100%' align='center'>
			<tr><td colspan='3'></td><th colspan='4' align='center' bgcolor='#D0D0D0'>Assigned Pin Function(s)</th></tr>
			<tr>
				<th bgcolor='#E8E8E8'>Package Pin #</th><th bgcolor='#E8E8E8'>Pin Name</th><th bgcolor='#E8E8E8'>User Assigned Signal Name</th><th bgcolor='#E8E8E8'>Assigned Peripheral</th><th bgcolor='#E8E8E8'>Assigned Function</th><th bgcolor='#E8E8E8'>Package Function</th><th bgcolor='#E8E8E8'>Dir</th>
			</tr>
			<tr>
				<td>1</td><td>PTE0/UART1_TX/RTC_CLKOUT/CMP0_OUT/I2C1_SDA</td><td>J2_18</td>
				<td bgcolor='#5FE356'>UART1</td><td bgcolor='#5FE356'>uart_tx</td><td bgcolor='#5FE356'>alt3</td><td bgcolor='#5FE356'>Output</td>
			</tr>
			<tr>
				<td>2</td><td>PTE1/SPI1_MOSI/UART1_RX/SPI1_MISO/I2C1_SCL</td><td>J2_20</td>
				<td bgcolor='#5FE356'>UART1</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>alt3</td><td bgcolor='#5FE356'>Input</td>
			</tr>
			<tr>
				<td>3</td><td>PTE2/SPI1_SCK</td><td>J9_9</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>4</td><td>PTE3/SPI1_MISO/SPI1_MOSI</td><td>J9_11</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>5</td><td>PTE4/SPI1_PCS0</td><td>J9_13</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>6</td><td>PTE5</td><td>J9_15</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>7</td><td>VDD8</td><td><small><i>same</i></small></td>
				<td bgcolor='#F7DCFF'>SUPPLY</td><td bgcolor='#F7DCFF'>pwr_vdd0</td><td bgcolor='#F7DCFF'>alt0</td><td bgcolor='#F7DCFF'>Input</td>
			</tr>
			<tr>
				<td>8</td><td>VSS9</td><td><small><i>same</i></small></td>
				<td bgcolor='#F7DCFF'>SUPPLY</td><td bgcolor='#F7DCFF'>pwr_vss0</td><td bgcolor='#F7DCFF'>alt0</td><td bgcolor='#F7DCFF'>Input</td>
			</tr>
			<tr>
				<td>9</td><td>USB0_DP</td><td><small><i>same</i></small></td>
				<td bgcolor='#00CA3A'>USB0</td><td bgcolor='#00CA3A'>usb_dp</td><td bgcolor='#00CA3A'>alt0</td><td bgcolor='#00CA3A'>Input</td>
			</tr>
			<tr>
				<td>10</td><td>USB0_DM</td><td><small><i>same</i></small></td>
				<td bgcolor='#00CA3A'>USB0</td><td bgcolor='#00CA3A'>usb_dm</td><td bgcolor='#00CA3A'>alt0</td><td bgcolor='#00CA3A'>Input</td>
			</tr>
			<tr>
				<td>11</td><td>VOUT33</td><td><small><i>same</i></small></td>
				<td bgcolor='#00CA3A'>USB0</td><td bgcolor='#00CA3A'>usb_vout</td><td bgcolor='#00CA3A'>alt0</td><td bgcolor='#00CA3A'>Output</td>
			</tr>
			<tr>
				<td>12</td><td>VREGIN</td><td><small><i>same</i></small></td>
				<td bgcolor='#00CA3A'>USB0</td><td bgcolor='#00CA3A'>usb_vrin</td><td bgcolor='#00CA3A'>alt0</td><td bgcolor='#00CA3A'>Input</td>
			</tr>
			<tr>
				<td rowspan='2'>13</td><td rowspan='2'>ADC0_DP0/ADC0_SE0/PTE20/TPM1_CH0/UART0_TX</td><td rowspan='2'>J10_1</td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_dp0</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC0</td><td>adc_se0</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='2'>14</td><td rowspan='2'>ADC0_DM0/ADC0_SE4a/PTE21/TPM1_CH1/UART0_RX</td><td rowspan='2'>J10_3</td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_dm0</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC0</td><td>adc_sea4</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='2'>15</td><td rowspan='2'>ADC0_DP3/ADC0_SE3/PTE22/TPM2_CH0/UART2_TX</td><td rowspan='2'>J10_5</td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_dp3</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC0</td><td>adc_se3</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='2'>16</td><td rowspan='2'>ADC0_DM3/ADC0_SE7a/PTE23/TPM2_CH1/UART2_RX</td><td rowspan='2'>J10_7</td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_dm3</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC0</td><td>adc_sea7</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='2'>17</td><td rowspan='2'>VDDA</td><td rowspan='2'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_vref_vdda</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F7DCFF'><td>SUPPLY</td><td>pwr_vdda0</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td>18</td><td>VREFH</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_vref_vrefh</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr>
				<td>19</td><td>VREFL</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_vref_vrefl</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr>
				<td rowspan='2'>20</td><td rowspan='2'>VSSA</td><td rowspan='2'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_vref_vssa</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F7DCFF'><td>SUPPLY</td><td>pwr_vssa0</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='4'>21</td><td rowspan='4'>CMP0_IN5/ADC0_SE4b/PTE29/TPM0_CH2/TPM_CLKIN0</td><td rowspan='4'>J10_9</td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>cmp_in5</td><td bgcolor='#EFF174'>alt0</td><td bgcolor='#EFF174'>Input</td>
			</tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>cmp_neg5</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>cmp_pos5</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#F8FF9A'><td>ADC0</td><td>adc_seb4</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td>22</td><td>DAC0_OUT/ADC0_SE23/CMP0_IN4/PTE30/TPM0_CH3/TPM_CLKIN1</td><td>J10_11</td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port30</td><td bgcolor='#F7DCFF'>alt1</td><td bgcolor='#F7DCFF'>Output</td>
			</tr>
			<tr>
				<td>23</td><td>PTE31/TPM0_CH4</td><td>J2_13</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>24</td><td>PTE24/TPM0_CH0/I2C0_SCL</td><td>ACCEL_SCL</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>25</td><td>PTE25/TPM0_CH1/I2C0_SDA</td><td>ACCEL_SDA</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>26</td><td>TSI0_CH1/PTA0/TPM0_CH5/SWD_CLK</td><td>SWD_CLK/J11_1</td>
				<td bgcolor='#EBD4BD'>SWD</td><td bgcolor='#EBD4BD'>swd_clk</td><td bgcolor='#EBD4BD'>alt7</td><td bgcolor='#EBD4BD'>Input/Output</td>
			</tr>
			<tr>
				<td>27</td><td>TSI0_CH2/PTA1/UART0_RX/TPM2_CH0</td><td>DBG_CONSOLE_RX/J1_2</td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port1</td><td bgcolor='#F7DCFF'>alt1</td><td bgcolor='#F7DCFF'>Output</td>
			</tr>
			<tr>
				<td>28</td><td>TSI0_CH3/PTA2/UART0_TX/TPM2_CH1</td><td>DBG_CONSOLE_TX/J1_4</td>
				<td bgcolor='#E5C3FF'>TSI0</td><td bgcolor='#E5C3FF'>tsi_ch3</td><td bgcolor='#E5C3FF'>alt0</td><td bgcolor='#E5C3FF'>Input</td>
			</tr>
			<tr>
				<td>29</td><td>TSI0_CH4/PTA3/I2C1_SCL/TPM0_CH0/SWD_DIO</td><td>SWD_DIO</td>
				<td bgcolor='#EBD4BD'>SWD</td><td bgcolor='#EBD4BD'>swd_dio</td><td bgcolor='#EBD4BD'>alt7</td><td bgcolor='#EBD4BD'>Input/Output</td>
			</tr>
			<tr>
				<td rowspan='2'>30</td><td rowspan='2'>TSI0_CH5/PTA4/I2C1_SDA/TPM0_CH1/NMI_b</td><td rowspan='2'>J1_10</td>
				<td bgcolor='#C7A886'>SystemControl</td><td bgcolor='#C7A886'>scb_nmi</td><td bgcolor='#C7A886'>alt7</td><td bgcolor='#C7A886'>Input</td>
			</tr>
			<tr bgcolor='#969696'><td>non-peripheral</td><td>NMI</td><td>alt7</td><td>Not Specified</td></tr>
			<tr>
				<td>31</td><td>PTA5/USB_CLKIN/TPM0_CH2</td><td>J1_12</td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port5</td><td bgcolor='#F7DCFF'>alt1</td><td bgcolor='#F7DCFF'>Output</td>
			</tr>
			<tr>
				<td>32</td><td>PTA12/TPM1_CH0</td><td>J1_8</td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port12</td><td bgcolor='#F7DCFF'>alt1</td><td bgcolor='#F7DCFF'>Not Specified</td>
			</tr>
			<tr>
				<td>33</td><td>PTA13/TPM1_CH1</td><td>J2_2</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>34</td><td>PTA14/SPI0_PCS0/UART0_TX</td><td>ACCEL_INT1</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>35</td><td>PTA15/SPI0_SCK/UART0_RX</td><td>ACCEL_INT2</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>36</td><td>PTA16/SPI0_MOSI/SPI0_MISO</td><td>J2_9</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>37</td><td>PTA17/SPI0_MISO/SPI0_MOSI</td><td>J2_11</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>38</td><td>VDD48</td><td><small><i>same</i></small></td>
				<td bgcolor='#F7DCFF'>SUPPLY</td><td bgcolor='#F7DCFF'>pwr_vdd1</td><td bgcolor='#F7DCFF'>alt0</td><td bgcolor='#F7DCFF'>Input</td>
			</tr>
			<tr>
				<td>39</td><td>VSS49</td><td><small><i>same</i></small></td>
				<td bgcolor='#F7DCFF'>SUPPLY</td><td bgcolor='#F7DCFF'>pwr_vss1</td><td bgcolor='#F7DCFF'>alt0</td><td bgcolor='#F7DCFF'>Input</td>
			</tr>
			<tr>
				<td>40</td><td>EXTAL0/PTA18/UART1_RX/TPM_CLKIN0</td><td>EXTAL</td>
				<td bgcolor='#DDC7B5'>OSC0</td><td bgcolor='#DDC7B5'>extal</td><td bgcolor='#DDC7B5'>alt0</td><td bgcolor='#DDC7B5'>Input</td>
			</tr>
			<tr>
				<td>41</td><td>XTAL0/PTA19/UART1_TX/TPM_CLKIN1/LPTMR0_ALT1</td><td>XTAL</td>
				<td bgcolor='#DDC7B5'>OSC0</td><td bgcolor='#DDC7B5'>xtal</td><td bgcolor='#DDC7B5'>alt0</td><td bgcolor='#DDC7B5'>Output</td>
			</tr>
			<tr>
				<td>42</td><td>PTA20/RESET_b</td><td>RESET</td>
				<td bgcolor='#CCB6A0'>RCM</td><td bgcolor='#CCB6A0'>reset</td><td bgcolor='#CCB6A0'>alt7</td><td bgcolor='#CCB6A0'>Input</td>
			</tr>
			<tr>
				<td>43</td><td>ADC0_SE8/TSI0_CH0/PTB0/LLWU_P5/I2C0_SCL/TPM1_CH0</td><td>J10_2</td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sclk</td><td bgcolor='#AFFF8E'>alt2</td><td bgcolor='#AFFF8E'>Input/Output</td>
			</tr>
			<tr>
				<td>44</td><td>ADC0_SE9/TSI0_CH6/PTB1/I2C0_SDA/TPM1_CH1</td><td>J10_4</td>
				<td bgcolor='#86DAFF'>TPM1</td><td bgcolor='#86DAFF'>tmr_ch1</td><td bgcolor='#86DAFF'>alt3</td><td bgcolor='#86DAFF'>Not Specified</td>
			</tr>
			<tr>
				<td rowspan='2'>45</td><td rowspan='2'>ADC0_SE12/TSI0_CH7/PTB2/I2C0_SCL/TPM2_CH0</td><td rowspan='2'>J10_6</td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_se12</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#E5C3FF'><td>TSI0</td><td>tsi_ch7</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td>46</td><td>ADC0_SE13/TSI0_CH8/PTB3/I2C0_SDA/TPM2_CH1</td><td>J10_8</td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sda</td><td bgcolor='#AFFF8E'>alt2</td><td bgcolor='#AFFF8E'>Input/Output</td>
			</tr>
			<tr>
				<td>47</td><td>PTB8/EXTRG_IN</td><td>J9_1</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>48</td><td>PTB9</td><td>J9_3</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>49</td><td>PTB10/SPI1_PCS0</td><td>J9_5</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>50</td><td>PTB11/SPI1_SCK</td><td>J9_7</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>51</td><td>TSI0_CH9/PTB16/SPI1_MOSI/UART0_RX/TPM_CLKIN0/SPI1_MISO</td><td>TOUCH_SLIDER_A</td>
				<td bgcolor='#E5C3FF'>TSI0</td><td bgcolor='#E5C3FF'>tsi_ch9</td><td bgcolor='#E5C3FF'>alt0</td><td bgcolor='#E5C3FF'>Input</td>
			</tr>
			<tr>
				<td>52</td><td>TSI0_CH10/PTB17/SPI1_MISO/UART0_TX/TPM_CLKIN1/SPI1_MOSI</td><td>TOUCH_SLIDER_B</td>
				<td bgcolor='#E5C3FF'>TSI0</td><td bgcolor='#E5C3FF'>tsi_ch10</td><td bgcolor='#E5C3FF'>alt0</td><td bgcolor='#E5C3FF'>Input</td>
			</tr>
			<tr>
				<td>53</td><td>TSI0_CH11/PTB18/TPM2_CH0</td><td>LEDRGB_RED</td>
				<td bgcolor='#E5C3FF'>TSI0</td><td bgcolor='#E5C3FF'>tsi_ch11</td><td bgcolor='#E5C3FF'>alt0</td><td bgcolor='#E5C3FF'>Input</td>
			</tr>
			<tr>
				<td>54</td><td>TSI0_CH12/PTB19/TPM2_CH1</td><td>LEDRGB_GREEN</td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port19</td><td bgcolor='#F7DCFF'>alt1</td><td bgcolor='#F7DCFF'>Output</td>
			</tr>
			<tr>
				<td>55</td><td>ADC0_SE14/TSI0_CH13/PTC0/EXTRG_IN/CMP0_OUT</td><td>J1_3</td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port0</td><td bgcolor='#F7DCFF'>alt1</td><td bgcolor='#F7DCFF'>Output</td>
			</tr>
			<tr>
				<td>56</td><td>ADC0_SE15/TSI0_CH14/PTC1/LLWU_P6/RTC_CLKIN/I2C1_SCL/TPM0_CH0</td><td>J10_12</td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch0</td><td bgcolor='#86DAFF'>alt4</td><td bgcolor='#86DAFF'>Not Specified</td>
			</tr>
			<tr>
				<td>57</td><td>ADC0_SE11/TSI0_CH15/PTC2/I2C1_SDA/TPM0_CH1</td><td>J10_10</td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port2</td><td bgcolor='#F7DCFF'>alt1</td><td bgcolor='#F7DCFF'>Output</td>
			</tr>
			<tr>
				<td>58</td><td>PTC3/LLWU_P7/UART1_RX/TPM0_CH2/CLKOUTa</td><td>J1_5</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>59</td><td>VSS74</td><td><small><i>same</i></small></td>
				<td bgcolor='#F7DCFF'>SUPPLY</td><td bgcolor='#F7DCFF'>pwr_vss2</td><td bgcolor='#F7DCFF'>alt0</td><td bgcolor='#F7DCFF'>Input</td>
			</tr>
			<tr>
				<td>60</td><td>VDD75</td><td><small><i>same</i></small></td>
				<td bgcolor='#F7DCFF'>SUPPLY</td><td bgcolor='#F7DCFF'>pwr_vdd2</td><td bgcolor='#F7DCFF'>alt0</td><td bgcolor='#F7DCFF'>Input</td>
			</tr>
			<tr>
				<td>61</td><td>PTC4/LLWU_P8/SPI0_PCS0/UART1_TX/TPM0_CH3</td><td>J1_7</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>62</td><td>PTC5/LLWU_P9/SPI0_SCK/LPTMR0_ALT2/CMP0_OUT</td><td>J1_9</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td rowspan='3'>63</td><td rowspan='3'>CMP0_IN0/PTC6/LLWU_P10/SPI0_MOSI/EXTRG_IN/SPI0_MISO</td><td rowspan='3'>J1_11</td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>cmp_in0</td><td bgcolor='#EFF174'>alt0</td><td bgcolor='#EFF174'>Input</td>
			</tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>cmp_neg0</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>cmp_pos0</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='3'>64</td><td rowspan='3'>CMP0_IN1/PTC7/SPI0_MISO/SPI0_MOSI</td><td rowspan='3'>J1_1</td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>cmp_in1</td><td bgcolor='#EFF174'>alt0</td><td bgcolor='#EFF174'>Input</td>
			</tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>cmp_neg1</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>cmp_pos1</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='3'>65</td><td rowspan='3'>CMP0_IN2/PTC8/I2C0_SCL/TPM0_CH4</td><td rowspan='3'>J1_14</td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>cmp_in2</td><td bgcolor='#EFF174'>alt0</td><td bgcolor='#EFF174'>Input</td>
			</tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>cmp_neg2</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>cmp_pos2</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='3'>66</td><td rowspan='3'>CMP0_IN3/PTC9/I2C0_SDA/TPM0_CH5</td><td rowspan='3'>J1_16</td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>cmp_in3</td><td bgcolor='#EFF174'>alt0</td><td bgcolor='#EFF174'>Input</td>
			</tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>cmp_neg3</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>cmp_pos3</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td>67</td><td>PTC10/I2C1_SCL</td><td>J1_13</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>68</td><td>PTC11/I2C1_SDA</td><td>J1_15</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>69</td><td>PTC12/TPM_CLKIN0</td><td>J2_1</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>70</td><td>PTC13/TPM_CLKIN1</td><td>J2_3</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>71</td><td>PTC16</td><td>J2_5</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>72</td><td>PTC17</td><td>J2_7</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>73</td><td>PTD0/SPI0_PCS0/TPM0_CH0</td><td>J2_6</td>
				<td bgcolor='#F7DCFF'>GPIOD</td><td bgcolor='#F7DCFF'>port0</td><td bgcolor='#F7DCFF'>alt1</td><td bgcolor='#F7DCFF'>Not Specified</td>
			</tr>
			<tr>
				<td>74</td><td>ADC0_SE5b/PTD1/SPI0_SCK/TPM0_CH1</td><td>LEDRGB_BLUE/J2_12</td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_seb5</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr>
				<td>75</td><td>PTD2/SPI0_MOSI/UART2_RX/TPM0_CH2/SPI0_MISO</td><td>J2_8</td>
				<td bgcolor='#5FE356'>UART2</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>alt3</td><td bgcolor='#5FE356'>Input</td>
			</tr>
			<tr>
				<td>76</td><td>PTD3/SPI0_MISO/UART2_TX/TPM0_CH3/SPI0_MOSI</td><td>J2_10</td>
				<td bgcolor='#5FE356'>UART2</td><td bgcolor='#5FE356'>uart_tx</td><td bgcolor='#5FE356'>alt3</td><td bgcolor='#5FE356'>Output</td>
			</tr>
			<tr>
				<td>77</td><td>PTD4/LLWU_P14/SPI1_PCS0/UART2_RX/TPM0_CH4</td><td>J1_6</td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>78</td><td>ADC0_SE6b/PTD5/SPI1_SCK/UART2_TX/TPM0_CH5</td><td>J2_4</td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_seb6</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr>
				<td>79</td><td>ADC0_SE7b/PTD6/LLWU_P15/SPI1_MOSI/UART0_RX/SPI1_MISO</td><td>J2_17</td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_seb7</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr>
				<td>80</td><td>PTD7/SPI1_MISO/UART0_TX/SPI1_MOSI</td><td>J2_19</td>
				<td></td><td></td><td></td><td></td>
			</tr>
		</table>

		<h2 style='font-family: Arial;'>Routable Pins</h2>
		<table cellpadding='2' border='1' style='border: 2px solid #000000;' bgcolor='WHITE' width='100%' align='center'>
			<tr><td colspan='3'></td><th colspan='3' align='center' bgcolor='#D0D0D0'>alt0</th><th colspan='3' align='center' bgcolor='#D0D0D0'>alt1</th><th colspan='3' align='center' bgcolor='#D0D0D0'>alt2</th><th colspan='3' align='center' bgcolor='#D0D0D0'>alt3</th><th colspan='3' align='center' bgcolor='#D0D0D0'>alt4</th><th colspan='3' align='center' bgcolor='#D0D0D0'>alt5</th><th colspan='3' align='center' bgcolor='#D0D0D0'>alt6</th><th colspan='3' align='center' bgcolor='#D0D0D0'>alt7</th></tr>
			<tr>
				<th bgcolor='#E8E8E8'>Package Pin #</th><th bgcolor='#E8E8E8'>Pin Name</th><th bgcolor='#E8E8E8'>User Assigned Signal Name</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
			</tr>
			<tr>
				<td>1</td><td>PTE0/UART1_TX/RTC_CLKOUT/CMP0_OUT/I2C1_SDA</td><td>J2_18</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port0</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#5FE356'>UART1</td><td bgcolor='#5FE356'>uart_tx</td><td bgcolor='#5FE356'>Output</td>
				<td bgcolor='#B3EAFF'>RTC</td><td bgcolor='#B3EAFF'>rtc_clkout</td><td bgcolor='#B3EAFF'>Output</td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>cmp_out</td><td bgcolor='#EFF174'>Output</td>
				<td bgcolor='#AFFF8E'>I2C1</td><td bgcolor='#AFFF8E'>i2c_sda</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>2</td><td>PTE1/SPI1_MOSI/UART1_RX/SPI1_MISO/I2C1_SCL</td><td>J2_20</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port1</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_mosi</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#5FE356'>UART1</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
				<td></td><td></td><td></td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_miso</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C1</td><td bgcolor='#AFFF8E'>i2c_sclk</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>3</td><td>PTE2/SPI1_SCK</td><td>J9_9</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port2</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_sck</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>4</td><td>PTE3/SPI1_MISO/SPI1_MOSI</td><td>J9_11</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port3</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_miso</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_mosi</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>5</td><td>PTE4/SPI1_PCS0</td><td>J9_13</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port4</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_cs0<br/>spi_ss</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>6</td><td>PTE5</td><td>J9_15</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port5</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>7</td><td>VDD8</td><td><small><i>same</i></small></td>
				<td bgcolor='#F7DCFF'>SUPPLY</td><td bgcolor='#F7DCFF'>pwr_vdd0</td><td bgcolor='#F7DCFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>8</td><td>VSS9</td><td><small><i>same</i></small></td>
				<td bgcolor='#F7DCFF'>SUPPLY</td><td bgcolor='#F7DCFF'>pwr_vss0</td><td bgcolor='#F7DCFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>9</td><td>USB0_DP</td><td><small><i>same</i></small></td>
				<td bgcolor='#00CA3A'>USB0</td><td bgcolor='#00CA3A'>usb_dp</td><td bgcolor='#00CA3A'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>10</td><td>USB0_DM</td><td><small><i>same</i></small></td>
				<td bgcolor='#00CA3A'>USB0</td><td bgcolor='#00CA3A'>usb_dm</td><td bgcolor='#00CA3A'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>11</td><td>VOUT33</td><td><small><i>same</i></small></td>
				<td bgcolor='#00CA3A'>USB0</td><td bgcolor='#00CA3A'>usb_vout</td><td bgcolor='#00CA3A'>Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>12</td><td>VREGIN</td><td><small><i>same</i></small></td>
				<td bgcolor='#00CA3A'>USB0</td><td bgcolor='#00CA3A'>usb_vrin</td><td bgcolor='#00CA3A'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>13</td><td>ADC0_DP0/ADC0_SE0/PTE20/TPM1_CH0/UART0_TX</td><td>J10_1</td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_dp0<br/>adc_se0</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port20</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM1</td><td bgcolor='#86DAFF'>tmr_ch0</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td bgcolor='#20E04E'>UART0</td><td bgcolor='#20E04E'>uart_tx</td><td bgcolor='#20E04E'>Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>14</td><td>ADC0_DM0/ADC0_SE4a/PTE21/TPM1_CH1/UART0_RX</td><td>J10_3</td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_dm0<br/>adc_sea4</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port21</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM1</td><td bgcolor='#86DAFF'>tmr_ch1</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td bgcolor='#20E04E'>UART0</td><td bgcolor='#20E04E'>uart_rx</td><td bgcolor='#20E04E'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>15</td><td>ADC0_DP3/ADC0_SE3/PTE22/TPM2_CH0/UART2_TX</td><td>J10_5</td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_dp3<br/>adc_se3</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port22</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM2</td><td bgcolor='#86DAFF'>tmr_ch0</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td bgcolor='#5FE356'>UART2</td><td bgcolor='#5FE356'>uart_tx</td><td bgcolor='#5FE356'>Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>16</td><td>ADC0_DM3/ADC0_SE7a/PTE23/TPM2_CH1/UART2_RX</td><td>J10_7</td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_dm3<br/>adc_sea7</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port23</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM2</td><td bgcolor='#86DAFF'>tmr_ch1</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td bgcolor='#5FE356'>UART2</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>17</td><td>VDDA</td><td><small><i>same</i></small></td>
				<td bgcolor='#FFFFFF'>ADC0<br/>ADC0<br/>ADC0<br/>ADC0<br/>SUPPLY</td><td bgcolor='#FFFFFF'>adc_vrefh<br/>adc_se29<br/>adc_dp29<br/>adc_vref_vdda<br/>pwr_vdda0</td><td bgcolor='#FFFFFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>18</td><td>VREFH</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_vrefh<br/>adc_se29<br/>adc_dp29<br/>adc_vref_vrefh</td><td bgcolor='#F8FF9A'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>19</td><td>VREFL</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_vrefl<br/>adc_se30<br/>adc_dm29<br/>adc_vref_vrefl</td><td bgcolor='#F8FF9A'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>20</td><td>VSSA</td><td><small><i>same</i></small></td>
				<td bgcolor='#FFFFFF'>ADC0<br/>ADC0<br/>ADC0<br/>ADC0<br/>SUPPLY</td><td bgcolor='#FFFFFF'>adc_vrefl<br/>adc_se30<br/>adc_dm29<br/>adc_vref_vssa<br/>pwr_vssa0</td><td bgcolor='#FFFFFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>21</td><td>CMP0_IN5/ADC0_SE4b/PTE29/TPM0_CH2/TPM_CLKIN0</td><td>J10_9</td>
				<td bgcolor='#FFFFFF'>CMP0<br/>CMP0<br/>CMP0<br/>ADC0</td><td bgcolor='#FFFFFF'>cmp_in5<br/>cmp_neg5<br/>cmp_pos5<br/>adc_seb4</td><td bgcolor='#FFFFFF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port29</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch2</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td bgcolor='#86DAFF'>TPM0<br/>TPM1<br/>TPM2</td><td bgcolor='#86DAFF'>tmr_clk</td><td bgcolor='#86DAFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>22</td><td>DAC0_OUT/ADC0_SE23/CMP0_IN4/PTE30/TPM0_CH3/TPM_CLKIN1</td><td>J10_11</td>
				<td bgcolor='#FFFFFF'>DAC0<br/>ADC0<br/>CMP0<br/>CMP0<br/>CMP0</td><td bgcolor='#FFFFFF'>dac_out<br/>adc_se23<br/>cmp_in4<br/>cmp_neg4<br/>cmp_pos4</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port30</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch3</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td bgcolor='#86DAFF'>TPM0<br/>TPM1<br/>TPM2</td><td bgcolor='#86DAFF'>tmr_clk</td><td bgcolor='#86DAFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>23</td><td>PTE31/TPM0_CH4</td><td>J2_13</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port31</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch4</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>24</td><td>PTE24/TPM0_CH0/I2C0_SCL</td><td>ACCEL_SCL</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port24</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch0</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sclk</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>25</td><td>PTE25/TPM0_CH1/I2C0_SDA</td><td>ACCEL_SDA</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port25</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch1</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sda</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>26</td><td>TSI0_CH1/PTA0/TPM0_CH5/SWD_CLK</td><td>SWD_CLK/J11_1</td>
				<td bgcolor='#E5C3FF'>TSI0</td><td bgcolor='#E5C3FF'>tsi_ch1</td><td bgcolor='#E5C3FF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port0</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch5</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#EBD4BD'>SWD</td><td bgcolor='#EBD4BD'>swd_clk</td><td bgcolor='#EBD4BD'>Input/Output</td>
			</tr>
			<tr>
				<td>27</td><td>TSI0_CH2/PTA1/UART0_RX/TPM2_CH0</td><td>DBG_CONSOLE_RX/J1_2</td>
				<td bgcolor='#E5C3FF'>TSI0</td><td bgcolor='#E5C3FF'>tsi_ch2</td><td bgcolor='#E5C3FF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port1</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#20E04E'>UART0</td><td bgcolor='#20E04E'>uart_rx</td><td bgcolor='#20E04E'>Input</td>
				<td bgcolor='#86DAFF'>TPM2</td><td bgcolor='#86DAFF'>tmr_ch0</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>28</td><td>TSI0_CH3/PTA2/UART0_TX/TPM2_CH1</td><td>DBG_CONSOLE_TX/J1_4</td>
				<td bgcolor='#E5C3FF'>TSI0</td><td bgcolor='#E5C3FF'>tsi_ch3</td><td bgcolor='#E5C3FF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port2</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#20E04E'>UART0</td><td bgcolor='#20E04E'>uart_tx</td><td bgcolor='#20E04E'>Output</td>
				<td bgcolor='#86DAFF'>TPM2</td><td bgcolor='#86DAFF'>tmr_ch1</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>29</td><td>TSI0_CH4/PTA3/I2C1_SCL/TPM0_CH0/SWD_DIO</td><td>SWD_DIO</td>
				<td bgcolor='#E5C3FF'>TSI0</td><td bgcolor='#E5C3FF'>tsi_ch4</td><td bgcolor='#E5C3FF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port3</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C1</td><td bgcolor='#AFFF8E'>i2c_sclk</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch0</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#EBD4BD'>SWD</td><td bgcolor='#EBD4BD'>swd_dio</td><td bgcolor='#EBD4BD'>Input/Output</td>
			</tr>
			<tr>
				<td>30</td><td>TSI0_CH5/PTA4/I2C1_SDA/TPM0_CH1/NMI_b</td><td>J1_10</td>
				<td bgcolor='#E5C3FF'>TSI0</td><td bgcolor='#E5C3FF'>tsi_ch5</td><td bgcolor='#E5C3FF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port4</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C1</td><td bgcolor='#AFFF8E'>i2c_sda</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch1</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>SystemControl<br/>non-peripheral</td><td bgcolor='#FFFFFF'>scb_nmi<br/>NMI</td><td bgcolor='#FFFFFF'>Input</td>
			</tr>
			<tr>
				<td>31</td><td>PTA5/USB_CLKIN/TPM0_CH2</td><td>J1_12</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port5</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#00CA3A'>USB0</td><td bgcolor='#00CA3A'>usb_clkin</td><td bgcolor='#00CA3A'>Input</td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch2</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>32</td><td>PTA12/TPM1_CH0</td><td>J1_8</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port12</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM1</td><td bgcolor='#86DAFF'>tmr_ch0</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>33</td><td>PTA13/TPM1_CH1</td><td>J2_2</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port13</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM1</td><td bgcolor='#86DAFF'>tmr_ch1</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>34</td><td>PTA14/SPI0_PCS0/UART0_TX</td><td>ACCEL_INT1</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port14</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_cs0<br/>spi_ss</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#20E04E'>UART0</td><td bgcolor='#20E04E'>uart_tx</td><td bgcolor='#20E04E'>Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>35</td><td>PTA15/SPI0_SCK/UART0_RX</td><td>ACCEL_INT2</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port15</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_sck</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#20E04E'>UART0</td><td bgcolor='#20E04E'>uart_rx</td><td bgcolor='#20E04E'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>36</td><td>PTA16/SPI0_MOSI/SPI0_MISO</td><td>J2_9</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port16</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_mosi</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_miso</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>37</td><td>PTA17/SPI0_MISO/SPI0_MOSI</td><td>J2_11</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port17</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_miso</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_mosi</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>38</td><td>VDD48</td><td><small><i>same</i></small></td>
				<td bgcolor='#F7DCFF'>SUPPLY</td><td bgcolor='#F7DCFF'>pwr_vdd1</td><td bgcolor='#F7DCFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>39</td><td>VSS49</td><td><small><i>same</i></small></td>
				<td bgcolor='#F7DCFF'>SUPPLY</td><td bgcolor='#F7DCFF'>pwr_vss1</td><td bgcolor='#F7DCFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>40</td><td>EXTAL0/PTA18/UART1_RX/TPM_CLKIN0</td><td>EXTAL</td>
				<td bgcolor='#DDC7B5'>OSC0</td><td bgcolor='#DDC7B5'>extal</td><td bgcolor='#DDC7B5'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port18</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#5FE356'>UART1</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
				<td bgcolor='#86DAFF'>TPM0<br/>TPM1<br/>TPM2</td><td bgcolor='#86DAFF'>tmr_clk</td><td bgcolor='#86DAFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>41</td><td>XTAL0/PTA19/UART1_TX/TPM_CLKIN1/LPTMR0_ALT1</td><td>XTAL</td>
				<td bgcolor='#DDC7B5'>OSC0</td><td bgcolor='#DDC7B5'>xtal</td><td bgcolor='#DDC7B5'>Output</td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port19</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#5FE356'>UART1</td><td bgcolor='#5FE356'>uart_tx</td><td bgcolor='#5FE356'>Output</td>
				<td bgcolor='#86DAFF'>TPM0<br/>TPM1<br/>TPM2</td><td bgcolor='#86DAFF'>tmr_clk</td><td bgcolor='#86DAFF'>Input</td>
				<td></td><td></td><td></td>
				<td bgcolor='#CEFFFF'>LPTMR0</td><td bgcolor='#CEFFFF'>tmr_clk1</td><td bgcolor='#CEFFFF'>Input</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>42</td><td>PTA20/RESET_b</td><td>RESET</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port20</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#CCB6A0'>RCM</td><td bgcolor='#CCB6A0'>reset</td><td bgcolor='#CCB6A0'>Input</td>
			</tr>
			<tr>
				<td>43</td><td>ADC0_SE8/TSI0_CH0/PTB0/LLWU_P5/I2C0_SCL/TPM1_CH0</td><td>J10_2</td>
				<td bgcolor='#FFFFFF'>ADC0<br/>TSI0</td><td bgcolor='#FFFFFF'>adc_se8<br/>tsi_ch0</td><td bgcolor='#FFFFFF'>Input</td>
				<td bgcolor='#FFFFFF'>GPIOB<br/>LLWU</td><td bgcolor='#FFFFFF'>port0<br/>llwu_wakeup5</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sclk</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td bgcolor='#86DAFF'>TPM1</td><td bgcolor='#86DAFF'>tmr_ch0</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>44</td><td>ADC0_SE9/TSI0_CH6/PTB1/I2C0_SDA/TPM1_CH1</td><td>J10_4</td>
				<td bgcolor='#FFFFFF'>ADC0<br/>TSI0</td><td bgcolor='#FFFFFF'>adc_se9<br/>tsi_ch6</td><td bgcolor='#FFFFFF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port1</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sda</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td bgcolor='#86DAFF'>TPM1</td><td bgcolor='#86DAFF'>tmr_ch1</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>45</td><td>ADC0_SE12/TSI0_CH7/PTB2/I2C0_SCL/TPM2_CH0</td><td>J10_6</td>
				<td bgcolor='#FFFFFF'>ADC0<br/>TSI0</td><td bgcolor='#FFFFFF'>adc_se12<br/>tsi_ch7</td><td bgcolor='#FFFFFF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port2</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sclk</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td bgcolor='#86DAFF'>TPM2</td><td bgcolor='#86DAFF'>tmr_ch0</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>46</td><td>ADC0_SE13/TSI0_CH8/PTB3/I2C0_SDA/TPM2_CH1</td><td>J10_8</td>
				<td bgcolor='#FFFFFF'>ADC0<br/>TSI0</td><td bgcolor='#FFFFFF'>adc_se13<br/>tsi_ch8</td><td bgcolor='#FFFFFF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port3</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sda</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td bgcolor='#86DAFF'>TPM2</td><td bgcolor='#86DAFF'>tmr_ch1</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>47</td><td>PTB8/EXTRG_IN</td><td>J9_1</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port8</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>ADC0<br/>ADC0<br/>TPM0<br/>TPM1<br/>TPM2</td><td bgcolor='#FFFFFF'>adc_triggerA<br/>adc_triggerB<br/>tmr_trigger<br/>tmr_trigger<br/>tmr_trigger</td><td bgcolor='#FFFFFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>48</td><td>PTB9</td><td>J9_3</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port9</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>49</td><td>PTB10/SPI1_PCS0</td><td>J9_5</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port10</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_cs0<br/>spi_ss</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>50</td><td>PTB11/SPI1_SCK</td><td>J9_7</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port11</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_sck</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>51</td><td>TSI0_CH9/PTB16/SPI1_MOSI/UART0_RX/TPM_CLKIN0/SPI1_MISO</td><td>TOUCH_SLIDER_A</td>
				<td bgcolor='#E5C3FF'>TSI0</td><td bgcolor='#E5C3FF'>tsi_ch9</td><td bgcolor='#E5C3FF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port16</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_mosi</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#20E04E'>UART0</td><td bgcolor='#20E04E'>uart_rx</td><td bgcolor='#20E04E'>Input</td>
				<td bgcolor='#86DAFF'>TPM0<br/>TPM1<br/>TPM2</td><td bgcolor='#86DAFF'>tmr_clk</td><td bgcolor='#86DAFF'>Input</td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_miso</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>52</td><td>TSI0_CH10/PTB17/SPI1_MISO/UART0_TX/TPM_CLKIN1/SPI1_MOSI</td><td>TOUCH_SLIDER_B</td>
				<td bgcolor='#E5C3FF'>TSI0</td><td bgcolor='#E5C3FF'>tsi_ch10</td><td bgcolor='#E5C3FF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port17</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_miso</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#20E04E'>UART0</td><td bgcolor='#20E04E'>uart_tx</td><td bgcolor='#20E04E'>Output</td>
				<td bgcolor='#86DAFF'>TPM0<br/>TPM1<br/>TPM2</td><td bgcolor='#86DAFF'>tmr_clk</td><td bgcolor='#86DAFF'>Input</td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_mosi</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>53</td><td>TSI0_CH11/PTB18/TPM2_CH0</td><td>LEDRGB_RED</td>
				<td bgcolor='#E5C3FF'>TSI0</td><td bgcolor='#E5C3FF'>tsi_ch11</td><td bgcolor='#E5C3FF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port18</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM2</td><td bgcolor='#86DAFF'>tmr_ch0</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>54</td><td>TSI0_CH12/PTB19/TPM2_CH1</td><td>LEDRGB_GREEN</td>
				<td bgcolor='#E5C3FF'>TSI0</td><td bgcolor='#E5C3FF'>tsi_ch12</td><td bgcolor='#E5C3FF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port19</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM2</td><td bgcolor='#86DAFF'>tmr_ch1</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>55</td><td>ADC0_SE14/TSI0_CH13/PTC0/EXTRG_IN/CMP0_OUT</td><td>J1_3</td>
				<td bgcolor='#FFFFFF'>ADC0<br/>TSI0</td><td bgcolor='#FFFFFF'>adc_se14<br/>tsi_ch13</td><td bgcolor='#FFFFFF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port0</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>ADC0<br/>ADC0<br/>TPM0<br/>TPM1<br/>TPM2</td><td bgcolor='#FFFFFF'>adc_triggerA<br/>adc_triggerB<br/>tmr_trigger<br/>tmr_trigger<br/>tmr_trigger</td><td bgcolor='#FFFFFF'>Input</td>
				<td></td><td></td><td></td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>cmp_out</td><td bgcolor='#EFF174'>Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>56</td><td>ADC0_SE15/TSI0_CH14/PTC1/LLWU_P6/RTC_CLKIN/I2C1_SCL/TPM0_CH0</td><td>J10_12</td>
				<td bgcolor='#FFFFFF'>ADC0<br/>TSI0</td><td bgcolor='#FFFFFF'>adc_se15<br/>tsi_ch14</td><td bgcolor='#FFFFFF'>Input</td>
				<td bgcolor='#FFFFFF'>GPIOC<br/>LLWU<br/>RTC</td><td bgcolor='#FFFFFF'>port1<br/>llwu_wakeup6<br/>rtc_clkin</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C1</td><td bgcolor='#AFFF8E'>i2c_sclk</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch0</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>57</td><td>ADC0_SE11/TSI0_CH15/PTC2/I2C1_SDA/TPM0_CH1</td><td>J10_10</td>
				<td bgcolor='#FFFFFF'>ADC0<br/>TSI0</td><td bgcolor='#FFFFFF'>adc_se11<br/>tsi_ch15</td><td bgcolor='#FFFFFF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port2</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C1</td><td bgcolor='#AFFF8E'>i2c_sda</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch1</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>58</td><td>PTC3/LLWU_P7/UART1_RX/TPM0_CH2/CLKOUTa</td><td>J1_5</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>GPIOC<br/>LLWU</td><td bgcolor='#FFFFFF'>port3<br/>llwu_wakeup7</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#5FE356'>UART1</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch2</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td bgcolor='#FFE1C7'>SIM</td><td bgcolor='#FFE1C7'>clkout</td><td bgcolor='#FFE1C7'>Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>59</td><td>VSS74</td><td><small><i>same</i></small></td>
				<td bgcolor='#F7DCFF'>SUPPLY</td><td bgcolor='#F7DCFF'>pwr_vss2</td><td bgcolor='#F7DCFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>60</td><td>VDD75</td><td><small><i>same</i></small></td>
				<td bgcolor='#F7DCFF'>SUPPLY</td><td bgcolor='#F7DCFF'>pwr_vdd2</td><td bgcolor='#F7DCFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>61</td><td>PTC4/LLWU_P8/SPI0_PCS0/UART1_TX/TPM0_CH3</td><td>J1_7</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>GPIOC<br/>LLWU</td><td bgcolor='#FFFFFF'>port4<br/>llwu_wakeup8</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_cs0<br/>spi_ss</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#5FE356'>UART1</td><td bgcolor='#5FE356'>uart_tx</td><td bgcolor='#5FE356'>Output</td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch3</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>62</td><td>PTC5/LLWU_P9/SPI0_SCK/LPTMR0_ALT2/CMP0_OUT</td><td>J1_9</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>GPIOC<br/>LLWU</td><td bgcolor='#FFFFFF'>port5<br/>llwu_wakeup9</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_sck</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#CEFFFF'>LPTMR0</td><td bgcolor='#CEFFFF'>tmr_clk2</td><td bgcolor='#CEFFFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>cmp_out</td><td bgcolor='#EFF174'>Output</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>63</td><td>CMP0_IN0/PTC6/LLWU_P10/SPI0_MOSI/EXTRG_IN/SPI0_MISO</td><td>J1_11</td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>cmp_in0<br/>cmp_neg0<br/>cmp_pos0</td><td bgcolor='#EFF174'>Input</td>
				<td bgcolor='#FFFFFF'>GPIOC<br/>LLWU</td><td bgcolor='#FFFFFF'>port6<br/>llwu_wakeup10</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_mosi</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#FFFFFF'>ADC0<br/>ADC0<br/>TPM0<br/>TPM1<br/>TPM2</td><td bgcolor='#FFFFFF'>adc_triggerA<br/>adc_triggerB<br/>tmr_trigger<br/>tmr_trigger<br/>tmr_trigger</td><td bgcolor='#FFFFFF'>Input</td>
				<td></td><td></td><td></td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_miso</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>64</td><td>CMP0_IN1/PTC7/SPI0_MISO/SPI0_MOSI</td><td>J1_1</td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>cmp_in1<br/>cmp_neg1<br/>cmp_pos1</td><td bgcolor='#EFF174'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port7</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_miso</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_mosi</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>65</td><td>CMP0_IN2/PTC8/I2C0_SCL/TPM0_CH4</td><td>J1_14</td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>cmp_in2<br/>cmp_neg2<br/>cmp_pos2</td><td bgcolor='#EFF174'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port8</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sclk</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch4</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>66</td><td>CMP0_IN3/PTC9/I2C0_SDA/TPM0_CH5</td><td>J1_16</td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>cmp_in3<br/>cmp_neg3<br/>cmp_pos3</td><td bgcolor='#EFF174'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port9</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sda</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch5</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>67</td><td>PTC10/I2C1_SCL</td><td>J1_13</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port10</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C1</td><td bgcolor='#AFFF8E'>i2c_sclk</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>68</td><td>PTC11/I2C1_SDA</td><td>J1_15</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port11</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C1</td><td bgcolor='#AFFF8E'>i2c_sda</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>69</td><td>PTC12/TPM_CLKIN0</td><td>J2_1</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port12</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM0<br/>TPM1<br/>TPM2</td><td bgcolor='#86DAFF'>tmr_clk</td><td bgcolor='#86DAFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>70</td><td>PTC13/TPM_CLKIN1</td><td>J2_3</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port13</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM0<br/>TPM1<br/>TPM2</td><td bgcolor='#86DAFF'>tmr_clk</td><td bgcolor='#86DAFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>71</td><td>PTC16</td><td>J2_5</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port16</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>72</td><td>PTC17</td><td>J2_7</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port17</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>73</td><td>PTD0/SPI0_PCS0/TPM0_CH0</td><td>J2_6</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOD</td><td bgcolor='#F7DCFF'>port0</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_cs0<br/>spi_ss</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch0</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>74</td><td>ADC0_SE5b/PTD1/SPI0_SCK/TPM0_CH1</td><td>LEDRGB_BLUE/J2_12</td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_seb5</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOD</td><td bgcolor='#F7DCFF'>port1</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_sck</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch1</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>75</td><td>PTD2/SPI0_MOSI/UART2_RX/TPM0_CH2/SPI0_MISO</td><td>J2_8</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOD</td><td bgcolor='#F7DCFF'>port2</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_mosi</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#5FE356'>UART2</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch2</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_miso</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>76</td><td>PTD3/SPI0_MISO/UART2_TX/TPM0_CH3/SPI0_MOSI</td><td>J2_10</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOD</td><td bgcolor='#F7DCFF'>port3</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_miso</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#5FE356'>UART2</td><td bgcolor='#5FE356'>uart_tx</td><td bgcolor='#5FE356'>Output</td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch3</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_mosi</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>77</td><td>PTD4/LLWU_P14/SPI1_PCS0/UART2_RX/TPM0_CH4</td><td>J1_6</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>GPIOD<br/>LLWU</td><td bgcolor='#FFFFFF'>port4<br/>llwu_wakeup14</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_cs0<br/>spi_ss</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#5FE356'>UART2</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch4</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>78</td><td>ADC0_SE6b/PTD5/SPI1_SCK/UART2_TX/TPM0_CH5</td><td>J2_4</td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_seb6</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOD</td><td bgcolor='#F7DCFF'>port5</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_sck</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#5FE356'>UART2</td><td bgcolor='#5FE356'>uart_tx</td><td bgcolor='#5FE356'>Output</td>
				<td bgcolor='#86DAFF'>TPM0</td><td bgcolor='#86DAFF'>tmr_ch5</td><td bgcolor='#86DAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>79</td><td>ADC0_SE7b/PTD6/LLWU_P15/SPI1_MOSI/UART0_RX/SPI1_MISO</td><td>J2_17</td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_seb7</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#FFFFFF'>GPIOD<br/>LLWU</td><td bgcolor='#FFFFFF'>port6<br/>llwu_wakeup15</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_mosi</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#20E04E'>UART0</td><td bgcolor='#20E04E'>uart_rx</td><td bgcolor='#20E04E'>Input</td>
				<td></td><td></td><td></td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_miso</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>80</td><td>PTD7/SPI1_MISO/UART0_TX/SPI1_MOSI</td><td>J2_19</td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOD</td><td bgcolor='#F7DCFF'>port7</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_miso</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#20E04E'>UART0</td><td bgcolor='#20E04E'>uart_tx</td><td bgcolor='#20E04E'>Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#90EE67'>SPI1</td><td bgcolor='#90EE67'>spi_mosi</td><td bgcolor='#90EE67'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
		</table>

*/
