VUT Brno®

# Permanent Magnet Synchronous Motor

Model of Permanent Magnet Synchronous Motor

## Library

Electromechanical Drives

## Description

Model of Permanent Magnet Synchronous Motor is in the five variants, created by

- Simulink blocks (PMSM Block)

- S-function Lvel-2 in language C as continous (PMSM C continous)

- S-function Lvel-2 in language C as discrete (PMSM C discrete)

- S-function Lvel-2 in language M as continous (PMSM M continous)

- S-function Lvel-2 in language M as discrete (PMSM M discrete)

## Data Type Support

The block of PMSM accepts only one dimension input signals and any numeric data type supported by Simulink software.

## Parameters and Dialog Box

Input parameters

  Enter the value of parameters or mark checkbox, if you want created new input insted of parameter.

Sample time (Only in discrete type of model)

  Enter the time interval between sample time hits. Model use Euler method.

Non zeros initial conditions

  After this button is clicked, new window is opened. Enter the value of initial state variables. Default values of initial conditions are set to zero.

Output paramters

  You may add another outputs to block.

## Table of model parameters

## Mathematical model

where
Model use Park and Clarke transformation.

## See Also

`AC Induction Motor`, `PMDCM`