# Adafruit NeoPixel Library [![Build Status](https://travis-ci.org/adafruit/Adafruit_NeoPixel.svg?branch=master)](https://travis-ci.org/adafruit/Adafruit_NeoPixel)

Arduino library for controlling single-wire-based LED pixels and strip such as the [Adafruit 60 LED/meter Digital LED strip][strip], the [Adafruit FLORA RGB Smart Pixel][flora], the [Adafruit Breadboard-friendly RGB Smart Pixel][pixel], the [Adafruit NeoPixel Stick][stick], and the [Adafruit NeoPixel Shield][shield].

After downloading, rename folder to 'Adafruit_NeoPixel' and install in Arduino Libraries folder. Restart Arduino IDE, then open File->Sketchbook->Library->Adafruit_NeoPixel->strandtest sketch.

Compatibility notes: Port A is not supported on any AVR processors at this time

[flora]:  http://adafruit.com/products/1060
[strip]:  http://adafruit.com/products/1138
[pixel]:  http://adafruit.com/products/1312
[stick]:  http://adafruit.com/products/1426
[shield]: http://adafruit.com/products/1430
