-> SCC_DAQ_a0.0
	GYRO init

-> SCC_DAQ_a0.1
	GYRO data check
	
-> SCC_DAQ_a0.6
	ACCEL init (no self tests)
	ACCEL data check

-> SCC_DAQ_a0.9
	ACCEL ID read OK
	
-> SCC_DAQ_a1.2
	>>> CS routines - not tested <<<

-> SCC_DAQ_a2.0
	SPI_1 - OK

-> SCC_DAQ_a3.0
	UART send review - BigEndian data transfer
	UART baudrate 115200Bd
	
-> SCC_DAQ_b0.0
	uart baudrate 3M6Bd
	scc module number added (into status word)

-> SCC_DAQ_b1.0
	BB_PWB embedded

-> SCC_DAQ_b2.0
	4 SCC OK 4MHz

-> SCC_DAQ_b3.0
	4 SCC OK 8MHz
	Timer 500Hz added
	New boot.bat -> no cygwin needed

-> SCC_DAQ_v0.0
	5Hz filter, calibration (dummy)
	Averaging

-> SCC_DAQ_v1.0
	On boot-up led
	Run time led blinker 10Hz