# example configuration for a dialup connection authenticated with PAP or CHAP
#
# This is the default configuration used by pon(1) and poff(1).
# See the manual page pppd(8) for information on all the options.

# MUST CHANGE: replace myusername@realm with the PPP login name given to
# your by your provider.
# There should be a matching entry with the password in /etc/ppp/pap-secrets
# and/or /etc/ppp/chap-secrets.
user "myusername@realm"

# MUST CHANGE: replace ******** with the phone number of your provider.
# The /etc/chatscripts/pap chat script may be modified to change the
# modem initialization string.
connect "/usr/sbin/chat -v -f /etc/chatscripts/pap -T *99***1#"

# Serial device to which the modem is connected.
/dev/ttyS4

# Speed of the serial line.
115200

# Assumes that your IP address is allocated dynamically by the ISP.
noipdefault
# Try to get the name server addresses from the ISP.
usepeerdns
replacedefaultroute
# Use this connection as the default route.
defaultroute
usepeerdns

debug
noauth
name wvdial
replacedefaultroute
noipdefault
nomagic
usepeerdns
ipcp-accept-local
ipcp-accept-remote
nomp
noccp
nopredictor1
novj
novjccomp
nobsdcomp

# Makes pppd "dial again" when the connection is lost.
persist
lock

# Do not ask the remote to authenticate.
noauth

