SparkFun TSL2561 Arduino Library
========================================
![TSL2561 Luminosity Sensor Breakout](https://dlnmh9ip6v2uc.cloudfront.net//images/products/1/2/0/5/5/12055-01.jpg)](https://www.sparkfun.com/products/12055)

[TSL2561 Luminosity Sensor Breakout (SEN-12055)](https://www.sparkfun.com/products/12055)

This is a Arduino Library for the AMS/TAOS TSL2561 Luminiosity sensor.
This illumination sensor has a flat response across most of the visible spectrum and has an adjustable integration time. 
It communicates via I2C and runs at 3.3V. 

Repository Contents
-------------------

* **/examples** - Example sketches for the library (.ino). Run these from the Arduino IDE. 
* **/src** - Source files for the library (.cpp, .h).
* **library.properties** - General library properties for the Arduino package manager. 

Documentation
--------------

* **[Installing an Arduino Library Guide](https://learn.sparkfun.com/tutorials/installing-an-arduino-library)** - Basic information on how to install an Arduino library.
* **[Product Repository](https://github.com/sparkfun/TSL2561_Luminosity_Sensor_BOB/)** - Main repository (including hardware files) for the TSL2561 Luminosity Sensor.
* **[Hookup Guide](https://learn.sparkfun.com/tutorials/tsl2561-luminosity-sensor-hookup-guide)** - Basic hookup guide for the TSL2561 Luminosity Sensor.

Products that use this Library 
---------------------------------

* [SEN-12055](Shttps://www.sparkfun.com/products/12055)- TSL2561 Luminosity Sensor.



License Information
-------------------

This product is _**open source**_! 

The **code** is beerware; if you see me (or any other SparkFun employee) at the local, and you've found our code helpful, please buy us a round!

Please use, reuse, and modify these files as you see fit. Please maintain attribution to SparkFun Electronics and release anything derivative under the same license.

Distributed as-is; no warranty is given.

- Your friends at SparkFun.
