Configuration	Code
STM32CubeMX 	4.21.0
Date	05/29/2017
MCU	STM32F103RBTx



PERIPHERALS	MODES	FUNCTIONS	PINS
ADC1	IN4	ADC1_IN4	PA4
ADC1	IN5	ADC1_IN5	PA5
ADC1	IN6	ADC1_IN6	PA6
ADC1	IN7	ADC1_IN7	PA7
ADC1	IN10	ADC1_IN10	PC0
ADC1	IN11	ADC1_IN11	PC1
I2C1	I2C	I2C1_SCL	PB6
I2C1	I2C	I2C1_SDA	PB7
SYS	Trace Asynchronous Sw	SYS_JTMS-SWDIO	PA13
SYS	Trace Asynchronous Sw	SYS_JTCK-SWCLK	PA14
SYS	Trace Asynchronous Sw	SYS_JTDO-TRACESWO	PB3
SYS	SysTick	SYS_VS_Systick	VP_SYS_VS_Systick
USART1	Asynchronous	USART1_RX	PA10
USART1	Asynchronous	USART1_TX	PA9



Pin Nb	PINs	FUNCTIONs	LABELs
8	PC0	ADC1_IN10	U1
9	PC1	ADC1_IN11	U2
11	PC3	GPIO_Input	S5
14	PA0-WKUP	GPIO_Input	S1
15	PA1	GPIO_Input	S2
16	PA2	GPIO_Input	S3
17	PA3	GPIO_Input	S4
20	PA4	ADC1_IN4	IC10-REF
21	PA5	ADC1_IN5	IC10-OUT
22	PA6	ADC1_IN6	IC9-REF
23	PA7	ADC1_IN7	IC9-OUT
25	PC5	GPIO_Output	LED4
26	PB0	GPIO_Output	LED3
27	PB1	GPIO_Output	LED2
28	PB2	GPIO_Output	LED1
39	PC8	GPIO_Output	H4
40	PC9	GPIO_Output	H3
42	PA9	USART1_TX	TX
43	PA10	USART1_RX	RX
46	PA13	SYS_JTMS-SWDIO	SWDIO
49	PA14	SYS_JTCK-SWCLK	SWCLK
55	PB3	SYS_JTDO-TRACESWO	SWO
58	PB6	I2C1_SCL	SCL
59	PB7	I2C1_SDA	SDA
61	PB8	GPIO_Output	H2
62	PB9	GPIO_Output	H1



SOFTWARE PROJECT

Project Settings : 
Project Name : Code
Project Folder : D:\VUT\6 semestr\Bakalářská práce\Přílohy\Program
Toolchain / IDE : MDK-ARM V5
Firmware Package Name and Version : STM32Cube FW_F1 V1.4.0


Code Generation Settings : 
STM32Cube Firmware Library Package : Copy all used libraries into the project folder
Generate peripheral initialization as a pair of '.c/.h' files per peripheral : No
Backup previously generated files when re-generating : No
Delete previously generated files when not re-generated : Yes
Set all free pins as analog (to optimize the power consumption) : No


Toolchains Settings : 
Compiler Optimizations : Balanced Size/Speed






