What: software part of system for monitoring patient head posture.
Purpose: post-operation monitoring of patients treated with retinal tears. The monitored parameter is head posture, specifically tilt difference from required position.




The program is in an executable called Helma.exe. It needs a number of DLL files with names stgarting "ft", precisely:

ftbusui.dll
ftcserco.dll
ftd2xx.dll
ftlang.dll
ftserui2.dll

Make sure these are in the same folder as Helma.exe!



To run the program, you should have a computer with Windows 2000 or newer. Hardware needs an USB port to be plugged into.

Before running program for first time, install drivers for FTDI USB converter, available at:
http://www.ftdichip.com/Drivers/D2XX.htm



When started for first time, interface elements are in random positions. Take a few minutes to position them as wanted. The whole layout is saved and will be restored next time the program is run.



The whole system consists of: this program, wireless communication interface, sensor. If the interface is not plugged into USB port, the program can serve only as a simple viewer of already saved files. A few of these are supplied with the project (*.DAT).



As an user, you will not need any of the .CPP, .H, .DFM, .LIB & .BPR files.



    Vladimír Slávik, Brno, 2010
