!
version 15.2
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
service compress-config
!
hostname A1
!
boot-start-marker
boot-end-marker
!
!
enable secret 9 $9$CUTwztKVVgBceX$djDMo9s6jVR2YUYuyweTeQ04qMn20rKOoflS4QDPpU2
!
username admin privilege 15 secret 9 $9$MXRHgz4lVMWvOX$LNkNuLzPmX8nQYU9Os2Vt5LsIhs7I5UnjK.LQCm.uw6
no aaa new-model
clock timezone AFT 4 30
!
!
!
!
!
!
!
!
no ip domain-lookup
ip domain-name ENCOR.23
ip cef
no ipv6 cef
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
!
!
!
!
!
!
!
interface Port-channel1
 switchport trunk encapsulation dot1q
 switchport mode trunk
!
interface Port-channel2
 switchport trunk encapsulation dot1q
 switchport mode trunk
!
interface Ethernet0/0
 switchport trunk encapsulation dot1q
 switchport mode trunk
 channel-group 1 mode active
!
interface Ethernet0/1
!
interface Ethernet0/2
 switchport trunk encapsulation dot1q
 switchport mode trunk
 channel-group 2 mode active
!
interface Ethernet0/3
!
interface Ethernet1/0
!
interface Ethernet1/1
 switchport trunk encapsulation dot1q
 switchport mode trunk
 channel-group 1 mode active
!
interface Ethernet1/2
 switchport trunk encapsulation dot1q
 switchport mode trunk
 channel-group 2 mode active
!
interface Ethernet1/3
!
interface Ethernet2/0
 switchport access vlan 13
 switchport mode access
 spanning-tree portfast
!
interface Ethernet2/1
!
interface Ethernet2/2
!
interface Ethernet2/3
!
interface Ethernet3/0
 switchport access vlan 8
 switchport mode access
 spanning-tree portfast
!
interface Ethernet3/1
!
interface Ethernet3/2
!
interface Ethernet3/3
!
interface Ethernet4/0
!
interface Ethernet4/1
!
interface Ethernet4/2
!
interface Ethernet4/3
!
interface Ethernet5/0
!
interface Ethernet5/1
!
interface Ethernet5/2
!
interface Ethernet5/3
!
interface Ethernet6/0
!
interface Ethernet6/1
!
interface Ethernet6/2
!
interface Ethernet6/3
!
interface Ethernet7/0
!
interface Ethernet7/1
!
interface Ethernet7/2
!
interface Ethernet7/3
!
interface Ethernet8/0
!
interface Ethernet8/1
!
interface Ethernet8/2
!
interface Ethernet8/3
!
interface Ethernet9/0
!
interface Ethernet9/1
!
interface Ethernet9/2
!
interface Ethernet9/3
!
interface Vlan3
 ip address 172.16.3.3 255.255.255.0
 shutdown
 ipv6 address FE80::A1:1 link-local
 ipv6 address 2001:DB8:ACAD:3::3/64
!
ip default-gateway 172.16.3.254
ip forward-protocol nd
!
no ip http server
no ip http secure-server
!
!
ip access-list standard VTY-CONTROL
 permit 172.16.0.0 0.0.255.255
 deny   any log
!
!
!
!
!
control-plane
!
banner motd ^C This is A1, Trouble Ticket 23.1.4.1 ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
 login local
line aux 0
line vty 0 4
 access-class VTY-CONTROL in
 exec-timeout 0 0
 login local
 transport input telnet
!
!
end

