!
version 15.2
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
service compress-config
!
hostname D1
!
boot-start-marker
boot-end-marker
!
!
enable secret 9 $9$49S/lh2iovIyVn$tloH6t/AfRiTduwfeeBP5ZYW29hxD5m89ECIAGp4ymM
!
username admin privilege 15 secret 9 $9$gfakAvWnzGvCOn$mEUnJKnipmHb.IEAHP587ZHH1UF9OT1T4aimxSTBu6g
no aaa new-model
clock timezone AFT 4 30
!
!
!
!
!
!
ip dhcp excluded-address 172.16.8.1 172.16.8.5
ip dhcp excluded-address 172.16.8.11 172.16.8.254
ip dhcp excluded-address 172.16.13.1 172.16.13.5
ip dhcp excluded-address 172.16.13.11 172.16.13.254
!
ip dhcp pool VLAN8DHCP
 network 172.16.8.0 255.255.255.0
 default-router 172.16.8.254
!
ip dhcp pool VLAN13DHCP
 network 172.16.13.0 255.255.255.0
 default-router 172.16.13.254
!
!
no ip domain-lookup
ip domain-name ENCOR.23
ip cef
ipv6 unicast-routing
ipv6 cef
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
track 14 ip sla 14
!
track 16 ip sla 16
!
!
!
!
!
!
!
!
!
!
!
!
!
interface Port-channel1
 switchport trunk encapsulation dot1q
 switchport mode trunk
!
interface Port-channel12
 switchport trunk encapsulation dot1q
 switchport mode trunk
!
interface Ethernet0/0
 switchport trunk encapsulation dot1q
 switchport mode trunk
 channel-group 1 mode active
!
interface Ethernet0/1
 no switchport
 ip address 172.16.0.2 255.255.255.0
 duplex auto
 ipv6 address FE80::D1:1 link-local
 ipv6 address 2001:DB8:ACAD::2/64
 ospfv3 1 ipv6 area 0
 ospfv3 1 ipv4 area 0
!
interface Ethernet0/2
 switchport access vlan 3
 switchport mode access
 spanning-tree portfast
!
interface Ethernet0/3
!
interface Ethernet1/0
 switchport trunk encapsulation dot1q
 switchport mode trunk
 channel-group 12 mode active
!
interface Ethernet1/1
 switchport trunk encapsulation dot1q
 switchport mode trunk
 channel-group 1 mode active
!
interface Ethernet1/2
!
interface Ethernet1/3
!
interface Ethernet2/0
 switchport trunk encapsulation dot1q
 switchport mode trunk
 channel-group 12 mode active
!
interface Ethernet2/1
!
interface Ethernet2/2
!
interface Ethernet2/3
!
interface Ethernet3/0
 switchport trunk encapsulation dot1q
 switchport mode trunk
 channel-group 12 mode active
!
interface Ethernet3/1
!
interface Ethernet3/2
!
interface Ethernet3/3
!
interface Ethernet4/0
 switchport trunk encapsulation dot1q
 switchport mode trunk
 channel-group 12 mode active
!
interface Ethernet4/1
!
interface Ethernet4/2
!
interface Ethernet4/3
!
interface Ethernet5/0
!
interface Ethernet5/1
!
interface Ethernet5/2
!
interface Ethernet5/3
!
interface Ethernet6/0
!
interface Ethernet6/1
!
interface Ethernet6/2
!
interface Ethernet6/3
!
interface Ethernet7/0
!
interface Ethernet7/1
!
interface Ethernet7/2
!
interface Ethernet7/3
!
interface Vlan3
 ip address 172.16.3.1 255.255.255.0
 standby version 2
 standby 34 ip 172.16.3.254
 standby 34 priority 110
 standby 34 preempt
 standby 34 track 14 decrement 20
 standby 36 ipv6 autoconfig
 standby 36 priority 110
 standby 36 preempt
 standby 36 track 16 decrement 20
 ipv6 address FE80::D1:2 link-local
 ipv6 address 2001:DB8:ACAD:3::1/64
 ospfv3 1 ipv6 area 0
 ospfv3 1 ipv4 area 0
!
interface Vlan8
 ip address 172.16.8.1 255.255.255.0
 standby version 2
 standby 84 ip 172.16.8.254
 standby 84 preempt
 standby 84 track 14 decrement 20
 standby 86 ipv6 autoconfig
 standby 86 preempt
 standby 86 track 16 decrement 20
 ipv6 address FE80::D1:3 link-local
 ipv6 address 2001:DB8:ACAD:8::1/64
 ospfv3 1 ipv6 area 0
 ospfv3 1 ipv4 area 0
!
interface Vlan13
 no ip address
 standby 134 track 14 decrement 20
 standby 136 track 16 decrement 20
 shutdown
!
interface Vlan16
 ip address 172.16.13.1 255.255.255.0
 standby version 2
 standby 134 ip 172.16.13.254
 standby 134 priority 110
 standby 134 preempt
 standby 136 ipv6 autoconfig
 standby 136 priority 110
 standby 136 preempt
 ipv6 address 2001:DB8:ACAD:13::1/64
!
router ospfv3 1
 router-id 0.0.138.131
 !
 address-family ipv4 unicast
 exit-address-family
 !
 address-family ipv6 unicast
 exit-address-family
!
ip forward-protocol nd
!
no ip http server
no ip http secure-server
!
!
ip access-list standard VTY-CONTROL
 permit 172.16.0.0 0.0.255.255
 deny   any log
!
!
ip sla 14
 icmp-echo 209.165.200.2
 frequency 10
ip sla schedule 14 life forever start-time now
ip sla 16
 icmp-echo 2001:DB8:200::2
 frequency 10
ip sla schedule 16 life forever start-time now
!
!
!
control-plane
!
banner motd ^C This is D1, Trouble Ticket 23.1.4.3 ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
 login local
line aux 0
line vty 0 4
 access-class VTY-CONTROL in
 exec-timeout 0 0
 login local
 transport input telnet
!
!
end
