!
version 15.6
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
!
hostname D2
!
boot-start-marker
boot-end-marker
!
!
!
no aaa new-model
!
!
!
clock timezone AFT 4 30
!
!
!
!
!
!
!
!
!
!
!


!
!
!
ip audit notify log
ip audit po max-events 100

no ip domain lookup
ip cef
no ipv6 cef
!
!
!
!
!
!
!
multilink bundle-name authenticated
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
interface Loopback16
 ip address 10.10.16.1 255.255.255.0
 ip ospf network point-to-point
!
interface Loopback17
 ip address 10.10.17.1 255.255.255.0
 ip ospf network point-to-point
!
interface Loopback18
 ip address 10.10.18.1 255.255.255.0
 ip ospf network point-to-point
!
interface Loopback19
 ip address 10.10.19.1 255.255.255.0
 ip ospf network point-to-point
!
interface Loopback20
 ip address 10.10.20.1 255.255.255.0
 ip ospf network point-to-point
!
interface Loopback21
 ip address 10.10.21.1 255.255.255.0
 ip ospf network point-to-point
!
interface Loopback22
 ip address 10.10.22.1 255.255.255.0
 ip ospf network point-to-point
!
interface Loopback23
 ip address 10.10.23.1 255.255.255.0
 ip ospf network point-to-point
!
interface Ethernet0/0
 ip address 10.10.5.1 255.255.255.0
 duplex auto
!
interface Ethernet0/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/3
 ip address 10.10.4.2 255.255.255.252
 duplex auto
!
interface Ethernet1/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet1/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet1/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet1/3
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/3
 no ip address
 shutdown
 duplex auto
!
interface Ethernet3/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet3/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet3/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet3/3
 no ip address
 shutdown
 duplex auto
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
!
!
!
control-plane
!
banner motd ^C This is D2, OSPFv2 Route Summarization and Filtering Lab ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 login
!
end
