!
version 15.6
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
!
hostname D2
!
boot-start-marker
boot-end-marker
!
!
!
no aaa new-model
!
!
!
clock timezone AFT 4 30
!
!
!
!
!
!
!
!
!
!
!


!
!
!
ip audit notify log
ip audit po max-events 100

no ip domain lookup
ip cef
no ipv6 cef
!
!
!
!
!
!
!
multilink bundle-name authenticated
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
interface Ethernet0/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/3
 ip address 10.0.3.2 255.255.255.0
!
interface Ethernet1/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet1/1
 ip address 10.1.1.2 255.255.255.0
 duplex auto
!
interface Ethernet1/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet1/3
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/3
 no ip address
 shutdown
 duplex auto
!
interface Ethernet3/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet3/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet3/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet3/3
 ip address 10.0.2.2 255.255.255.0
 duplex auto
!
interface Ethernet4/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet4/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet4/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet4/3
 no ip address
 shutdown
 duplex auto
!
interface Ethernet5/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet5/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet5/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet5/3
 no ip address
 shutdown
 duplex auto
!
interface Ethernet6/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet6/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet6/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet6/3
 no ip address
 shutdown
 duplex auto
!
interface Ethernet7/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet7/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet7/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet7/3
 no ip address
 shutdown
 duplex auto
!
interface Ethernet8/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet8/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet8/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet8/3
 no ip address
 shutdown
 duplex auto
!
interface Ethernet9/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet9/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet9/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet9/3
 no ip address
 shutdown
 duplex auto
!
router ospf 1
 router-id 5.5.5.5
 network 10.0.2.0 0.0.0.255 area 0
 network 10.0.3.0 0.0.0.255 area 0
 network 10.1.1.0 0.0.0.255 area 1
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
!
!
!
control-plane
!
banner motd ^C This is D2, Trouble Ticket 8.1.2.3 ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 login
!
end

