!
version 15.4
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname R3
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$pBpD$2IDjiF.RHUQvdVxg3dpfu0
!
no aaa new-model
!
!
!
bsd-client server url https://cloudsso.cisco.com/as/token.oauth2
clock timezone AFT 4 30
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
!
!
!
!
!


!
ip dhcp excluded-address 10.0.16.1 10.0.16.5
ip dhcp excluded-address 10.0.27.1 10.0.27.5
!
ip dhcp pool NAT16
 network 10.0.16.0 255.255.255.0
 default-router 10.0.16.1
!
ip dhcp pool NAT27
 network 10.0.27.0 255.255.255.0
 default-router 10.0.27.1
!
!
!
no ip domain lookup
ip cef
no ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
!
!
cts logging verbose
!
!
username admin privilege 15 secret 9 $9$3IXqN0mX3y5obH$tD8VO7IBt67caD8BoljEKPfydp3AGemiwqUZ2eTTe3g
!
redundancy
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
interface Loopback0
 ip address 209.165.227.1 255.255.255.255
!
interface Loopback1
 ip address 209.165.228.1 255.255.255.255
!
interface Ethernet0/0
 no ip address
 shutdown
!
interface Ethernet0/1
 no ip address
 shutdown
!
interface Ethernet0/2
 no ip address
 shutdown
!
interface Ethernet0/3
 no ip address
 shutdown
!
interface Ethernet1/0
 no ip address
 shutdown
!
interface Ethernet1/1
 no ip address
 shutdown
!
interface Ethernet1/2
 no ip address
 shutdown
!
interface Ethernet1/3
 no ip address
 shutdown
!
interface Ethernet2/0
 no ip address
 shutdown
!
interface Ethernet2/1
 no ip address
 shutdown
!
interface Ethernet2/2
 no ip address
 shutdown
!
interface Ethernet2/3
 no ip address
 shutdown
!
interface Ethernet3/0
 no ip address
 shutdown
!
interface Ethernet3/1
 no ip address
 shutdown
!
interface Ethernet3/2
 no ip address
!
interface Ethernet3/2.16
 encapsulation dot1Q 16
 ip address 10.0.16.1 255.255.255.0
 ip nat inside
 ip virtual-reassembly in
!
interface Ethernet3/2.27
 encapsulation dot1Q 27
 ip address 10.0.27.1 255.255.255.0
 ip nat inside
 ip virtual-reassembly in
!
interface Ethernet3/3
 no ip address
 shutdown
!
interface Serial4/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial4/1
 ip address 209.165.201.2 255.255.255.0
 ip access-group BOGON-MARTIAN in
 ip nat outside
 ip virtual-reassembly in
 serial restart-delay 0
!
interface Serial4/2
 ip address 209.165.200.2 255.255.255.0
 ip access-group BOGON-MARTIAN in
 ip nat outside
 ip virtual-reassembly in
 serial restart-delay 0
!
interface Serial4/3
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial5/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial5/1
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial5/2
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial5/3
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial6/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial6/1
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial6/2
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial6/3
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial7/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial7/1
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial7/2
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial7/3
 no ip address
 shutdown
 serial restart-delay 0
!
router bgp 39457
 bgp router-id 209.165.227.1
 bgp log-neighbor-changes
 network 209.165.228.1 mask 255.255.255.255
 neighbor 209.165.226.1 remote-as 181035
 neighbor 209.165.226.1 ebgp-multihop 3
 neighbor 209.165.226.1 update-source Loopback0
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
ip nat inside source list NAT-ELIGIBLE interface Loopback1 overload
ip route 209.165.226.1 255.255.255.255 Serial4/2
ip route 209.165.226.1 255.255.255.255 Serial4/1
!
ip access-list standard BOGON-MARTIAN
 deny   209.165.228.1
 deny   209.165.227.1
 deny   10.0.0.0 0.255.255.255
 deny   172.0.0.0 0.31.255.255
 deny   192.168.0.0 0.0.255.255
 deny   127.0.0.0 0.255.255.255
 permit any
ip access-list standard NAT-ELIGIBLE
 permit 10.0.0.0 0.255.255.255
 deny   any log
!
!
!
!
control-plane
!
!
!
!
!
!
!
banner motd ^C This is R3, Trouble Ticket 21.1.2.3 ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 exec-timeout 5 0
 login local
 transport input telnet
!
!
end

