!
version 15.6
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
!
hostname D1
!
boot-start-marker
boot-end-marker
!
!
!
no aaa new-model
!
!
!
clock timezone AFT 4 30
!
!
!
!
!
!
!
!
!
!
!


!
!
!
ip audit notify log
ip audit po max-events 100

no ip domain lookup
ip cef
ipv6 unicast-routing
ipv6 cef
!
!
!
!
!
!
!
multilink bundle-name authenticated
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
interface Ethernet0/0
 switchport
 switchport access vlan 11
 switchport mode access
 duplex auto
!
interface Ethernet0/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/3
 no ip address
 shutdown
 duplex auto
!
interface Ethernet1/0
 ip address 10.1.2.2 255.255.255.0
 duplex auto
 ipv6 address FE80::D1:1 link-local
 ipv6 address 2001:DB8:ACAD:1012::2/64
!
interface Ethernet1/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet1/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet1/3
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/3
 no ip address
 shutdown
 duplex auto
!
interface Vlan11
 ip address 192.168.2.1 255.255.255.0
 ipv6 address FE80::D1:2 link-local
 ipv6 address 2001:DB8:ACAD:2000::1/64
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
ip route 0.0.0.0 0.0.0.0 Ethernet1/0 10.1.2.1
!
ipv6 route ::/0 Ethernet1/0 2001:DB8:ACAD:1012::1
!
!
!
control-plane
!
banner motd ^C D1, Implement VRF-Lite ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 exec-timeout 0 0
 privilege level 15
 password cisco123
 logging synchronous
 login
!
end
