!
version 15.4
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname R2
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$HpBK$cNW35AkYuDukPbfrnT1tt.
!
aaa new-model
!
!
aaa authentication login default local
aaa authorization exec default local
!
!
!
!
!
aaa session-id common
!
!
!
bsd-client server url https://cloudsso.cisco.com/as/token.oauth2
clock timezone EET 2 0
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
!
!
!
!
!


!
!
!
!
ip domain name ccnplab.local
ip cef
no ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
!
!
cts logging verbose
!
!
username admin privilege 15 secret 9 $9$.tKTtqfisOMR1X$Rj7CXX/lV6vk7qW5pTxAlnvMrsI9pXY4ILYd78NZOus
!
redundancy
!
!
ip ssh version 2
ip scp server enable
!
!
!
!
!
!
!
!
!
!
!
!
!
interface Loopback0
 ip address 2.2.2.2 255.255.255.255
!
interface Ethernet0/0
 no ip address
 shutdown
!
interface Ethernet0/1
 no ip address
 shutdown
!
interface Ethernet0/2
 no ip address
 shutdown
!
interface Ethernet0/3
 no ip address
 shutdown
!
interface Ethernet1/0
 no ip address
 shutdown
!
interface Ethernet1/1
 no ip address
 shutdown
!
interface Ethernet1/2
 no ip address
 shutdown
!
interface Ethernet1/3
 no ip address
 shutdown
!
interface Ethernet2/0
 no ip address
 shutdown
!
interface Ethernet2/1
 ip address 10.10.12.2 255.255.255.252
!
interface Ethernet2/2
 no ip address
 shutdown
!
interface Ethernet2/3
 no ip address
 shutdown
!
!
router eigrp 10
 network 10.10.12.0 0.0.0.3
 auto-summary
 eigrp router-id 10.10.12.2
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
logging trap debugging
logging source-interface Ethernet2/1
logging host 10.10.10.10
!
!
!
!
!
control-plane
!
!
!
!
!
!
!
banner motd ^C This is R2, Trouble Ticket 23.1.3.1 ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 transport input ssh
!
!
end
