!
version 15.6
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
!
hostname D2
!
boot-start-marker
boot-end-marker
!
!
!
no aaa new-model
!
!
!
clock timezone AFT 4 30
!
!
!
!
!
!
!
!
!
!
!


!
!
!
ip audit notify log
ip audit po max-events 100

no ip domain lookup
ip cef
ipv6 unicast-routing
ipv6 cef
!
!
!
!
!
!
!
multilink bundle-name authenticated
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
interface Loopback0
 ip address 198.51.100.1 255.255.255.128
 ipv6 address FE80::198:2 link-local
 ipv6 address 2001:DB8:198:51:100::1/80
!
interface Ethernet0/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/3
 ip address 10.1.32.2 255.255.255.0
 duplex auto
 ipv6 address FE80::32:2 link-local
 ipv6 address 2001:DB8:ACAD:32::2/64
!
!
router eigrp CISCO
 !
 address-family ipv4 unicast autonomous-system 64512
  !
  af-interface default
   shutdown
  exit-af-interface
  !
  af-interface Loopback0
   no shutdown
   passive-interface
  exit-af-interface
  !
  af-interface Ethernet0/3
   no shutdown
  exit-af-interface
  !
  topology base
  exit-af-topology
  network 10.1.32.0 0.0.0.255
  network 198.51.100.0 0.0.0.127
  eigrp router-id 22.22.22.22
 exit-address-family
 !
 address-family ipv6 unicast autonomous-system 64512
  !
  af-interface default
   shutdown
  exit-af-interface
  !
  af-interface Loopback0
   no shutdown
   passive-interface
  exit-af-interface
  !
  af-interface Ethernet0/3
   no shutdown
  exit-af-interface
  !
  topology base
  exit-af-topology
  eigrp router-id 22.22.22.22
 exit-address-family
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
!
!
!
control-plane
!
banner motd ^C D2, Configure Route Redistribution Between EIGRP and OSPF ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 login
!
end
