!
version 15.4
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$zHZQ$W5SCUAMXuMCYs4eMkhd8X/
!
no aaa new-model
!
!
!
bsd-client server url https://cloudsso.cisco.com/as/token.oauth2
clock timezone AFT 4 30
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
!
!
!
!
!


!
!
!
!
ip cef
ipv6 unicast-routing
ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
!
!
cts logging verbose
!
!
username admin privilege 15 secret 9 $9$EhABu1WPuIrzR1$UZux6eOUJ3DRZz45ZCrX8sSDimt7vRxdxeod4GldmNA
!
redundancy
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
interface Loopback0
 ip address 209.165.200.225 255.255.255.248
 ipv6 address FE80::1:3 link-local
 ipv6 address 2001:DB8:A:C::1/64
!
interface Ethernet0/0
 no ip address
 shutdown
!
interface Ethernet0/1
 no ip address
 shutdown
!
interface Ethernet0/2
 no ip address
 shutdown
!
interface Ethernet0/3
 no ip address
 shutdown
!
interface Ethernet1/0
 ip address 10.10.10.1 255.255.255.0
 ipv6 address FE80::1:2 link-local
 ipv6 address 2001:DB8:A:A::1/64
 ipv6 nd other-config-flag
 ipv6 dhcp relay destination  2001:DB8:A:B::2
!
interface Ethernet1/1
 no ip address
 shutdown
!
interface Ethernet1/2
 ip address 10.10.20.1 255.255.255.0
 ip helper-address 10.10.20.254
 ipv6 address FE80::1:1 link-local
 ipv6 address 2001:DB8:A:B::1/64
!
interface Ethernet1/3
 no ip address
 shutdown
!
interface Ethernet2/0
 no ip address
 shutdown
!
interface Ethernet2/1
 no ip address
 shutdown
!
interface Ethernet2/2
 no ip address
 shutdown
!
interface Ethernet2/3
 no ip address
 shutdown
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
ip route 0.0.0.0 0.0.0.0 Loopback0
!
ipv6 route ::/0 Loopback0
!
!
!
control-plane
!
!
!
!
!
!
!
banner motd ^C This is R1, Trouble Ticket 1.1.2.2 ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 login local
 transport input telnet
!
!
end

