!
version 15.4
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname R3
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$6vxg$AkSVp5.AmSvwtUXvyIB07/
!
no aaa new-model
!
!
!
bsd-client server url https://cloudsso.cisco.com/as/token.oauth2
clock timezone AFT 4 30
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
!
!
!
!
!


!
!
!
!
no ip domain lookup
ip cef
ipv6 unicast-routing
ipv6 cef
ipv6 dhcp pool LAN16
 address prefix 2001:DB8:ACAD:16::/64
!
ipv6 dhcp pool LAN27
 address prefix 2001:DB8:ACAD:27::/64
!
!
multilink bundle-name authenticated
!
!
!
!
!
!
!
cts logging verbose
!
!
username admin privilege 15 secret 9 $9$OBG5HWoA4HUhVH$1c6oCpPiENmOSxP5XlLRtcm5eJCS8tqy71pBrlQxA9k
!
redundancy
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
interface Loopback0
 no ip address
 ipv6 address FE80::3:5 link-local
 ipv6 address 2001:DB8:ACAD:227::1/64
!
interface Ethernet0/0
 no ip address
 shutdown
!
interface Ethernet0/1
 no ip address
 shutdown
!
interface Ethernet0/2
 no ip address
 shutdown
!
interface Ethernet0/3
 no ip address
 shutdown
!
interface Ethernet1/0
 no ip address
 shutdown
!
interface Ethernet1/1
 no ip address
 shutdown
!
interface Ethernet1/2
 no ip address
 shutdown
!
interface Ethernet1/3
 no ip address
 shutdown
!
interface Ethernet2/0
 no ip address
 shutdown
!
interface Ethernet2/1
 no ip address
 shutdown
!
interface Ethernet2/2
 no ip address
 shutdown
!
interface Ethernet2/3
 no ip address
 shutdown
!
interface Ethernet3/0
 no ip address
 shutdown
!
interface Ethernet3/1
 no ip address
 shutdown
!
interface Ethernet3/2
 no ip address
!
interface Ethernet3/2.1
!
interface Ethernet3/2.16
 encapsulation dot1Q 16
 ipv6 address FE80::3:1 link-local
 ipv6 address 2001:DB8:ACAD:16::1/64
 ipv6 nd managed-config-flag
 ipv6 dhcp server LAN16
!
interface Ethernet3/2.27
 encapsulation dot1Q 27
 ipv6 address FE80::3:2 link-local
 ipv6 address 2001:DB8:ACAD:27::1/64
 ipv6 nd managed-config-flag
 ipv6 dhcp server LAN27
!
interface Ethernet3/3
 no ip address
 shutdown
!
interface Serial4/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial4/1
 no ip address
 ipv6 address FE80::3:4 link-local
 ipv6 address 2001:DB8:ACAD:2001::2/64
 serial restart-delay 0
!
interface Serial4/2
 no ip address
 ipv6 address FE80::3:3 link-local
 ipv6 address 2001:DB8:ACAD:2000::2/64
 serial restart-delay 0
!
interface Serial4/3
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial5/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial5/1
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial5/2
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial5/3
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial6/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial6/1
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial6/2
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial6/3
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial7/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial7/1
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial7/2
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial7/3
 no ip address
 shutdown
 serial restart-delay 0
!
router bgp 41
 bgp router-id 3.3.3.3
 bgp log-neighbor-changes
 neighbor 2001:DB8:ACAD:226::1 remote-as 15
 neighbor 2001:DB8:ACAD:226::1 ebgp-multihop 3
 neighbor 2001:DB8:ACAD:226::1 update-source Loopback0
 !
 address-family ipv4
  no neighbor 2001:DB8:ACAD:226::1 activate
 exit-address-family
 !
 address-family ipv6
  network 2001:DB8:ACAD:16::/64
  network 2001:DB8:ACAD:27::/64
  neighbor 2001:DB8:ACAD:226::1 activate
 exit-address-family
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
ipv6 route 2001:DB8:ACAD:226::/64 Serial4/1 2001:DB8:ACAD:2001::1
ipv6 route 2001:DB8:ACAD:226::/64 Serial4/2 2001:DB8:ACAD:2000::1
!
!
!
control-plane
!
!
!
!
!
!
!
banner motd ^C This is R3, Trouble Ticket 21.1.3.1  ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 exec-timeout 5 0
 login local
 transport input telnet
!
!
end

