!
version 15.6
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
!
hostname D1
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$lywm$DF.Use7oNddWv8f8WuMcO.
!
no aaa new-model
!
!
!
clock timezone AFT 4 30
!
!
!
!
!
!
!
!
!
!
!


ip dhcp excluded-address 209.165.224.1 209.165.224.5
ip dhcp excluded-address 209.165.225.1 209.165.225.5
!
ip dhcp pool VLAN11
 network 209.165.224.0 255.255.255.0
 default-router 209.165.224.1
!
ip dhcp pool VLAN12
 network 209.165.225.0 255.255.255.0
 default-router 209.165.225.1
!
!
!
ip audit notify log
ip audit po max-events 100

no ip domain lookup
ip cef
no ipv6 cef
!
!
!
!
!
!
!
multilink bundle-name authenticated
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
username admin privilege 15 secret 9 $9$1x0R124E/rBWsH$/UG.BkC7B87xFuftaXuGP7hg3iexm/h7loGe4XUcExs
!
vlan internal allocation policy ascending
!
!
!
!
!
interface Ethernet0/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/3
 no ip address
 shutdown
 duplex auto
!
interface Ethernet1/0
 switchport
 switchport access vlan 11
 switchport mode access
 duplex auto
 spanning-tree portfast
!
interface Ethernet1/1
 ip address 192.0.0.2 255.255.255.0
!
interface Ethernet1/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet1/3
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/0
 switchport
 switchport access vlan 12
 switchport mode access
 duplex auto
 spanning-tree portfast
!
interface Ethernet2/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/3
 no ip address
 shutdown
 duplex auto
!
interface Vlan11
 ip address 209.165.224.1 255.255.255.0
!
interface Vlan12
 ip address 209.165.225.1 255.255.255.0
!
router ospf 1
 router-id 131.131.131.131
 passive-interface Vlan11
 passive-interface Vlan12
 network 192.0.0.0 0.0.0.255 area 0
 network 209.165.224.0 0.0.1.255 area 0
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
ip access-list extended VTY-CONTROL
 permit ip 209.165.224.0 0.0.0.255 any time-range REMOTE-CONTROL
 deny   ip any any log
!
!
!
!
control-plane
!
banner motd ^C This is D1, Trouble Ticket 21.1.2.2 ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 access-class VTY-CONTROL in
 exec-timeout 5 0
 login local
 transport input telnet
!
time-range REMOTE-CONTROL
 periodic weekdays 5:00 to 23:59
 periodic weekend 5:00 to 23:59
!
end

