!
version 15.4
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname R2
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$e4jT$FdkhSnOxQDIRjv/MZYeok.
!
no aaa new-model
!
!
!
bsd-client server url https://cloudsso.cisco.com/as/token.oauth2
clock timezone AFT 4 30
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
!
!
!
!
!


!
!
!
!
no ip domain lookup
ip cef
ipv6 unicast-routing
ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
!
!
cts logging verbose
!
!
username admin secret 9 $9$t/.leieuXmGZUX$mNCk89/j7LEJHUWu/CbMcaYw7BifP2780ZAKEjuGoM2
!
redundancy
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
interface Loopback0
 no ip address
 ipv6 address FE80::2:3 link-local
 ipv6 address 2001:DB8:ACAD:2000::1/64
 ipv6 eigrp 513
!
interface Loopback1
 no ip address
 ipv6 address FE80::2:4 link-local
 ipv6 address 2001:DB8:ACAD:2001::1/64
!
interface Ethernet0/0
 no ip address
 shutdown
!
interface Ethernet0/1
 no ip address
 shutdown
!
interface Ethernet0/2
 no ip address
 shutdown
!
interface Ethernet0/3
 no ip address
 shutdown
!
interface Ethernet1/0
 no ip address
 shutdown
!
interface Ethernet1/1
 no ip address
 shutdown
!
interface Ethernet1/2
 no ip address
 shutdown
!
interface Ethernet1/3
 no ip address
 shutdown
!
interface Ethernet2/0
 no ip address
 shutdown
!
interface Ethernet2/1
 no ip address
 ipv6 address FE80::2:1 link-local
 ipv6 address 2001:DB8:12::2/64
 ipv6 eigrp 513
 ipv6 summary-address eigrp 513 ::/0
!
interface Ethernet2/2
 no ip address
 shutdown
!
interface Ethernet2/3
 no ip address
 ipv6 address FE80::2:2 link-local
 ipv6 address 2001:DB8:23::2/64
 ipv6 eigrp 513
 ipv6 summary-address eigrp 513 ::/0
!
interface Ethernet3/0
 no ip address
 shutdown
!
interface Ethernet3/1
 no ip address
 shutdown
!
interface Ethernet3/2
 no ip address
 shutdown
!
interface Ethernet3/3
 no ip address
 shutdown
!
interface Serial4/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial4/1
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial4/2
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial4/3
 no ip address
 shutdown
 serial restart-delay 0
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
ipv6 router eigrp 513
 eigrp router-id 2.2.2.2
!
!
!
!
control-plane
!
!
!
!
!
!
!
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 login local
 transport input telnet
!
!
end
