!
version 15.4
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname R3
!
boot-start-marker
boot-end-marker
!
!
!
no aaa new-model
!
!
!
bsd-client server url https://cloudsso.cisco.com/as/token.oauth2
clock timezone AFT 4 30
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
!
!
!
!
!


!
!
!
!
no ip domain lookup
ip cef
ipv6 unicast-routing
ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
!
!
cts logging verbose
!
!
!
redundancy
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
interface Loopback0
 description Loopback for BGP peering
 ip address 192.168.99.3 255.255.255.255
 ipv6 address FE80::99:3 link-local
 ipv6 address 2001:DB8:C0C0:99::3/128
 ospfv3 1 ipv6 area 0
 ospfv3 1 ipv4 area 0
!
interface Loopback1
 ip address 192.168.6.1 255.255.255.0
 ipv6 address FE80::A031:1 link-local
 ipv6 address 2001:DB8:C0C0:A031::1/64
 ospfv3 1 ipv6 area 0
 ospfv3 1 ipv6 network point-to-point
 ospfv3 1 ipv4 area 0
 ospfv3 1 ipv4 network point-to-point
!
interface Ethernet0/0
 no ip address
 shutdown
!
interface Ethernet0/1
 no ip address
 shutdown
!
interface Ethernet0/2
 no ip address
 shutdown
!
interface Ethernet0/3
 no ip address
 shutdown
!
interface Ethernet1/0
 no ip address
 shutdown
!
interface Ethernet1/1
 no ip address
 shutdown
!
interface Ethernet1/2
 no ip address
 shutdown
!
interface Ethernet1/3
 no ip address
 shutdown
!
interface Ethernet2/0
 no ip address
 shutdown
!
interface Ethernet2/1
 no ip address
 shutdown
!
interface Ethernet2/2
 no ip address
 shutdown
!
interface Ethernet2/3
 no ip address
 shutdown
!
interface Ethernet3/0
 ip address 172.16.2.2 255.255.255.252
 ipv6 address FE80::F001:2 link-local
 ipv6 address 2001:DB8:B0B:F001::2/64
!
interface Ethernet3/1
 no ip address
 shutdown
!
interface Ethernet3/2
 ip address 192.168.5.1 255.255.255.0
 ipv6 address FE80::A002:1 link-local
 ipv6 address 2001:DB8:C0C0:A002::1/64
 ospfv3 1 ipv6 area 0
 ospfv3 1 ipv4 area 0
!
interface Ethernet3/3
 no ip address
 shutdown
!
router ospfv3 1
 !
 address-family ipv4 unicast
  router-id 3.3.3.3
 exit-address-family
 !
 address-family ipv6 unicast
  router-id 3.3.3.3
 exit-address-family
!
router bgp 65000
 bgp router-id 3.3.3.3
 bgp log-neighbor-changes
 neighbor 2001:DB8:B0B:F001::1 remote-as 65200
 neighbor 2001:DB8:C0C0:99::1 remote-as 65000
 neighbor 2001:DB8:C0C0:99::1 update-source Loopback0
 neighbor 2001:DB8:C0C0:99::2 remote-as 65000
 neighbor 2001:DB8:C0C0:99::2 update-source Loopback0
 neighbor 172.16.2.1 remote-as 65200
 neighbor 192.168.99.1 remote-as 65000
 neighbor 192.168.99.1 update-source Loopback0
 neighbor 192.168.99.2 remote-as 65000
 neighbor 192.168.99.2 update-source Loopback0
 !
 address-family ipv4
  network 192.168.6.0
  no neighbor 2001:DB8:B0B:F001::1 activate
  no neighbor 2001:DB8:C0C0:99::1 activate
  no neighbor 2001:DB8:C0C0:99::2 activate
  neighbor 172.16.2.1 activate
  neighbor 192.168.99.1 activate
  neighbor 192.168.99.1 next-hop-self
  neighbor 192.168.99.2 activate
  neighbor 192.168.99.2 next-hop-self
 exit-address-family
 !
 address-family ipv6
  network 2001:DB8:C0C0:A031::/64
  neighbor 2001:DB8:B0B:F001::1 activate
  neighbor 2001:DB8:B0B:F001::1 route-map AS65200-CAFE in
  neighbor 2001:DB8:C0C0:99::1 activate
  neighbor 2001:DB8:C0C0:99::1 next-hop-self
  neighbor 2001:DB8:C0C0:99::2 activate
  neighbor 2001:DB8:C0C0:99::2 next-hop-self
 exit-address-family
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
!
!
ipv6 prefix-list CAFE-POLICY seq 5 permit 2001:DB8:CAFE::/48
route-map AS65200-CAFE permit 10
 match ipv6 address prefix-list CAFE-POLICY
 set weight 400
!
route-map AS65200-CAFE permit 20
!
!
!
control-plane
!
!
!
!
!
!
!
banner motd ^C This is R3, Trouble Ticket 14.1.2.2 ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 login
 transport input none
!
!
end
