!
version 15.6
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
!
hostname D2
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$hTBn$1wgpIciSaNFXA1xRspaPz0
!
no aaa new-model
!
!
!
clock timezone AFT 4 30
!
!
!
!
!
!
!
!
!
!
!


ip dhcp excluded-address 10.0.16.1 10.0.16.5
ip dhcp excluded-address 10.0.27.1 10.0.27.5
!
ip dhcp pool VLAN16DHCP4
 network 10.0.16.0 255.255.255.0
 default-router 10.0.16.1
!
ip dhcp pool VLAN27DHCP4
 network 10.0.27.0 255.255.255.0
 default-router 10.0.27.1
!
!
!
ip audit notify log
ip audit po max-events 100

no ip domain lookup
ip cef
ipv6 unicast-routing
ipv6 dhcp pool VLAN16DHCP6
 address prefix 2001:DB8:ACAD:16::/64
!
ipv6 dhcp pool VLAN27DHCP6
 address prefix 2001:DB8:ACAD:27::/64
!
ipv6 cef
!
!
!
!
!
!
!
multilink bundle-name authenticated
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
username admin privilege 15 secret 9 $9$pS3WJNv7NlwFQc$f/TdVqiB1C1QIGJHy.hwTW37P5GHxWUVZwBiZ/v34CY
!
vlan internal allocation policy ascending
!
!
!
!
!
interface Ethernet0/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/3
 no ip address
 shutdown
 duplex auto
!
interface Ethernet1/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet1/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet1/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet1/3
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/3
 ip address 10.0.0.2 255.255.255.0
 ipv6 address FE80::D2:1 link-local
 ipv6 address 2001:DB8:ACAD:10::2/64
!
interface Ethernet3/0
 switchport
 switchport access vlan 16
 switchport mode access
 duplex auto
 spanning-tree portfast
!
interface Ethernet3/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet3/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet3/3
 no ip address
 shutdown
 duplex auto
!
interface Ethernet4/0
 switchport
 switchport access vlan 27
 switchport mode access
 duplex auto
 spanning-tree portfast
!
interface Ethernet4/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet4/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet4/3
 no ip address
 shutdown
 duplex auto
!
interface Vlan16
 ip address 10.0.16.1 255.255.255.0
 ipv6 address FE80::D2:2 link-local
 ipv6 address 2001:DB8:ACAD:16::1/64
 ipv6 nd managed-config-flag
 ipv6 dhcp server VLAN16DHCP6
!
interface Vlan27
 ip address 10.0.27.1 255.255.255.0
 ipv6 address FE80::D2:3 link-local
 ipv6 address 2001:DB8:ACAD:27::1/64
 ipv6 nd managed-config-flag
 ipv6 dhcp server VLAN27DHCP6
!
!
router eigrp LAB2114
 !
 address-family ipv4 unicast autonomous-system 1
  !
  topology base
  exit-af-topology
  network 10.0.0.0 0.0.255.255
  eigrp router-id 0.0.0.132
 exit-address-family
 !
 address-family ipv6 unicast autonomous-system 1
  !
  af-interface default
   passive-interface
  exit-af-interface
  !
  af-interface Ethernet2/3
   no passive-interface
  exit-af-interface
  !
  topology base
  exit-af-topology
  eigrp router-id 0.0.0.132
 exit-address-family
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
!
!
!
control-plane
!
banner motd ^C This is D2, Trouble Ticket 21.1.4.1  ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 exec-timeout 5 0
 login local
 transport input telnet
!
end

