!
version 15.4
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
vrf definition Mgmt-intf
 !
 address-family ipv4
 exit-address-family
 !
 address-family ipv6
 exit-address-family
!
enable secret 5 $1$E0aR$kf2iom9z44BvTxXYSt6hb/
!
aaa new-model
!
!
aaa authentication login default local enable
!
!
!
!
!
aaa session-id common
!
!
!
bsd-client server url https://cloudsso.cisco.com/as/token.oauth2
clock timezone AFT 4 30
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
!
!
!
!
!


!
!
!
!
no ip domain lookup
ip domain name CCNPv8.CoPP.Lab
ip cef
login on-success log
no ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
!
!
cts logging verbose
!
!
username admin privilege 15 secret 9 $9$pTX0bv8cHqHVbH$xibDa0wuZT9HeclfiMinFSSfjLAFa4Hg7Ms4A3wT3Rk
!
redundancy
!
!
ip tftp source-interface Ethernet1/2
!
class-map match-all CM-TELNET
 match access-group name TELNET
class-map match-all CM-MGMT
 match access-group name MGMT
class-map match-all CM-ICMP
 match access-group name ICMP
class-map match-all CM-EIGRP
 match access-group name EIGRP
class-map match-all CM-SSH
 match access-group name SSH
!
policy-map PM-COPP
 class CM-EIGRP
  police rate 10 pps conform-action transmit  exceed-action transmit
 class CM-MGMT
  police 8000 conform-action transmit  exceed-action transmit
 class CM-SSH
  police 50000 conform-action transmit  exceed-action transmit
 class CM-ICMP
  police rate 10 pps conform-action transmit  exceed-action drop
 class CM-TELNET
  police 8000 conform-action drop  exceed-action drop
 class class-default
  police 12000 conform-action transmit  exceed-action transmit
!
!
!
!
!
!
!
!
!
!
!
!
!
!
interface Ethernet0/0
 no ip address
 shutdown
!
interface Ethernet0/1
 no ip address
 shutdown
!
interface Ethernet0/2
 no ip address
 shutdown
!
interface Ethernet0/3
 no ip address
 shutdown
!
interface Ethernet1/0
 no ip address
 shutdown
!
interface Ethernet1/1
 ip address 10.10.1.1 255.255.255.0
!
interface Ethernet1/2
 ip address 172.16.12.1 255.255.255.252
!
interface Ethernet1/3
 no ip address
 shutdown
!
interface Ethernet2/0
 no ip address
 shutdown
!
interface Ethernet2/1
 no ip address
 shutdown
!
interface Ethernet2/2
 no ip address
 shutdown
!
interface Ethernet2/3
 no ip address
 shutdown
!
!
router eigrp 123
 network 10.10.1.0 0.0.0.255
 network 172.16.12.0 0.0.0.3
 eigrp router-id 0.0.0.1
!
ip forward-protocol nd
!
!
no ip http server
ip http secure-server
!
ip access-list extended EIGRP
 permit eigrp any any
ip access-list extended ICMP
 permit icmp any any echo
 permit icmp any any echo-reply
 permit icmp any any ttl-exceeded
 permit icmp any any packet-too-big
 permit icmp any any port-unreachable
 permit icmp any any unreachable
ip access-list extended MGMT
 permit tcp any eq telnet any established
 permit tcp 10.10.1.0 0.0.0.255 any eq 22
 permit tcp 10.10.1.0 0.0.0.255 eq 22 any established
 permit udp 10.10.1.0 0.0.0.255 any eq snmp
 permit tcp 10.10.1.0 0.0.0.255 any eq www
 permit udp 10.10.1.0 0.0.0.255 any eq 443
 permit tcp 10.10.1.0 0.0.0.255 any eq ftp
 permit tcp 10.10.1.0 0.0.0.255 any eq ftp-data
 permit tcp 10.10.1.0 0.0.0.255 any
 permit udp any any eq syslog
 permit udp any eq domain any
 permit udp any any eq ntp
ip access-list extended SSH
 permit tcp any any eq 22
 permit tcp any eq 22 any established
ip access-list extended TELNET
 permit tcp any any eq telnet
!
!
!
!
!
!
control-plane
 service-policy input PM-COPP
!
!
!
!
!
!
!
banner motd ^CR1: Lab Trouble Ticket 1^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
 stopbits 1
line aux 0
 stopbits 1
line vty 0 4
 transport input telnet ssh
!
!
end
