!
version 15.6
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
!
hostname D2
!
boot-start-marker
boot-end-marker
!
!
!
no aaa new-model
!
!
!
clock timezone AFT 4 30
!
!
!
!
!
!
!
!
!
!
!


!
!
!
ip audit notify log
ip audit po max-events 100

no ip domain lookup
ip cef
ipv6 unicast-routing
ipv6 cef
!
!
!
!
!
!
!
multilink bundle-name authenticated
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
interface Loopback1
 ip address 10.2.1.1 255.255.255.0
 ipv6 address FE80::B0B:F002:1 link-local
 ipv6 address 2001:DB8:B0B:F002::1/64
!
interface Loopback10
 ip address 10.2.10.1 255.255.255.0
 ipv6 address 2001:DB8:B0B1::1/48
!
interface Loopback20
 ip address 10.2.20.1 255.255.255.0
 ipv6 address 2001:DB8:B0B2::1/48
!
interface Loopback30
 ip address 10.2.30.1 255.255.255.0
 ipv6 address 2001:DB8:B0B3::1/48
!
interface Loopback48
 no ip address
 ipv6 address 2001:DB8:CAFE::1/48
!
interface Ethernet0/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/3
 ip address 172.16.2.1 255.255.255.252
 ipv6 address FE80::B0B:F001:1 link-local
 ipv6 address 2001:DB8:B0B:F001::1/64
!
interface Ethernet1/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet1/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet1/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet1/3
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/3
 no ip address
 shutdown
 duplex auto
!
interface Ethernet3/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet3/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet3/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet3/3
 no ip address
 shutdown
 duplex auto
!
router bgp 65200
 bgp router-id 2.0.0.2
 bgp log-neighbor-changes
 neighbor 2001:DB8:B0B:F001::2 remote-as 65000
 neighbor 172.16.2.2 remote-as 65000
 !
 address-family ipv4
  network 10.2.1.0 mask 255.255.255.0
  network 10.2.10.0 mask 255.255.255.0
  network 10.2.20.0 mask 255.255.255.0
  network 10.2.30.0 mask 255.255.255.0
  no neighbor 2001:DB8:B0B:F001::2 activate
  neighbor 172.16.2.2 activate
 exit-address-family
 !
 address-family ipv6
  network 2001:DB8:B0B:F002::/64
  network 2001:DB8:B0B1::/48
  network 2001:DB8:B0B2::/48
  network 2001:DB8:B0B3::/48
  network 2001:DB8:CAFE::/48
  neighbor 2001:DB8:B0B:F001::2 activate
  neighbor 2001:DB8:B0B:F001::2 route-map SET-AS-PATH-CAFE out
 exit-address-family
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
!
!
ipv6 prefix-list CAFE-POLICY seq 5 permit 2001:DB8:CAFE::/48
route-map SET-AS-PATH-CAFE permit 10
 match ipv6 address prefix-list CAFE-POLICY
 set as-path prepend 65200 65200 65200 65200
!
route-map SET-AS-PATH-CAFE permit 20
!
!
!
control-plane
!
banner motd ^C This is D2, Trouble Ticket 14.1.2.1 ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 login
!
end
