!
version 15.4
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname R2
!
boot-start-marker
boot-end-marker
!
!
!
no aaa new-model
!
!
!
bsd-client server url https://cloudsso.cisco.com/as/token.oauth2
clock timezone AFT 4 30
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
!
!
!
!
!


!
!
!
!
no ip domain lookup
ip cef
ipv6 unicast-routing
ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
!
!
cts logging verbose
!
!
!
redundancy
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
interface Loopback0
 description Loopback for BGP peering
 ip address 192.168.99.2 255.255.255.255
 ipv6 address FE80::99:2 link-local
 ipv6 address 2001:DB8:C0C0:99::2/128
 ospfv3 1 ipv6 area 0
 ospfv3 1 ipv4 area 0
!
interface Loopback1
 ip address 192.168.3.1 255.255.255.0
 ipv6 address FE80::A021:1 link-local
 ipv6 address 2001:DB8:C0C0:A021::1/64
 ospfv3 1 ipv6 area 0
 ospfv3 1 ipv6 network point-to-point
 ospfv3 1 ipv4 area 0
 ospfv3 1 ipv4 network point-to-point
!
interface Loopback2
 ip address 192.168.4.1 255.255.255.0
 ipv6 address FE80::A022:1 link-local
 ipv6 address 2001:DB8:C0C0:A022::1/64
 ospfv3 1 ipv6 area 0
 ospfv3 1 ipv6 network point-to-point
 ospfv3 1 ipv4 area 0
 ospfv3 1 ipv4 network point-to-point
!
interface Ethernet0/0
 no ip address
 shutdown
!
interface Ethernet0/1
 no ip address
 shutdown
!
interface Ethernet0/2
 no ip address
 shutdown
!
interface Ethernet0/3
 no ip address
 shutdown
!
interface Ethernet1/0
 no ip address
 shutdown
!
interface Ethernet1/1
 no ip address
 shutdown
!
interface Ethernet1/2
 no ip address
 shutdown
!
interface Ethernet1/3
 no ip address
 shutdown
!
interface Ethernet2/0
 no ip address
 shutdown
!
interface Ethernet2/1
 ip address 192.168.2.2 255.255.255.0
 ipv6 address FE80::A001:2 link-local
 ipv6 address 2001:DB8:C0C0:A001::2/64
 ospfv3 1 ipv6 area 0
 ospfv3 1 ipv4 area 0
!
interface Ethernet2/2
 no ip address
 shutdown
!
interface Ethernet2/3
 ip address 192.168.5.2 255.255.255.0
 ipv6 address FE80::A002:2 link-local
 ipv6 address 2001:DB8:C0C0:A002::2/64
 ospfv3 1 ipv6 area 0
 ospfv3 1 ipv4 area 0
!
interface Ethernet3/0
 no ip address
 shutdown
!
interface Ethernet3/1
 no ip address
 shutdown
!
interface Ethernet3/2
 no ip address
 shutdown
!
interface Ethernet3/3
 no ip address
 shutdown
!
router ospfv3 1
 !
 address-family ipv4 unicast
  router-id 2.2.2.2
 exit-address-family
 !
 address-family ipv6 unicast
  router-id 2.2.2.2
 exit-address-family
!
router bgp 65000
 bgp router-id 2.2.2.2
 bgp log-neighbor-changes
 neighbor 2001:DB8:C0C0:99::1 remote-as 65000
 neighbor 2001:DB8:C0C0:99::1 update-source Loopback0
 neighbor 2001:DB8:C0C0:99::3 remote-as 65000
 neighbor 2001:DB8:C0C0:99::3 update-source Loopback0
 neighbor 192.168.99.1 remote-as 65000
 neighbor 192.168.99.1 update-source Loopback0
 neighbor 192.168.99.3 remote-as 65000
 neighbor 192.168.99.3 update-source Loopback0
 !
 address-family ipv4
  network 192.168.3.0
  network 192.168.4.0
  no neighbor 2001:DB8:C0C0:99::1 activate
  no neighbor 2001:DB8:C0C0:99::3 activate
  neighbor 192.168.99.1 activate
  neighbor 192.168.99.3 activate
 exit-address-family
 !
 address-family ipv6
  network 2001:DB8:C0C0:A021::/64
  network 2001:DB8:C0C0:A022::/64
  neighbor 2001:DB8:C0C0:99::1 activate
  neighbor 2001:DB8:C0C0:99::3 activate
 exit-address-family
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
!
!
!
control-plane
!
!
!
!
!
!
!
banner motd ^C This is R2, Trouble Ticket 14.1.2.2 ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 login
 transport input none
!
!
end

