!
version 15.6
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
!
hostname D1
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$9Jcy$6Se4KncXsgiSGnwYpUuaP0
!
no aaa new-model
!
!
!
clock timezone AFT 4 30
!
!
!
!
!
!
!
!
!
!
!


!
!
!
ip audit notify log
ip audit po max-events 100

no ip domain lookup
ip cef
ipv6 unicast-routing
ipv6 cef
!
!
!
!
!
!
!
multilink bundle-name authenticated
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
username admin privilege 15 secret 9 $9$bmiPiBc9xWGUJQ$SBjLxHJmN/VwOQHW3s7pi/tOK3/EaUqXeES5yTlhXBM
!
vlan internal allocation policy ascending
!
!
!
!
!
interface Ethernet0/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/3
 no ip address
 shutdown
 duplex auto
!
interface Ethernet1/0
 switchport
 switchport access vlan 11
 switchport mode access
 duplex auto
 spanning-tree portfast
!
interface Ethernet1/1
 no ip address
 ipv6 address FE80::D1:1 link-local
 ipv6 address 2001:DB8:ACAD:192::2/64
 ospfv3 1 ipv6 area 0
!
interface Ethernet1/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet1/3
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/0
 switchport
 switchport access vlan 12
 switchport mode access
 duplex auto
 spanning-tree portfast
!
interface Ethernet2/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/3
 no ip address
 shutdown
 duplex auto
!
interface Vlan11
 no ip address
 ipv6 address FE80::D1:2 link-local
 ipv6 address 2001:DB8:ACAD:224::1/64
 ipv6 traffic-filter CLIENT-CONTROL-VLAN11 in
 ospfv3 1 ipv6 area 0
!
interface Vlan12
 no ip address
 ipv6 address FE80::D1:3 link-local
 ipv6 address 2001:DB8:ACAD:225::1/64
 ipv6 traffic-filter CLIENT-CONTROL-VLAN12 in
 ospfv3 1 ipv6 area 0
!
router ospfv3 1
 router-id 0.0.13.1
 !
 address-family ipv6 unicast
  passive-interface Vlan11
  passive-interface Vlan12
 exit-address-family
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
!
!
!
ipv6 access-list CLIENT-CONTROL-VLAN11
 permit ipv6 2001:DB8:ACAD:224::/64 any
 permit icmp any any echo-request
 permit icmp any any echo-reply
 permit icmp any any nd-na
 permit icmp any any nd-ns
 deny ipv6 any any
!
ipv6 access-list CLIENT-CONTROL-VLAN12
 permit ipv6 2001:DB8:ACAD:225::/64 any
 permit icmp any any echo-request
 permit icmp any any echo-reply
 permit icmp any any nd-na
 permit icmp any any nd-ns
 deny ipv6 any any
!
control-plane
!
banner motd ^C This is D1, Trouble Ticket 21.1.3.2  ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 exec-timeout 5 0
 login local
 transport input telnet
!
end

