!
version 15.4
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname R2
!
boot-start-marker
boot-end-marker
!
!
!
no aaa new-model
!
!
!
bsd-client server url https://cloudsso.cisco.com/as/token.oauth2
clock timezone AFT 4 30
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
!
!
!
!
!


!
!
!
!
no ip domain lookup
ip cef
no ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
!
!
cts logging verbose
!
!
!
redundancy
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
interface Ethernet0/0
 no ip address
 shutdown
!
interface Ethernet0/1
 no ip address
 shutdown
!
interface Ethernet0/2
 no ip address
 shutdown
!
interface Ethernet0/3
 no ip address
 shutdown
!
interface Ethernet1/0
 no ip address
 shutdown
!
interface Ethernet1/1
 no ip address
 shutdown
!
interface Ethernet1/2
 no ip address
 shutdown
!
interface Ethernet1/3
 no ip address
 shutdown
!
interface Ethernet2/0
 no ip address
 shutdown
!
interface Ethernet2/1
 description Connection to R1
 ip address 172.16.0.1 255.255.255.252
!
interface Ethernet2/2
 no ip address
 shutdown
!
interface Ethernet2/3
 description Connection to R3
 ip address 172.16.1.1 255.255.255.252
!
interface Ethernet3/0
 no ip address
 shutdown
!
interface Ethernet3/1
 no ip address
 shutdown
!
interface Ethernet3/2
 no ip address
 shutdown
!
interface Ethernet3/3
 no ip address
 shutdown
!
router ospf 123
 router-id 2.2.2.1
 auto-cost reference-bandwidth 1000
 network 172.16.0.0 0.0.0.3 area 0
 network 172.16.1.0 0.0.0.3 area 0
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
!
!
!
control-plane
!
!
!
!
!
!
!
banner motd ^C This is R2, Troubleshoot Route Maps and PBR ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 login
 transport input none
!
!
end

