!
version 15.4
no service timestamps debug uptime
no service timestamps log uptime
no service password-encryption
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$aeWa$hAjTUz8uADO93FnS7mO9m/
!
aaa new-model
!
!
aaa authentication login default local
!
!
!
!
!
aaa session-id common
!
!
!
bsd-client server url https://cloudsso.cisco.com/as/token.oauth2
clock timezone EET 2 0
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
!
!
!
!
!


!
!
!
!
ip domain name ccnplab.local
ip cef
no ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
!
!
cts logging verbose
!
!
username admin privilege 15 secret 9 $9$IAW20fIvwvYL2H$jW9nCIwSvFnxl4GYewLmpRhWoENNC6QcVwvE1Hpf0n6
!
redundancy
!
!
ip ssh version 2
!
!
!
!
!
!
!
!
!
!
!
!
!
interface Loopback0
 ip address 1.1.1.1 255.255.255.255
!
interface Ethernet0/0
 no ip address
 shutdown
!
interface Ethernet0/1
 no ip address
 shutdown
!
interface Ethernet0/2
 no ip address
 shutdown
!
interface Ethernet0/3
 no ip address
 shutdown
!
interface Ethernet1/0
 no ip address
 shutdown
!
interface Ethernet1/1
 ip address 10.10.10.1 255.255.255.0
 ip access-group ALLOW-TFTP out
!
interface Ethernet1/2
 ip address 10.10.12.1 255.255.255.252
!
interface Ethernet1/3
 no ip address
 shutdown
!
interface Ethernet2/0
 no ip address
 shutdown
!
interface Ethernet2/1
 no ip address
 shutdown
!
interface Ethernet2/2
 no ip address
 shutdown
!
interface Ethernet2/3
 no ip address
 shutdown
!
!
router eigrp 10
 network 10.10.10.0 0.0.0.255
 network 10.10.12.0 0.0.0.3
 passive-interface Ethernet1/1
 eigrp router-id 10.10.10.1
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
ip access-list standard PERMIT-ADMIN
 permit 10.10.10.0 0.0.0.255
!
ip access-list extended ALLOW-TFTP
 permit udp 10.10.0.0 0.0.255.255 host 10.10.10.10 eq tftp
 permit udp 10.10.0.0 0.0.255.255 host 10.10.10.10 gt 1024
 permit udp 10.10.0.0 0.0.255.255 host 10.10.10.10 eq syslog
 permit udp 10.10.0.0 0.0.255.255 host 10.10.10.10 eq snmp
 permit udp 10.10.0.0 0.0.255.255 host 10.10.10.10 eq snmptrap
 permit tcp 10.10.0.0 0.0.255.255 eq 22 host 10.10.10.10
 permit icmp any any
!
logging trap debugging
logging host 10.10.10.10
!
snmp-server group ADMIN v3 priv read SNMP-RO access PERMIT-ADMIN
snmp-server view SNMP-RO iso included
!
!
!
!
control-plane
!
!
!
!
!
!
!
banner motd ^C This is R1, Trouble Ticket 23.1.3.2 ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 transport input ssh
!
!
end
