!
version 15.4
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$w1/W$2XLTlsafizwKFkCbIov620
!
no aaa new-model
!
!
!
bsd-client server url https://cloudsso.cisco.com/as/token.oauth2
clock timezone AFT 4 30
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
!
!
!
!
!


!
!
!
!
no ip domain lookup
ip cef
no ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
!
!
cts logging verbose
!
!
username admin privilege 15 secret 9 $9$qYvCsYOR08UaZH$SJK/pcvmDeDPw2gAzyhL7fq8R2IobtcIZMZUeK.RBWc
!
redundancy
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
interface Loopback0
 ip address 209.165.226.1 255.255.255.255
!
interface Ethernet0/0
 no ip address
 shutdown
!
interface Ethernet0/1
 no ip address
 shutdown
!
interface Ethernet0/2
 no ip address
 shutdown
!
interface Ethernet0/3
 no ip address
 shutdown
!
interface Ethernet1/0
 no ip address
 shutdown
!
interface Ethernet1/1
 ip address 192.0.0.1 255.255.255.0
 ip access-group IPCHECK in
!
interface Ethernet1/2
 no ip address
 shutdown
!
interface Ethernet1/3
 no ip address
 shutdown
!
interface Serial2/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial2/1
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial2/2
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial2/3
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial3/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial3/1
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial3/2
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial3/3
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial4/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial4/1
 ip address 209.165.201.1 255.255.255.0
 ip access-group BOGON-MARTIAN in
 serial restart-delay 0
!
interface Serial4/2
 ip address 209.165.200.1 255.255.255.0
 ip access-group BOGON-MARTIAN in
 serial restart-delay 0
!
interface Serial4/3
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial5/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial5/1
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial5/2
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial5/3
 no ip address
 shutdown
 serial restart-delay 0
!
router ospf 1
 router-id 1.1.1.1
 network 192.0.0.0 0.0.0.255 area 0
 default-information originate always
!
router bgp 181035
 bgp router-id 209.165.226.1
 bgp log-neighbor-changes
 network 192.0.0.0
 network 209.165.224.0
 network 209.165.225.0
 neighbor 209.165.227.1 remote-as 39457
 neighbor 209.165.227.1 ebgp-multihop 3
 neighbor 209.165.227.1 update-source Loopback0
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
ip route 209.165.227.1 255.255.255.255 Serial4/2
ip route 209.165.227.1 255.255.255.255 Serial4/1
!
ip access-list standard BOGON-MARTIAN
 deny   209.165.226.1
 deny   10.0.0.0 0.255.255.255
 deny   172.0.0.0 0.31.255.255
 deny   192.168.0.0 0.0.255.255
 deny   127.0.0.0 0.255.255.255
 deny   192.0.0.0 0.0.0.255
 deny   209.165.224.0 0.0.0.255
 deny   209.165.225.0 0.0.0.255
 permit any
!
ip access-list extended IPCHECK
 permit ip 209.165.224.0 0.0.1.255 any
 permit ip 192.0.0.0 0.0.0.255 any
ip access-list extended VTY-CONTROL
 permit ip 209.165.224.0 0.0.0.255 any time-range REMOTE-CONTROL
 deny   ip any any log
!
!
!
!
control-plane
!
!
!
!
!
!
!
banner motd ^C This is R1, Trouble Ticket 21.1.2.3 ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 access-class VTY-CONTROL in
 exec-timeout 5 0
 login local
 transport input telnet
!
time-range REMOTE-CONTROL
 periodic weekdays 0:00 to 5:00
 periodic weekend 0:00 to 5:00
!
!
end

