!
version 15.6
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
!
hostname D1
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$1i0n$E5koYFzrKP7l3CkSxGyCJ0
!
no aaa new-model
!
!
!
clock timezone AFT 4 30
!
!
!
!
!
!
!
!
!
!
!


!
!
!
ip audit notify log
ip audit po max-events 100

no ip domain lookup
ip cef
ipv6 unicast-routing
ipv6 cef
!
!
!
!
!
!
!
multilink bundle-name authenticated
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
username admin secret 9 $9$YUNLThP45YZsOd$qEWtGR8AMQSt8pPta2f87Kpv/boGr/hmMzpb136SpII
!
vlan internal allocation policy ascending
!
!
!
!
!
interface Loopback0
 no ip address
 ipv6 address FE80::D1:2 link-local
 ipv6 address 2001:DB8:ACAD:1000::1/64
!
interface Loopback1
 no ip address
 ipv6 address FE80::D1:3 link-local
 ipv6 address 2001:DB8:ACAD:1001::1/64
!
interface Loopback2
 no ip address
 ipv6 address FE80::D1:4 link-local
 ipv6 address 2001:DB8:ACAD:1002::1/64
!
interface Loopback3
 no ip address
 ipv6 address FE80::D1:5 link-local
 ipv6 address 2001:DB8:ACAD:1003::1/64
!
interface Ethernet0/0
 no ip address
 duplex auto
 ipv6 address FE80::D1:1 link-local
 ipv6 address 2001:DB8:1D1::2/64
!
interface Ethernet0/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/3
 no ip address
 shutdown
 duplex auto
!
!
router eigrp LAB513
 !
 address-family ipv6 unicast autonomous-system 513
  !
  af-interface Ethernet0/0
   summary-address 2001:DB8:ACAD:1000::/62
  exit-af-interface
  !
  topology base
  exit-af-topology
  eigrp router-id 131.131.131.131
  eigrp stub receive-only
 exit-address-family
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
!
!
!
control-plane
!
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 login local
 transport input telnet
!
end
