!
version 15.4
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname R2
!
boot-start-marker
boot-end-marker
!
!
!
no aaa new-model
!
!
!
bsd-client server url https://cloudsso.cisco.com/as/token.oauth2
clock timezone AFT 4 30
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
!
!
!
!
!


!
!
!
!
no ip domain lookup
ip cef
ipv6 unicast-routing
ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
!
!
cts logging verbose
!
!
!
redundancy
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
interface Loopback0
 no ip address
 ipv6 address FE80::A202:1 link-local
 ipv6 address 2001:DB8:ACAD:A202::1/64
 ospfv3 1 ipv6 area 2
 ospfv3 1 ipv6 network point-to-point
!
interface Ethernet0/0
 no ip address
 shutdown
!
interface Ethernet0/1
 no ip address
 shutdown
!
interface Ethernet0/2
 no ip address
 shutdown
!
interface Ethernet0/3
 no ip address
 shutdown
!
interface Ethernet1/0
 no ip address
 shutdown
!
interface Ethernet1/1
 no ip address
 shutdown
!
interface Ethernet1/2
 no ip address
 shutdown
!
interface Ethernet1/3
 no ip address
 shutdown
!
interface Ethernet2/0
 no ip address
 shutdown
!
interface Ethernet2/1
 no ip address
 ipv6 address FE80::A201:2 link-local
 ipv6 address 2001:DB8:ACAD:A201::2/64
 ospfv3 1 ipv6 area 2
!
interface Ethernet2/2
 no ip address
 shutdown
!
interface Ethernet2/3
 no ip address
 shutdown
!
interface Ethernet3/0
 no ip address
 shutdown
!
interface Ethernet3/1
 no ip address
 shutdown
!
interface Ethernet3/2
 no ip address
 shutdown
!
interface Ethernet3/3
 no ip address
 shutdown
!
interface Ethernet4/0
 no ip address
 shutdown
!
interface Ethernet4/1
 no ip address
 shutdown
!
interface Ethernet4/2
 no ip address
 shutdown
!
interface Ethernet4/3
 no ip address
 shutdown
!
interface Ethernet5/0
 no ip address
 shutdown
!
interface Ethernet5/1
 no ip address
 shutdown
!
interface Ethernet5/2
 no ip address
 shutdown
!
interface Ethernet5/3
 no ip address
 shutdown
!
interface Ethernet6/0
 no ip address
 shutdown
!
interface Ethernet6/1
 no ip address
 shutdown
!
interface Ethernet6/2
 no ip address
 shutdown
!
interface Ethernet6/3
 no ip address
 shutdown
!
interface Ethernet7/0
 no ip address
 shutdown
!
interface Ethernet7/1
 no ip address
 shutdown
!
interface Ethernet7/2
 no ip address
 shutdown
!
interface Ethernet7/3
 no ip address
 shutdown
!
interface Ethernet8/0
 no ip address
 shutdown
!
interface Ethernet8/1
 no ip address
 shutdown
!
interface Ethernet8/2
 no ip address
 shutdown
!
interface Ethernet8/3
 no ip address
 shutdown
!
interface Ethernet9/0
 no ip address
 shutdown
!
interface Ethernet9/1
 no ip address
 shutdown
!
interface Ethernet9/2
 no ip address
 shutdown
!
interface Ethernet9/3
 no ip address
 shutdown
!
router ospfv3 1
 !
 address-family ipv6 unicast
  router-id 2.2.2.2
 exit-address-family
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
!
!
!
control-plane
!
!
!
!
!
!
!
banner motd ^C This is R2, Trouble Ticket 10.1.2.2 ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 login
 transport input none
!
!
end

