!
version 15.4
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$MeIm$7LuXI8o0u6kmpbDS4BdIa0
!
no aaa new-model
!
!
!
bsd-client server url https://cloudsso.cisco.com/as/token.oauth2
clock timezone AFT 4 30
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
!
!
!
!
!


!
!
!
!
ip cef
ipv6 unicast-routing
ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
!
!
cts logging verbose
!
!
username admin privilege 15 secret 9 $9$1Hj7C8zm5XLdlX$38gaeQIojkS4/JrvBFHo5FiwS180j4Ph0C5BTkViT.A
!
redundancy
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
interface Ethernet0/0
 no ip address
 shutdown
!
interface Ethernet0/1
 no ip address
 shutdown
!
interface Ethernet0/2
 no ip address
 shutdown
!
interface Ethernet0/3
 no ip address
 shutdown
!
interface Ethernet1/0
 no ip address
 ipv6 address FE80::1:2 link-local
 ipv6 address 2001:DB8:0:1::1/64
!
interface Ethernet1/1
 no ip address
 shutdown
!
interface Ethernet1/2
 no ip address
 ipv6 address FE80::1:1 link-local
 ipv6 address 2001:DB8:0:12::1/64
!
interface Ethernet1/3
 no ip address
 shutdown
!
interface Ethernet2/0
 no ip address
 shutdown
!
interface Ethernet2/1
 no ip address
 shutdown
!
interface Ethernet2/2
 no ip address
 shutdown
!
interface Ethernet2/3
 no ip address
 shutdown
!
interface Ethernet3/0
 no ip address
 shutdown
!
interface Ethernet3/1
 no ip address
 shutdown
!
interface Ethernet3/2
 no ip address
 shutdown
!
interface Ethernet3/3
 no ip address
 shutdown
!
interface Serial4/0
 no ip address
 ipv6 address FE80::1:3 link-local
 ipv6 address 2001:DB8:0:13::1/64
 serial restart-delay 0
!
interface Serial4/1
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial4/2
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial4/3
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial5/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial5/1
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial5/2
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial5/3
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial6/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial6/1
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial6/2
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial6/3
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial7/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial7/1
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial7/2
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial7/3
 no ip address
 shutdown
 serial restart-delay 0
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
ipv6 route 2001:DB8:0:3::/64 2001:DB8:0:12::2 12
ipv6 route 2001:DB8:0:3::/64 2001:DB8:0:13::2 10
!
!
!
control-plane
!
!
!
!
!
!
!
banner motd ^C This is R1, Trouble Ticket 1.1.3.2 ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 login local
 transport input telnet
!
!
end

