!
version 15.4
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname R3
!
boot-start-marker
boot-end-marker
!
!
!
no aaa new-model
!
!
!
bsd-client server url https://cloudsso.cisco.com/as/token.oauth2
clock timezone AFT 4 30
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
!
!
!
!
!


!
!
!
!
no ip domain lookup
ip cef
no ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
!
!
cts logging verbose
!
!
!
redundancy
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
interface Loopback0
 ip address 192.168.3.1 255.255.255.0
!
interface Loopback1
 ip address 172.16.3.1 255.255.255.0
!
interface Tunnel1
 ip address 100.100.100.3 255.255.255.248
 ip mtu 1400
 ip nhrp authentication NHRPauth
 ip nhrp map multicast 192.0.2.1
 ip nhrp map 100.100.100.1 192.0.2.1
 ip nhrp network-id 1
 ip nhrp nhs 100.100.100.1
 ip tcp adjust-mss 1360
 tunnel source Loopback0
 tunnel destination 192.0.2.1
 tunnel key 999
!
interface Ethernet0/0
 no ip address
 shutdown
!
interface Ethernet0/1
 no ip address
 shutdown
!
interface Ethernet0/2
 no ip address
 shutdown
!
interface Ethernet0/3
 no ip address
 shutdown
!
interface Ethernet1/0
 no ip address
 shutdown
!
interface Ethernet1/1
 no ip address
 shutdown
!
interface Ethernet1/2
 no ip address
 shutdown
!
interface Ethernet1/3
 no ip address
 shutdown
!
interface Ethernet2/0
 no ip address
 shutdown
!
interface Ethernet2/1
 no ip address
 shutdown
!
interface Ethernet2/2
 no ip address
 shutdown
!
interface Ethernet2/3
 no ip address
 shutdown
!
interface Ethernet3/0
 ip address 203.0.113.2 255.255.255.252
!
interface Ethernet3/1
 no ip address
 shutdown
!
interface Ethernet3/2
 no ip address
 shutdown
!
interface Ethernet3/3
 no ip address
 shutdown
!
!
router eigrp DMVPN_TUNNEL_NET
 !
 address-family ipv4 unicast autonomous-system 68
  !
  topology base
  exit-af-topology
  network 100.100.100.0 0.0.0.7
  network 172.16.3.0 0.0.0.255
  eigrp router-id 3.3.3.3
  eigrp stub connected
 exit-address-family
!
!
router eigrp DMVPN_TRANS_NET
 !
 address-family ipv4 unicast autonomous-system 168
  !
  topology base
  exit-af-topology
  network 192.168.3.0
  network 203.0.113.0 0.0.0.3
  eigrp router-id 30.3.3.3
  eigrp stub connected
 exit-address-family
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
!
!
!
control-plane
!
!
!
!
!
!
!
banner motd ^C R3, Implement DMVPN Spoke 2 ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 exec-timeout 0 0
 privilege level 15
 password cisco123
 logging synchronous
 login
 transport input none
!
!
end
