!
version 15.6
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
!
hostname D2
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$GSfh$uqimDyQuIhq3/HjL9UFoa0
!
no aaa new-model
!
!
!
clock timezone AFT 4 30
!
!
!
!
!
!
!
!
!
!
!


!
!
!
ip audit notify log
ip audit po max-events 100

no ip domain lookup
ip cef
no ipv6 cef
!
!
!
!
!
!
!
multilink bundle-name authenticated
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
username admin privilege 15 secret 9 $9$i7lHrTMtou3QAD$c2eSXtvgkF.puDShofFP41/oYKnbaw.K4UzvxMGacM.
!
vlan internal allocation policy ascending
!
!
!
!
!
interface Ethernet0/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/3
 no ip address
 shutdown
 duplex auto
!
interface Ethernet1/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet1/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet1/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet1/3
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/3
 switchport
 switchport trunk encapsulation dot1q
 switchport mode trunk
 switchport nonegotiate
 duplex auto
!
interface Ethernet3/0
 switchport
 switchport access vlan 16
 switchport mode access
 duplex auto
 spanning-tree portfast
!
interface Ethernet3/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet3/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet3/3
 no ip address
 shutdown
 duplex auto
!
interface Ethernet4/0
 switchport
 switchport access vlan 27
 switchport mode access
 duplex auto
 spanning-tree portfast
!
interface Ethernet4/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet4/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet4/3
 no ip address
 shutdown
 duplex auto
!
interface Vlan27
 ip address 10.0.27.2 255.255.255.0
!
ip default-gateway 10.0.27.1
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
!
!
!
control-plane
!
banner motd ^C This is D2, Trouble Ticket 21.1.2.3 ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 exec-timeout 5 0
 login local
 transport input telnet
!
end

