!
version 15.6
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
!
hostname D2
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$dlJw$nlJp0mjX4Jfbt6p8A54N4.
!
no aaa new-model
!
!
!
clock timezone AFT 4 30
!
!
!
!
!
!
!
!
!
!
!


!
!
!
ip audit notify log
ip audit po max-events 100

ip cef
no ipv6 cef
!
!
!
!
!
!
!
multilink bundle-name authenticated
!
key chain security
 key 1
   key-string cisco12345
!
!
!
!
spanning-tree mode rapid-pvst
spanning-tree extend system-id
username admin privilege 15 secret 9 $9$2x2e9J3QZj.lvP$8NIs7K/5UGGVR8l09qq3jOJQLekLrM23kGq4wPKO94k
!
vlan internal allocation policy ascending
!
!
!
!
!
interface Loopback0
 ip address 192.168.20.1 255.255.255.0
!
interface Loopback1
 ip address 192.168.21.1 255.255.255.0
!
interface Ethernet0/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/1
 ip address 172.16.1.2 255.255.255.0
 ip authentication mode eigrp 421 md5
 ip authentication key-chain eigrp 421 security
!
interface Ethernet0/2
 ip address 172.16.13.2 255.255.255.0
 ip authentication mode eigrp 421 md5
 ip authentication key-chain eigrp 421 security
!
interface Ethernet0/3
 no ip address
 shutdown
 duplex auto
!
interface Ethernet1/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet1/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet1/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet1/3
 no ip address
 shutdown
 duplex auto
!
!
router eigrp 421
 network 172.16.1.0 0.0.0.255
 network 172.16.13.0 0.0.0.255
 network 192.168.20.0
 network 192.168.21.0
 eigrp router-id 132.132.132.132
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
!
!
!
control-plane
!
banner motd ^C This is D2, Trouble Ticket 4.1.2.3 ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 login local
 transport input telnet
!
end
