!
version 15.4
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname R3
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$7tEU$2pP8mjFxwrQuJwg9SaxkK1
!
no aaa new-model
!
!
!
bsd-client server url https://cloudsso.cisco.com/as/token.oauth2
clock timezone AFT 4 30
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
!
!
!
!
!


!
!
!
!
no ip domain lookup
ip cef
ipv6 unicast-routing
ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
!
!
cts logging verbose
!
!
username admin privilege 15 secret 9 $9$mXx54XjZht5GDH$LTq3WohJk6a3di13wIa79.oVnzGEqzoz4aEL2DxytSo
!
redundancy
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
interface Loopback0
 ip address 209.165.200.227 255.255.255.255
 ipv6 address FE80::3:5 link-local
 ipv6 address 2001:DB8:ACAD:227::1/64
!
interface Loopback1
 ip address 209.165.227.1 255.255.255.255
!
interface Ethernet0/0
 no ip address
 shutdown
!
interface Ethernet0/1
 no ip address
 shutdown
!
interface Ethernet0/2
 no ip address
 shutdown
!
interface Ethernet0/3
 no ip address
 shutdown
!
interface Ethernet1/0
 no ip address
 shutdown
!
interface Ethernet1/1
 no ip address
 shutdown
!
interface Ethernet1/2
 no ip address
 shutdown
!
interface Ethernet1/3
 no ip address
 shutdown
!
interface Ethernet2/0
 no ip address
 shutdown
!
interface Ethernet2/1
 no ip address
 shutdown
!
interface Ethernet2/2
 no ip address
 shutdown
!
interface Ethernet2/3
 no ip address
 shutdown
!
interface Ethernet3/0
 no ip address
 shutdown
!
interface Ethernet3/1
 no ip address
 shutdown
!
interface Ethernet3/2
 ip address 10.0.0.1 255.255.255.0
 ip nat inside
 ip virtual-reassembly in
 ipv6 address FE80::3:1 link-local
 ipv6 address 2001:DB8:ACAD:10::1/64
!
interface Ethernet3/3
 no ip address
 shutdown
!
interface Serial4/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial4/1
 ip address 209.165.241.2 255.255.255.240
 ip nat outside
 ip virtual-reassembly in
 ipv6 address FE80::3:4 link-local
 ipv6 address 2001:DB8:ACAD:2001::2/64
 serial restart-delay 0
!
interface Serial4/2
 ip address 209.165.240.2 255.255.255.240
 ip nat outside
 ip virtual-reassembly in
 ipv6 address FE80::3:3 link-local
 ipv6 address 2001:DB8:ACAD:2000::2/64
 serial restart-delay 0
!
interface Serial4/3
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial5/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial5/1
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial5/2
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial5/3
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial6/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial6/1
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial6/2
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial6/3
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial7/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial7/1
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial7/2
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial7/3
 no ip address
 shutdown
 serial restart-delay 0
!
!
router eigrp LAB2114
 !
 address-family ipv4 unicast autonomous-system 1
  !
  topology base
   distribute-list prefix ROUTE-CONTROL4 out Ethernet3/2
   redistribute static
  exit-af-topology
  network 10.0.0.0 0.0.0.255
  eigrp router-id 0.0.0.3
 exit-address-family
 !
 address-family ipv6 unicast autonomous-system 1
  !
  af-interface default
   shutdown
  exit-af-interface
  !
  af-interface Ethernet3/2
   no shutdown
  exit-af-interface
  !
  topology base
   distribute-list prefix-list ROUTE-CONTROL6 out Ethernet3/2
   redistribute static
  exit-af-topology
  eigrp router-id 0.0.0.3
 exit-address-family
!
router bgp 41
 bgp router-id 3.3.3.3
 bgp log-neighbor-changes
 neighbor 2001:DB8:ACAD:2000::1 remote-as 15
 neighbor 2001:DB8:ACAD:2001::1 remote-as 15
 neighbor 209.165.200.226 remote-as 15
 neighbor 209.165.200.226 ebgp-multihop 3
 neighbor 209.165.200.226 update-source Loopback0
 !
 address-family ipv4
  network 209.165.227.1 mask 255.255.255.255
  no neighbor 2001:DB8:ACAD:2000::1 activate
  no neighbor 2001:DB8:ACAD:2001::1 activate
  neighbor 209.165.200.226 activate
 exit-address-family
 !
 address-family ipv6
  network 2001:DB8:ACAD:16::/64
  network 2001:DB8:ACAD:27::/64
  neighbor 2001:DB8:ACAD:2000::1 activate
  neighbor 2001:DB8:ACAD:2001::1 activate
  neighbor 2001:DB8:ACAD:2001::1 route-map ROUTE-BALANCE6 in
 exit-address-family
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
ip nat inside source list NAT-ELIGIBLE interface Loopback1 overload
ip route 0.0.0.0 0.0.0.0 209.165.200.226
ip route 209.165.200.226 255.255.255.255 209.165.240.1
ip route 209.165.200.226 255.255.255.255 209.165.241.1
!
ip access-list standard NAT-ELIGIBLE
 permit 10.0.0.0 0.0.255.255
!
!
ip prefix-list ROUTE-CONTROL4 seq 5 permit 0.0.0.0/0
ipv6 route 2001:DB8:ACAD:226::/64 Serial4/1 2001:DB8:ACAD:2001::1
ipv6 route 2001:DB8:ACAD:226::/64 Serial4/2 2001:DB8:ACAD:2000::1
ipv6 route ::/0 2001:DB8:ACAD:226::1
!
!
ipv6 prefix-list EVEN-NETWORK-6 seq 5 permit 2001:DB8:ACAD:224::/63
!
ipv6 prefix-list ROUTE-CONTROL6 seq 5 permit ::/0
route-map ROUTE-BALANCE6 permit 10
 match ipv6 address prefix-list EVEN-NETWORK-6
 set local-preference 200
!
!
!
control-plane
!
!
!
!
!
!
!
banner motd ^C This is R3, Trouble Ticket 21.1.4.2 ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 exec-timeout 5 0
 login local
 transport input telnet
!
!
end

