!
version 15.6
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
!
hostname D1
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$GFJo$KQzHi7zSkVRXtkuzUmHnS/
!
no aaa new-model
!
!
!
clock timezone AFT 4 30
!
!
!
!
!
!
!
!
!
!
!


!
!
!
ip audit notify log
ip audit po max-events 100

no ip domain lookup
ip cef
ipv6 unicast-routing
ipv6 cef
!
!
!
!
!
!
!
multilink bundle-name authenticated
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
username admin privilege 15 secret 9 $9$GK1QFJPBGuDRJN$K2rjF70T9rs4IoKD4inr6EzEFLZlm0Dgz7FJ5iMT1o6
!
vlan internal allocation policy ascending
!
!
!
!
!
interface Loopback0
 ip address 209.165.201.1 255.255.255.128
 ipv6 address FE80::209:1 link-local
 ipv6 address 2001:DB8:209:165:201::1/80
!
interface Ethernet0/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/1
 ip address 10.1.11.2 255.255.255.0
 ipv6 address FE80::11:2 link-local
 ipv6 address 2001:DB8:ACAD:11::2/64
 ospfv3 1 ipv4 area 11
 ospfv3 1 ipv6 area 11
!
interface Ethernet0/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/3
 no ip address
 shutdown
 duplex auto
!
router ospfv3 1
 router-id 11.11.11.11
 !
 address-family ipv4 unicast
  passive-interface Loopback0
  default-information originate
 exit-address-family
 !
 address-family ipv6 unicast
  passive-interface Loopback0
  default-information originate
 exit-address-family
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
ip route 0.0.0.0 0.0.0.0 Loopback0
!
ipv6 route ::/0 Loopback0
!
!
!
control-plane
!
banner motd ^C This is D1, Trouble Ticket 17.1.2.3  ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 exec-timeout 5 0
 login local
 transport input telnet
!
end

