!
version 15.4
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname R3
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$EMK6$xOXFeKw4oznULvksK01bV/
!
no aaa new-model
!
!
!
bsd-client server url https://cloudsso.cisco.com/as/token.oauth2
clock timezone AFT 4 30
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
!
!
!
!
!


!
!
!
!
no ip domain lookup
ip cef
no ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
!
!
cts logging verbose
!
!
username admin privilege 15 secret 9 $9$s5NDb3tOEakJ2H$lCP07ERncESyUX6AtrCkA9sBDa4Mu9lhlpJN153DzcI
!
redundancy
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
interface Loopback0
 ip address 209.165.201.1 255.255.255.128
!
interface Ethernet0/0
 no ip address
 shutdown
!
interface Ethernet0/1
 no ip address
 shutdown
!
interface Ethernet0/2
 no ip address
 shutdown
!
interface Ethernet0/3
 no ip address
 shutdown
!
interface Ethernet1/0
 no ip address
 shutdown
!
interface Ethernet1/1
 no ip address
 shutdown
!
interface Ethernet1/2
 no ip address
 shutdown
!
interface Ethernet1/3
 no ip address
 shutdown
!
interface Ethernet2/0
 no ip address
 shutdown
!
interface Ethernet2/1
 no ip address
 shutdown
!
interface Ethernet2/2
 no ip address
 shutdown
!
interface Ethernet2/3
 no ip address
 shutdown
!
interface Ethernet3/0
 no ip address
 shutdown
!
interface Ethernet3/1
 no ip address
 shutdown
!
interface Ethernet3/2
 ip address 192.168.23.3 255.255.255.0
!
interface Ethernet3/3
 no ip address
 shutdown
!
router bgp 64512
 bgp router-id 3.3.3.3
 bgp log-neighbor-changes
 no bgp default ipv4-unicast
 neighbor 192.168.23.2 remote-as 64512
 !
 address-family ipv4
  network 209.165.201.0 mask 255.255.255.128
  neighbor 192.168.23.2 activate
 exit-address-family
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
!
!
!
control-plane
!
!
!
!
!
!
!
banner motd ^C This is R3, Trouble Ticket 17.1.2.1 ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 login
 transport input none
!
!
end
