!
version 15.4
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname R3
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$Ic2N$92GE1vgq3L9ouA4EWPGkS/
!
no aaa new-model
!
!
!
bsd-client server url https://cloudsso.cisco.com/as/token.oauth2
clock timezone AFT 4 30
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
!
!
!
!
!


!
!
!
!
no ip domain lookup
ip cef
ipv6 unicast-routing
ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
!
!
cts logging verbose
!
!
username admin privilege 15 secret 9 $9$7CRTBdPVQtrqJ1$H4rL87VuwltaeN99d1wjM0FIdZ4GFcFHHEkxWk/S8Y2
!
redundancy
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
interface Loopback0
 ip address 10.3.3.3 255.255.255.0
 ipv6 address FE80::3:3 link-local
 ipv6 address 2001:DB8:ACAD:3::3/64
!
interface Ethernet0/0
 no ip address
 shutdown
!
interface Ethernet0/1
 no ip address
 shutdown
!
interface Ethernet0/2
 no ip address
 shutdown
!
interface Ethernet0/3
 no ip address
 shutdown
!
interface Ethernet1/0
 no ip address
 shutdown
!
interface Ethernet1/1
 no ip address
 shutdown
!
interface Ethernet1/2
 no ip address
 shutdown
!
interface Ethernet1/3
 no ip address
 shutdown
!
interface Ethernet2/0
 no ip address
 shutdown
!
interface Ethernet2/1
 no ip address
 shutdown
!
interface Ethernet2/2
 no ip address
 shutdown
!
interface Ethernet2/3
 no ip address
 shutdown
!
interface Ethernet3/0
 ip address 10.1.32.3 255.255.255.0
 ipv6 address FE80::32:3 link-local
 ipv6 address 2001:DB8:ACAD:32::3/64
!
interface Ethernet3/1
 no ip address
 shutdown
!
interface Ethernet3/2
 ip address 10.1.23.3 255.255.255.0
 ipv6 address FE80::23:3 link-local
 ipv6 address 2001:DB8:ACAD:23::3/64
!
interface Ethernet3/3
 no ip address
 shutdown
!
!
router eigrp CISCO
 !
 address-family ipv4 unicast autonomous-system 64512
  !
  af-interface default
   shutdown
  exit-af-interface
  !
  af-interface Ethernet3/2
   no shutdown
  exit-af-interface
  !
  af-interface Ethernet3/0
   no shutdown
  exit-af-interface
  !
  af-interface Loopback0
   no shutdown
  exit-af-interface
  !
  topology base
  exit-af-topology
  network 10.1.23.0 0.0.0.255
  network 10.1.32.0 0.0.0.255
  network 10.3.3.0 0.0.0.255
  eigrp router-id 3.3.3.3
 exit-address-family
 !
 address-family ipv6 unicast autonomous-system 64512
  !
  af-interface default
   shutdown
  exit-af-interface
  !
  af-interface Ethernet3/2
   no shutdown
  exit-af-interface
  !
  af-interface Ethernet3/0
   no shutdown
  exit-af-interface
  !
  af-interface Loopback0
   no shutdown
  exit-af-interface
  !
  topology base
  exit-af-topology
  eigrp router-id 3.3.3.3
 exit-address-family
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
!
!
!
control-plane
!
!
!
!
!
!
!
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 login
 transport input none
!
!
end
