!
version 15.4
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$PDp1$YwOZVReBNqfbR5gz84qbJ/
!
no aaa new-model
!
!
!
bsd-client server url https://cloudsso.cisco.com/as/token.oauth2
clock timezone AFT 4 30
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
!
!
!
!
!


!
ip dhcp excluded-address 192.168.1.1 192.168.1.5
!
ip dhcp pool HOSTS
 network 192.168.1.0 255.255.255.0
 default-router 192.168.1.1
!
!
!
ip cef
no ipv6 cef
!
multilink bundle-name authenticated
!
!
!
key chain security
 key 1
  key-string cisco12345
!
!
!
!
!
cts logging verbose
!
!
username admin privilege 15 secret 9 $9$LlnpypfJkrQN.1$NKb0.W7eoFoeZPCrM/QmxBU.eBF0OVOGc8Obj1V8PXQ
!
redundancy
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
interface Ethernet0/0
 no ip address
 shutdown
!
interface Ethernet0/1
 no ip address
 shutdown
!
interface Ethernet0/2
 no ip address
!
interface Ethernet0/2.1
 encapsulation dot1Q 1 native
 ip address 172.16.1.1 255.255.255.0
 ip authentication mode eigrp 412 md5
 ip authentication key-chain eigrp 412 security
!
interface Ethernet0/2.2
 encapsulation dot1Q 2
 ip address 192.168.1.1 255.255.255.0
!
interface Ethernet0/3
 no ip address
 shutdown
!
interface Ethernet1/0
 no ip address
 shutdown
!
interface Ethernet1/1
 no ip address
 shutdown
!
interface Ethernet1/2
 ip address 10.0.12.1 255.255.255.0
 ip authentication mode eigrp 412 md5
 ip authentication key-chain eigrp 412 security
!
interface Ethernet1/3
 no ip address
 shutdown
!
interface Ethernet2/0
 no ip address
 shutdown
!
interface Ethernet2/1
 no ip address
 shutdown
!
interface Ethernet2/2
 no ip address
 shutdown
!
interface Ethernet2/3
 no ip address
 shutdown
!
interface Ethernet3/0
 no ip address
 shutdown
!
interface Ethernet3/1
 no ip address
 shutdown
!
interface Ethernet3/2
 no ip address
 shutdown
!
interface Ethernet3/3
 no ip address
 shutdown
!
!
router eigrp 412
 network 10.0.12.0 0.0.0.255
 network 172.16.1.0 0.0.0.255
 network 192.168.1.0
 passive-interface Ethernet0/2.2
 eigrp router-id 1.1.1.1
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
!
!
!
control-plane
!
!
!
!
!
!
!
banner motd ^C This is R1, Trouble Ticket 4.1.2.3 ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 login local
 transport input telnet
!
!
end
