!
version 15.6
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
!
hostname D2
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$YIZW$XLXvHxxtmZt1h9OEP4vmQ.
!
no aaa new-model
!
!
!
clock timezone AFT 4 30
!
!
!
!
!
!
!
!
!
!
!


!
!
!
ip audit notify log
ip audit po max-events 100

no ip domain lookup
ip cef
ipv6 unicast-routing
ipv6 cef
!
!
!
!
!
!
!
multilink bundle-name authenticated
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
username admin secret 9 $9$ncDTVmWaRH2gAu$1aGejh/Q16Tm/3GyT67WOJtBptLZ9QpC2P/GUdm0fZc
!
vlan internal allocation policy ascending
!
!
!
!
!
interface Loopback0
 description SIMULATED INTERNET
 no ip address
 ipv6 address FE80::D2:2 link-local
 ipv6 address 2001:DB8:ACAD:4000::1/64
!
interface Loopback1
 description SIMULATED EXTRANET
 no ip address
 ipv6 address FE80::D2:3 link-local
 ipv6 address 2001:DB8:ACAD:4001::1/64
!
interface Ethernet0/0
 no ip address
 duplex auto
 ipv6 address FE80::D2:1 link-local
 ipv6 address 2001:DB8:3D2::2/64
!
interface Ethernet0/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/3
 no ip address
 shutdown
 duplex auto
!
!
router eigrp LAB513
 !
 address-family ipv6 unicast autonomous-system 513
  !
  topology base
   distribute-list prefix-list NO-EXTRA out Ethernet0/0
   redistribute static
  exit-af-topology
  eigrp router-id 132.132.132.132
 exit-address-family
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
ipv6 route 3FF3:DB8:ACAD::/48 Loopback1
ipv6 route ::/0 Loopback0
!
!
ipv6 prefix-list NO-EXTRA seq 5 deny 2001:DB8:ACAD:4000::/63
!
!
control-plane
!
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 login local
 transport input telnet
!
end
