!
version 15.4
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
enable secret 9 $9$PiYDX86ERSRK2X$PGOJUEmoEfBZeD653QxEHd5n869FC7IXHHFOhgoDxvM
!
no aaa new-model
clock timezone AFT 4 30
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
 --More--
*May  5 03:56:08.131: %BGP-5-ADJCHANGE: neighbor 2001:DB8:200::2 Up
!
!
!
!
!
!
!


!
!
!
!
no ip domain lookup
ip domain name ENCOR.23
ip cef
ipv6 unicast-routing
ipv6 cef
!
!
flow exporter 2314-COLLECTOR
 destination 172.16.3.10
 transport udp 9999
!
!
flow record 2314-OUT
 description Custom Flow Record for outbound traffic
 match ipv4 destination address
 match transport destination-port
 collect counter bytes
 collect counter packets
!
!
flow monitor 2314-INBOUND-MON
 exporter 2314-COLLECTOR
 cache timeout active 30
 record netflow ipv4 original-input
!
!
flow monitor 2314-OUTBOUND-MON
 exporter 2314-COLLECTOR
 cache timeout active 30
 record 2314-OUT
!
multilink bundle-name authenticated
!
!
!
!
!
!
!
!
username admin privilege 15 secret 9 $9$azmtr8BOmvs.ZX$tjR3dvP50xxPt1bAlxyZvUyitpD1gh83WLyVp5Sb0iM
!
redundancy
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
interface Ethernet0/0
 no ip address
 shutdown
!
interface Ethernet0/1
 no ip address
 shutdown
!
interface Ethernet0/2
 no ip address
 shutdown
!
interface Ethernet0/3
 no ip address
 shutdown
!
interface Ethernet1/0
 ip address 172.16.0.1 255.255.255.0
 ipv6 address FE80::1:2 link-local
 ipv6 address 2001:DB8:ACAD::1/64
 ospfv3 1 ipv4 area 0
 ospfv3 1 ipv6 area 0
!
interface Ethernet1/1
 no ip address
 shutdown
!
interface Ethernet1/2
 ip address 209.165.200.1 255.255.255.0
 ipv6 address FE80::1:1 link-local
 ipv6 address 2001:DB8:200::1/64
!
interface Ethernet1/3
 no ip address
 shutdown
!
interface Ethernet2/0
 no ip address
 shutdown
!
interface Ethernet2/1
 no ip address
 shutdown
!
interface Ethernet2/2
 no ip address
 shutdown
!
interface Ethernet2/3
 no ip address
 shutdown
!
interface Ethernet3/0
 no ip address
 shutdown
!
interface Ethernet3/1
 no ip address
 shutdown
!
interface Ethernet3/2
 no ip address
 shutdown
!
interface Ethernet3/3
 no ip address
 shutdown
!
router ospfv3 1
 router-id 0.0.138.1
 !
 address-family ipv4 unicast
  default-information originate metric-type 1
 exit-address-family
 !
 address-family ipv6 unicast
  default-information originate metric-type 1
 exit-address-family
!
router bgp 138
 bgp router-id 4.6.138.1
 bgp log-neighbor-changes
 no bgp default ipv4-unicast
 neighbor 2001:DB8:200::2 remote-as 77
 neighbor 209.165.200.2 remote-as 77
 !
 address-family ipv4
  network 172.16.0.0
  neighbor 209.165.200.2 activate
 exit-address-family
 !
 address-family ipv6
  network 2001:DB8:ACAD::/48
  neighbor 2001:DB8:200::2 activate
 exit-address-family
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
ip route 0.0.0.0 0.0.0.0 209.165.200.2
ip route 172.16.0.0 255.255.0.0 Null0
!
ip access-list standard VTY-CONTROL
 permit 172.16.0.0 0.0.255.255
 deny   any log
!
ipv6 route 2001:DB8:ACAD::/48 Null0
ipv6 route ::/0 2001:DB8:200::2
!
!
!
control-plane
!
!
!
!
!
!
!
banner motd ^C This is R1, Trouble Ticket 23.1.4.2 ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
 login local
line aux 0
line vty 0 4
 access-class VTY-CONTROL in
 exec-timeout 0 0
 login local
 transport input telnet
!
!
end

