RP/0/0/CPU0:ios#show running-config
Wed May 19 18:27:21.707 UTC
Building configuration...
!! IOS XR Configuration 6.0.1
!! Last configuration change at Wed May 19 18:15:08 2021 by cisco
!
dhcp ipv4
 vrf default relay profile client
 profile R1 relay
  helper-address vrf default 10.10.10.1
  broadcast-flag policy check
  relay information check
  relay information option
  relay information option allow-untrusted
 !
 interface GigabitEthernet0/0/0/1 relay profile R1
!
ipv4 access-list acl1
 10 permit ipv4 host 10.10.10.26 any
 20 permit ipv4 host 10.10.10.25 any
 30 permit ipv4 host 10.10.10.27 any
 40 permit ipv4 host 10.10.10.28 any
 45 permit ipv4 host 10.10.10.23 any
 50 deny ipv4 host 10.10.10.23 any
!
ipv4 access-list acl2
 10 permit ipv4 10.10.10.0 0.255.255.255 any
 20 deny ipv4 any any
!
interface MgmtEth0/0/CPU0/0
 ipv4 address dhcp
 ipv4 access-group acl2 ingress
!
interface GigabitEthernet0/0/0/0
 shutdown
!
interface GigabitEthernet0/0/0/1
 ipv4 address 10.10.0.8 255.255.255.0
 ipv4 access-group acl1 ingress
!
interface GigabitEthernet0/0/0/2
 ipv4 address 10.10.0.9 255.255.255.0
 ipv4 access-group acl1 ingress
!
interface GigabitEthernet0/0/0/3
 shutdown
!
interface GigabitEthernet0/0/0/4
 shutdown
!
interface GigabitEthernet0/0/0/5
 shutdown
!
interface GigabitEthernet0/0/0/6
 shutdown
!
interface GigabitEthernet0/0/0/7
 shutdown
!
router ospf 1
 router-id 3.3.3.3
 area 0
  interface MgmtEth0/0/CPU0/0
  !
  interface GigabitEthernet0/0/0/1
  !
  interface GigabitEthernet0/0/0/2
  !
 !
!
end