RX

Frame 690 
  Arrival Time: Apr 24, 2016 11:13:14.250603000 Central Europe Daylight Time
  Epoch Time: 1461489194.250603000 seconds
  Frame is marked: False
  Frame is ignored: False
  Protocols in frame: raw:ip:udp:rtp:amr
Raw packet data
  No link information available
Internet Protocol Version 4, Src Addr: 10.225.139.196 (0x0AE18BC4), Dst Addr: 100.66.88.191 (0x644258BF)
  Version: 4
  Header length: 20 bytes
  Differentiated Services Field: 0xb8 (DSCP 0x2e: Expedited Forwarding; ECN: 0x00: Not-ECT (Not ECN-Capable Transport))
    1011 10.. = Differentiated Services Codepoint: Expedited Forwarding (0x2e)
    .... ..00 = Explicit Congestion Notification: Not-ECT (Not ECN-Capable Transport) (0x00)
  Total Length: 101
  Identification: 0x015d (349)
  Flags: 0x00
    0... .... = Reserved bit: Not set
    .0.. .... = Don't fragment: Not set
    ..0. .... = More fragments: Not set
  Fragment offset: 0
  Time to live: 250
  Protocol: UDP (17)
  Header checksum: 0x6acc [correct]
    Good: True
    Bad: False
  Source: 10.225.139.196 (10.225.139.196)
  Destination: 100.66.88.191 (100.66.88.191)
User Datagram Protocol, Src Port: 10932 (0x2AB4), Dst Port: 1234 (0x04D2)
  Source port: 10932 (0x2AB4)
  Destination port: 1234 (0x04D2)
  Length: 81
  Checksum: 0x79cd [validation disabled]
    Good Checksum: False
    Bad Checksum: False
Real-Time Transport Protocol
  Stream setup by SDP (frame 15)
    Setup frame: 15
    Setup Method: SDP
  10.. .... = Version: RFC 1889 Version (2)
  ..0. .... = Padding: False
  ...0 .... = Extension: False
  .... 0000 = Contributing source identifiers count: 0
  0... .... = Marker: False
  Payload type: AMR-WB (116)
  Sequence number: 349
  Extended sequence number: 65885
  Timestamp: 6246208
  Synchronization Source identifier: 0x0005dd8d (384397)
Adaptive Multi-Rate
  Payload decoded as RFC 3267 bandwidth-efficient mode
  1111 .... = CMR: No mode request (15)
  .... 0... = F bit: Last frame in this payload
  .... .100  0... .... = FT bits: AMR-WB 23.85 kbit/s (8) / Frame OK
  .1.. .... = Q bit: Ok
  Frame Data (60 Bytes)

  
  
  
  
TX
  
 Frame 729 
  Arrival Time: Apr 24, 2016 11:13:14.210094000 Central Europe Daylight Time
  Epoch Time: 1461489194.210094000 seconds
  Frame is marked: False
  Frame is ignored: False
  Protocols in frame: raw:ip:udp:rtp:amr
Raw packet data
  No link information available
Internet Protocol Version 4, Src Addr: 100.68.209.100 (0x6444D164), Dst Addr: 10.225.139.196 (0x0AE18BC4)
  Version: 4
  Header length: 20 bytes
  Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00: Not-ECT (Not ECN-Capable Transport))
    0000 00.. = Differentiated Services Codepoint: Default (0x00)
    .... ..00 = Explicit Congestion Notification: Not-ECT (Not ECN-Capable Transport) (0x00)
  Total Length: 101
  Identification: 0x0175 (373)
  Flags: 0x00
    0... .... = Reserved bit: Not set
    .0.. .... = Don't fragment: Not set
    ..0. .... = More fragments: Not set
  Fragment offset: 0
  Time to live: 255
  Protocol: UDP (17)
  Header checksum: 0xedc4 [correct]
    Good: True
    Bad: False
  Source: 100.68.209.100 (100.68.209.100)
  Destination: 10.225.139.196 (10.225.139.196)
User Datagram Protocol, Src Port: 1234 (0x04D2), Dst Port: 15230 (0x3B7E)
  Source port: 1234 (0x04D2)
  Destination port: 15230 (0x3B7E)
  Length: 81
  Checksum: 0xf05b [validation disabled]
    Good Checksum: False
    Bad Checksum: False
Real-Time Transport Protocol
  Stream setup by SDP (frame 16)
    Setup frame: 16
    Setup Method: SDP
  10.. .... = Version: RFC 1889 Version (2)
  ..0. .... = Padding: False
  ...0 .... = Extension: False
  .... 0000 = Contributing source identifiers count: 0
  0... .... = Marker: False
  Payload type: AMR-WB (116)
  Sequence number: 349
  Extended sequence number: 65885
  Timestamp: 6246208
  Synchronization Source identifier: 0x0005dd8d (384397)
Adaptive Multi-Rate
  Payload decoded as RFC 3267 bandwidth-efficient mode
  1111 .... = CMR: No mode request (15)
  .... 0... = F bit: Last frame in this payload
  .... .100  0... .... = FT bits: AMR-WB 23.85 kbit/s (8) / Frame OK
  .1.. .... = Q bit: Ok
  Frame Data (60 Bytes)

  
  
  
  
TX  
  
Frame 695 
  Arrival Time: Apr 24, 2016 11:13:14.358345000 Central Europe Daylight Time
  Epoch Time: 1461489194.358345000 seconds
  Frame is marked: False
  Frame is ignored: False
  Protocols in frame: raw:ip:udp:rtp:amr
Raw packet data
  No link information available
Internet Protocol Version 4, Src Addr: 100.66.88.191 (0x644258BF), Dst Addr: 10.225.139.196 (0x0AE18BC4)
  Version: 4
  Header length: 20 bytes
  Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00: Not-ECT (Not ECN-Capable Transport))
    0000 00.. = Differentiated Services Codepoint: Default (0x00)
    .... ..00 = Explicit Congestion Notification: Not-ECT (Not ECN-Capable Transport) (0x00)
  Total Length: 47
  Identification: 0x0158 (344)
  Flags: 0x00
    0... .... = Reserved bit: Not set
    .0.. .... = Don't fragment: Not set
    ..0. .... = More fragments: Not set
  Fragment offset: 0
  Time to live: 255
  Protocol: UDP (17)
  Header checksum: 0x66bf [correct]
    Good: True
    Bad: False
  Source: 100.66.88.191 (100.66.88.191)
  Destination: 10.225.139.196 (10.225.139.196)
User Datagram Protocol, Src Port: 1234 (0x04D2), Dst Port: 10932 (0x2AB4)
  Source port: 1234 (0x04D2)
  Destination port: 10932 (0x2AB4)
  Length: 27
  Checksum: 0x69b4 [validation disabled]
    Good Checksum: False
    Bad Checksum: False
Real-Time Transport Protocol
  Stream setup by SDP (frame 18)
    Setup frame: 18
    Setup Method: SDP
  10.. .... = Version: RFC 1889 Version (2)
  ..0. .... = Padding: False
  ...0 .... = Extension: False
  .... 0000 = Contributing source identifiers count: 0
  0... .... = Marker: False
  Payload type: AMR-WB (116)
  Sequence number: 320
  Extended sequence number: 65856
  Timestamp: 6369616
  Synchronization Source identifier: 0x0005f5de (390622)
Adaptive Multi-Rate
  Payload decoded as RFC 3267 bandwidth-efficient mode
  1111 .... = CMR: No mode request (15)
  .... 0... = F bit: Last frame in this payload
  .... .100  1... .... = FT bits: Illegal Frametype - For future use (9) / Frame OK
  .1.. .... = Q bit: Ok
  Frame Data (6 Bytes)

  
  
  
RX 
  
  
  Frame 741 
  Arrival Time: Apr 24, 2016 11:13:14.409960000 Central Europe Daylight Time
  Epoch Time: 1461489194.409960000 seconds
  Frame is marked: False
  Frame is ignored: False
  Protocols in frame: raw:ip:udp:rtp:amr
Raw packet data
  No link information available
Internet Protocol Version 4, Src Addr: 10.225.139.196 (0x0AE18BC4), Dst Addr: 100.68.209.100 (0x6444D164)
  Version: 4
  Header length: 20 bytes
  Differentiated Services Field: 0xb8 (DSCP 0x2e: Expedited Forwarding; ECN: 0x00: Not-ECT (Not ECN-Capable Transport))
    1011 10.. = Differentiated Services Codepoint: Expedited Forwarding (0x2e)
    .... ..00 = Explicit Congestion Notification: Not-ECT (Not ECN-Capable Transport) (0x00)
  Total Length: 47
  Identification: 0x0140 (320)
  Flags: 0x00
    0... .... = Reserved bit: Not set
    .0.. .... = Don't fragment: Not set
    ..0. .... = More fragments: Not set
  Fragment offset: 0
  Time to live: 250
  Protocol: UDP (17)
  Header checksum: 0xf277 [correct]
    Good: True
    Bad: False
  Source: 10.225.139.196 (10.225.139.196)
  Destination: 100.68.209.100 (100.68.209.100)
User Datagram Protocol, Src Port: 15230 (0x3B7E), Dst Port: 1234 (0x04D2)
  Source port: 15230 (0x3B7E)
  Destination port: 1234 (0x04D2)
  Length: 27
  Checksum: 0xe042 [validation disabled]
    Good Checksum: False
    Bad Checksum: False
Real-Time Transport Protocol
  Stream setup by SDP (frame 16)
    Setup frame: 16
    Setup Method: SDP
  10.. .... = Version: RFC 1889 Version (2)
  ..0. .... = Padding: False
  ...0 .... = Extension: False
  .... 0000 = Contributing source identifiers count: 0
  0... .... = Marker: False
  Payload type: AMR-WB (116)
  Sequence number: 320
  Extended sequence number: 65856
  Timestamp: 6369616
  Synchronization Source identifier: 0x0005f5de (390622)
Adaptive Multi-Rate
  Payload decoded as RFC 3267 bandwidth-efficient mode
  1111 .... = CMR: No mode request (15)
  .... 0... = F bit: Last frame in this payload
  .... .100  1... .... = FT bits: Illegal Frametype - For future use (9) / Frame OK
  .1.. .... = Q bit: Ok
  Frame Data (6 Bytes)
  
  

  
  
  
TX RTCP
 
  Frame 325 
  Arrival Time: Apr 24, 2016 11:13:00.838107000 Central Europe Daylight Time
  Epoch Time: 1461489180.838107000 seconds
  Frame is marked: False
  Frame is ignored: False
  Protocols in frame: raw:ip:udp:rtcp
Raw packet data
  No link information available
Internet Protocol Version 4, Src Addr: 100.66.88.191 (0x644258BF), Dst Addr: 10.225.139.196 (0x0AE18BC4)
  Version: 4
  Header length: 20 bytes
  Differentiated Services Field: 0x00 (DSCP 0x00: Default; ECN: 0x00: Not-ECT (Not ECN-Capable Transport))
    0000 00.. = Differentiated Services Codepoint: Default (0x00)
    .... ..00 = Explicit Congestion Notification: Not-ECT (Not ECN-Capable Transport) (0x00)
  Total Length: 104
  Identification: 0x005b (91)
  Flags: 0x00
    0... .... = Reserved bit: Not set
    .0.. .... = Don't fragment: Not set
    ..0. .... = More fragments: Not set
  Fragment offset: 0
  Time to live: 255
  Protocol: UDP (17)
  Header checksum: 0x6783 [correct]
    Good: True
    Bad: False
  Source: 100.66.88.191 (100.66.88.191)
  Destination: 10.225.139.196 (10.225.139.196)
User Datagram Protocol, Src Port: 1235 (0x04D3), Dst Port: 10933 (0x2AB5)
  Source port: 1235 (0x04D3)
  Destination port: 10933 (0x2AB5)
  Length: 84
  Checksum: 0xb0fd [validation disabled]
    Good Checksum: False
    Bad Checksum: False
Real-time Transport Control Protocol (Sender Report)
  Stream setup by SDP (frame 18)
    Setup frame: 18
    Setup Method: SDP
  10.. .... = Version: RFC 1889 Version (2)
  ..0. .... = Padding: False
  ...0 0001 = Reception report count: 1
  Packet type: Sender Report (200)
  Length: 12 (52 bytes)
  Sender SSRC: 0x0005f5de (390622)
  Timestamp, MSW: 400 (0x00000190)
  Timestamp, LSW: 2847563317 (0xa9ba5e35)
  MSW and LSW as NTP timestamp: Not representable
  RTP timestamp: 6153120
  Sender's packet count: 69
  Sender's octet count: 1689
  Source 1
    Identifier: 0x0005dd8d (384397)
    SSRC contents
      Fraction lost: 9 / 256
      Cumulative number of packets lost: 8
    Extended highest sequence number received: 232
      Sequence number cycles count: 0
      Highest sequence number received: 232
    Interarrival jitter: 22
    Last SR timestamp: 25849364 (0x018a6e14)
    Delay since last SR timestamp: 11993 (182 milliseconds)
Real-time Transport Control Protocol (Source description)
  Stream setup by SDP (frame 18)
    Setup frame: 18
    Setup Method: SDP
  10.. .... = Version: RFC 1889 Version (2)
  ..0. .... = Padding: False
  ...0 0001 = Source count: 1
  Packet type: Source description (202)
  Length: 5 (24 bytes)
  Chunk 1, SSRC/CSRC 0x5F5DE
    Identifier: 0x0005f5de (390622)
    SDES items
      Type: CNAME (user and domain) (1)
      Length: 13
      Text: 100.66.88.191
      Type: END (0)
RTCP frame length check: OK - 76 bytes






RX RTCP

Frame 365 
  Arrival Time: Apr 24, 2016 11:13:00.941802000 Central Europe Daylight Time
  Epoch Time: 1461489180.941802000 seconds
  Frame is marked: False
  Frame is ignored: False
  Protocols in frame: raw:ip:udp:rtcp
Raw packet data
  No link information available
Internet Protocol Version 4, Src Addr: 10.225.139.196 (0x0AE18BC4), Dst Addr: 100.68.209.100 (0x6444D164)
  Version: 4
  Header length: 20 bytes
  Differentiated Services Field: 0xb8 (DSCP 0x2e: Expedited Forwarding; ECN: 0x00: Not-ECT (Not ECN-Capable Transport))
    1011 10.. = Differentiated Services Codepoint: Expedited Forwarding (0x2e)
    .... ..00 = Explicit Congestion Notification: Not-ECT (Not ECN-Capable Transport) (0x00)
  Total Length: 104
  Identification: 0x0043 (67)
  Flags: 0x00
    0... .... = Reserved bit: Not set
    .0.. .... = Don't fragment: Not set
    ..0. .... = More fragments: Not set
  Fragment offset: 0
  Time to live: 250
  Protocol: UDP (17)
  Header checksum: 0xf33b [correct]
    Good: True
    Bad: False
  Source: 10.225.139.196 (10.225.139.196)
  Destination: 100.68.209.100 (100.68.209.100)
User Datagram Protocol, Src Port: 15231 (0x3B7F), Dst Port: 1235 (0x04D3)
  Source port: 15231 (0x3B7F)
  Destination port: 1235 (0x04D3)
  Length: 84
  Checksum: 0x278c [validation disabled]
    Good Checksum: False
    Bad Checksum: False
Real-time Transport Control Protocol (Sender Report)
  Stream setup by SDP (frame 16)
    Setup frame: 16
    Setup Method: SDP
  10.. .... = Version: RFC 1889 Version (2)
  ..0. .... = Padding: False
  ...0 0001 = Reception report count: 1
  Packet type: Sender Report (200)
  Length: 12 (52 bytes)
  Sender SSRC: 0x0005f5de (390622)
  Timestamp, MSW: 400 (0x00000190)
  Timestamp, LSW: 2847563317 (0xa9ba5e35)
  MSW and LSW as NTP timestamp: Not representable
  RTP timestamp: 6153120
  Sender's packet count: 69
  Sender's octet count: 1689
  Source 1
    Identifier: 0x0005dd8d (384397)
    SSRC contents
      Fraction lost: 9 / 256
      Cumulative number of packets lost: 8
    Extended highest sequence number received: 232
      Sequence number cycles count: 0
      Highest sequence number received: 232
    Interarrival jitter: 22
    Last SR timestamp: 25849364 (0x018a6e14)
    Delay since last SR timestamp: 11993 (182 milliseconds)
Real-time Transport Control Protocol (Source description)
  Stream setup by SDP (frame 16)
    Setup frame: 16
    Setup Method: SDP
  10.. .... = Version: RFC 1889 Version (2)
  ..0. .... = Padding: False
  ...0 0001 = Source count: 1
  Packet type: Source description (202)
  Length: 5 (24 bytes)
  Chunk 1, SSRC/CSRC 0x5F5DE
    Identifier: 0x0005f5de (390622)
    SDES items
      Type: CNAME (user and domain) (1)
      Length: 13
      Text: 100.66.88.191
      Type: END (0)
RTCP frame length check: OK - 76 bytes
