Par Statistics
Total Non-vccgnd Signals=3357
Total Non-vccgnd Design Pins=18516
Total Non-vccgnd Conns=18516
Total Non-vccgnd Timing Constrained Conns=18408
Phase 1 CPU=5.2 sec
Phase 2 CPU=5.7 sec
Phase 3 CPU=26.7 sec
Phase 4 CPU=27.6 sec
Phase 5 CPU=40.2 sec
Phase 6 CPU=40.2 sec
Phase 7 CPU=40.2 sec
Phase 8 CPU=40.2 sec
Phase 9 CPU=40.3 sec
Phase 10 CPU=40.8 sec
AvgWirelenPerPin Fanout 1=2.0
AvgWirelenPerPin Fanout 2=3.0
AvgWirelenPerPin Fanout 3=5.7
AvgWirelenPerPin Fanout 4=6.0
AvgWirelenPerPin Fanout 10=5.2
AvgWirelenPerPin Fanout 50=4.0
AvgWirelenPerPin Fanout 100=10.3
AvgWirelenPerPin Fanout 500=7.6
AvgWirelenPerPin Fanout 5000=5.6
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=3.5154