Anlg Ch State  Units/Div  Position  Coupling  BW Limit  Invert  Impedance 
 Ch 1:    On     2.00V/     0.0V       DC        Off      Off     1M Ohm  

Anlg Ch  Probe 
 Ch 1:  10 : 1 

Digital  Threshold 
 D0-D7: TTL (1.4V) 

Trigger  Mode   Coupling  Noise Rej  HF Reject   Holdoff 
  Edge  Normal     DC        Off        Off     60.000ns 

Trigger Source   Slope   Level 
         Ch 1   Rising  +2.40V 

Time Time Ref  Main s/div   Delay  
Main  Center    1.000ms/   25.60ms 

Acquisition Realtime  Vectors  Infinite Persistence 
   Normal      On        On             Off         

