Anlg Ch State  Units/Div  Position  Coupling  BW Limit  Invert  Impedance 
 Ch 1:    On     500mV/    4.000V      DC        Off      Off     1M Ohm  
 Ch 2:    On     2.00V/    -2.000V     DC        Off      Off     1M Ohm  
 Ch 3:    On     5.00V/    11.75V      DC        Off      Off     1M Ohm  

Anlg Ch  Probe 
 Ch 1:  10 : 1 
 Ch 2:  10 : 1 
 Ch 3:  10 : 1 

Trigger  Mode   Coupling  Noise Rej  HF Reject   Holdoff 
  Edge  Normal     DC        Off        Off     60.000ns 

Trigger Source   Slope   Level 
         Ch 2   Rising  +4.30V 

Time Time Ref  Main s/div   Delay  
Main  Center    5.000ms/   21.32ms 

Acquisition Realtime  Vectors  Infinite Persistence 
   Normal      On        On             Off         

