
[Saving user: root]
[Saving time: 2016-12-20 22:54:43+08:00]
[MA5600V800R013: 3910]
#
[sysmode]
  <sysmode>
 switch adsl mode to rfc2662 vdsl mode to tr129
 xpon mode switch-to profile-mode
 voice-spec set vag-num 8
 protocol support h248
 system ex-mode backup
 system workscene msan
 router mode basic
#
[global-config]
  <global-config>
 sysname gpon.huawei_MA5683T
 trap filter event condition id 0x0a300013
 trap filter event condition id 0x0a300015
 dba-profile add profile-id 10 profile-name "dba_profile10" type4 max 1024000
 ont-srvprofile gpon profile-id 10 profile-name "srv-profile10"
  ont-port eth 1
  port vlan eth 1 translation 701 user-vlan 701
  commit
 ont-srvprofile gpon profile-id 11 profile-name "srvprofil_11"
  ont-port pots 2 eth 4
  port vlan eth 1 translation 701 user-vlan 701
  commit
 ont-lineprofile gpon profile-id 0 profile-name "line-profile_default_0"
  tcont 0 dba-profile-id 2
  tcont 1 dba-profile-id 0
  commit
  quit
 ont-lineprofile gpon profile-id 10 profile-name "lineprofile10"
  tcont 4 dba-profile-id 10
  gem add 126 eth tcont 4
  gem mapping 126 0 vlan 701
  commit
  quit
 ont-lineprofile gpon profile-id 11 profile-name "Lineprofile_11"
  tcont 5 dba-profile-id 10
  gem add 126 eth tcont 5
  gem mapping 126 0 vlan 701
  commit
  quit
#
[device-config]
  <device-config>
 board add 0/0 H807GPBH
 board add 0/8 H801GICF
 board add 0/9 H801GICF
 board add standby
 rack info 0 description "Rack"
#
[public-config]
  <public-config>
 timezone GMT+ 01:00
 snmp-agent local-engineid 800007DB03643E8C884A9501
 snmp-agent sys-info contact unArt
 snmp-agent sys-info location Slavicin,Czech
#
[vlan-config]
  <vlan-config>
 vlan 10 smart
 vlan 701 smart
 port vlan 701 0/9 0
#
[gpon]
  <gpon-0/0>
 interface gpon 0/0
 port 0 ont-auto-find enable
 port 1 ont-auto-find enable
 port 2 ont-auto-find enable
 port 3 ont-auto-find enable
 port 4 ont-auto-find enable
 port 5 ont-auto-find enable
 port 6 ont-auto-find enable
 port 7 ont-auto-find enable
 ont add 0 0 sn-auth "424C4B47388A5741" omci ont-lineprofile-id 10
ont-srvprofile-id 10 desc "Netis"
 ont add 0 1 sn-auth "48575443D95D055A" omci ont-lineprofile-id 10
ont-srvprofile-id 10 desc "Huawei"
 ont port native-vlan 0 0 eth 1 vlan 701 priority 0
#
[emu-config]
  <emu-config>
 emu add 0 fan 0 1  "H801FCBI"
#
[bbs-config]
  <bbs-config>
 service-port 10 vlan 701 gpon 0/0/0 ont 1 gemport 126 multi-service user-vlan  701 tag-transform translate inbound traffic-table index 3 outbound traffic-table index 3
 service-port 11 vlan 701 gpon 0/0/0 ont 0 gemport 126 multi-service user-vlan  701 tag-transform translate inbound traffic-table index 3 outbound traffic-table index 3
#
[config]
  <config>
 mpls label start 8192
#
[prevlanif]
  <prevlanif>
 interface vlanif10
#
[vlanif]
  <vlanif10>
interface vlanif10
 ip address 192.168.10.1 255.255.255.0 description "managementInterface"
#
[meth]
  <meth0>
interface meth0
 ip address 10.143.125.55 255.255.255.0
#
[null]
  <null0>
interface null0
#
[aaa]
  <aaa>
aaa
 authentication-scheme "default"
 #
 authorization-scheme "default"
 #
 accounting-scheme "default"
 #
 domain "default"
 #
[post-system]
  <post-system>
ip route-static 0.0.0.0 0.0.0.0 10.143.125.1
#
return
